FdoBaseUnit
FdoBinaryLogicalOperations
FdoBinaryOperations
FdoClassType
FdoCommandType
FdoComparisonOperations
FdoConditionType
FdoConflictType
FdoConnectionState
FdoDataType
FdoDeleteRule
FdoDimensionality
FdoDistanceOperations
FdoExpressionType
FdoFunctionCategoryType
FdoGeometricType
FdoGeometryComponentType
FdoGeometryType
FdoLiteralValueType
FdoLockStrategy
FdoLockType
FdoLongTransactionConflictResolution
FdoLongTransactionFreezeOperations
FdoLongTransactionPrivilegeOperations
FdoLongTransactionPrivileges
FdoLongTransactionSetOperations
FdoObjectType
FdoOrderingOption
FdoOrderType
FdoPropertyType
FdoPropertyValueConstraintType
FdoProviderDatastoreType
FdoRasterDataModelType
FdoRasterDataOrganization
FdoRasterDataType
FdoSchemaElementNameType
FdoSchemaElementState
FdoSpatialContextExtentType
FdoSpatialOperations
FdoStreamReaderType
FdoThreadCapability
FdoUnaryLogicalOperations
FdoUnaryOperations
enum FdoRasterDataModelType
  The FdoRasterDataModelType enumeration specifies the type of data within each pixel. In all cases the data is 'packed', that is, adjacent pixels are contiguous in memory with no unused bits between them, except at the end of a row, where the row is padded to a byte boundary. For example, four bit grayscale data (BitsPerPixel=4) would be packed two pixels to a byte, and a row would be padded with four bits if the image width was odd. Tri-colour or four channel data is also organized adjacently in memory, with no intervening padding except at the ends of rows. For example, eight bit RGB (BitsPerPixel=24) occupies three bytes per pixel, and would never need padding at the end of a row. Multiband data (i.e. RGB) has the same number of bits allocated to each band, so for example RGBT data with eight bits for red, would also have eight bits for each of the three other bands totaling thirty-two bits (BitsPerPixel=32). () Enumerator:
  FdoRasterDataModelType_Unknown | Data is organized in an unknown or provider specific manner.
  FdoRasterDataModelType_Data | Data is rectangular grid, floating point data model.
  FdoRasterDataModelType_Bitonal | Data is one bit (black/white - bitonal) pixels.
  FdoRasterDataModelType_Gray | Data is monochrome (black->gray->white) pixels. It is necessary to know the BitsPerPixel value to interpret the data.
  FdoRasterDataModelType_RGB | Data is red/green/blue (in that order) pixels. It is necessary to know the BitsPerPixel value to interpret the data.
  FdoRasterDataModelType_RGBA | Data is red/green/blue/alpha (in that order) pixels; RGB with transparency. It is necessary to know the BitsPerPixel value to interpret the data.
  FdoRasterDataModelType_Palette | Data is monochrome but backed by a pallette (value->pallette->colour) pixels. It is necessary to know the BitsPerPixel value to interpret the data.
Definition at line 42 of file RasterDataModelType.h.