FdoBaseUnit
FdoBinaryLogicalOperations
FdoBinaryOperations
FdoClassType
FdoCommandType
FdoComparisonOperations
FdoConditionType
FdoConflictType
FdoConnectionState
FdoDataType
FdoDeleteRule
FdoDimensionality
FdoDistanceOperations
FdoExpressionType
FdoFunctionCategoryType
FdoGeometricType
FdoGeometryComponentType
FdoGeometryType
FdoLiteralValueType
FdoLockStrategy
FdoLockType
FdoLongTransactionConflictResolution
FdoLongTransactionFreezeOperations
FdoLongTransactionPrivilegeOperations
FdoLongTransactionPrivileges
FdoLongTransactionSetOperations
FdoObjectType
FdoOrderingOption
FdoOrderType
FdoPropertyType
FdoPropertyValueConstraintType
FdoProviderDatastoreType
FdoRasterDataModelType
FdoRasterDataOrganization
FdoRasterDataType
FdoSchemaElementNameType
FdoSchemaElementState
FdoSpatialContextExtentType
FdoSpatialOperations
FdoStreamReaderType
FdoThreadCapability
FdoUnaryLogicalOperations
FdoUnaryOperations
enum FdoRasterDataOrganization
  The FdoRasterDataOrganization enumeration specifies the way pixel data is interleaved. Data is stored/retrieved in left to right, and secondarily top to bottom order within the interleave order. Tiles are also stored/retrieved in left to right, top to bottom order. For tiled data, data for one tile is completely stored/retrieved before the next tile, so for example, with 'FdoRasterDataOrganization_Image' organization of RGB data with 24 bits per pixel, the TileSizeX by TileSizeY 8 bit data values for the red channel are stored first followed by the same number of green bytes, followed by the same number of blue bytes. This organization dependant storage should be considered when 'skipping' to the middle of an image. . () Enumerator:
  FdoRasterDataOrganization_Pixel | Data is interleaved by pixel, with all data for a pixel contiguous in memory.
  FdoRasterDataOrganization_Row | Data is interleaved by row, with all data of a channel for one row contiguous in memory, followed by a rows worth of the next channel, etc.
  FdoRasterDataOrganization_Image | Data is interleaved by image, with all data of a channel for a complete image contiguous in memory, followed by a complete image of the next channel, etc.
Definition at line 40 of file RasterDataOrganization.h.