# MBTiles

Starting with GDAL 1.10, the MBTiles driver allows reading rasters in the MBTiles format, which is a specification for storing tiled map data in SQLite databases.

GDAL/OGR must be compiled with OGR SQLite driver support, and JPEG and PNG drivers.

The SRS is always the Pseudo-Mercator (a.k.a Google Mercator) projection.

The driver can retrieve pixel attributes encoded according to the UTFGrid specification available in some MBTiles files. They can be obtained with the gdallocationinfo utility, or with a GetMetadataItem("Pixel_iCol_iLine", "LocationInfo") call on a band object.

## Examples:

- Accessing a remote MBTiles raster :

      $ gdalinfo /vsicurl/http://a.tiles.mapbox.com/v3/kkaefer.iceland.mbtiles

  Output:

      Driver: MBTiles/MBTiles
      Files: /vsicurl/http://a.tiles.mapbox.com/v3/kkaefer.iceland.mbtiles
      Size is 16384, 16384
      Coordinate System is:
      PROJCS["WGS 84 / Pseudo-Mercator",
          GEOGCS["WGS 84",
              DATUM["WGS_1984",
                  SPHEROID["WGS 84",6378137,298.257223563,
                      AUTHORITY["EPSG","7030"]],
                  AUTHORITY["EPSG","6326"]],
              PRIMEM["Greenwich",0,
                  AUTHORITY["EPSG","8901"]],
              UNIT["degree",0.0174532925199433,
                  AUTHORITY["EPSG","9122"]],
              AUTHORITY["EPSG","4326"]],
          PROJECTION["Mercator_1SP"],
          PARAMETER["central_meridian",0],
          PARAMETER["scale_factor",1],
          PARAMETER["false_easting",0],
          PARAMETER["false_northing",0],
          UNIT["metre",1,
              AUTHORITY["EPSG","9001"]],
          AXIS["X",EAST],
          AXIS["Y",NORTH],
          EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0.0 +lon_0=0.0 +x_0=0.0 +y_0=0 +k=1.0 +units=m +nadgrids=@null +wktext  +no_defs"],
          AUTHORITY["EPSG","3857"]]
      Origin = (-3757031.250000000000000,11271093.750000000000000)
      Pixel Size = (152.873992919921875,-152.873992919921875)
      Image Structure Metadata:
        INTERLEAVE=PIXEL
      Corner Coordinates:
      Upper Left  (-3757031.250,11271093.750) ( 33d44'59.95"W, 70d36'45.36"N)
      Lower Left  (-3757031.250, 8766406.250) ( 33d44'59.95"W, 61d36'22.97"N)
      Upper Right (-1252343.750,11271093.750) ( 11d14'59.98"W, 70d36'45.36"N)
      Lower Right (-1252343.750, 8766406.250) ( 11d14'59.98"W, 61d36'22.97"N)
      Center      (-2504687.500,10018750.000) ( 22d29'59.97"W, 66d30'47.68"N)
      Band 1 Block=256x256 Type=Byte, ColorInterp=Red
        Overviews: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
        Mask Flags: PER_DATASET ALPHA
        Overviews of mask band: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
      Band 2 Block=256x256 Type=Byte, ColorInterp=Green
        Overviews: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
        Mask Flags: PER_DATASET ALPHA
        Overviews of mask band: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
      Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
        Overviews: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
        Mask Flags: PER_DATASET ALPHA
        Overviews of mask band: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512
      Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha
        Overviews: 8192x8192, 4096x4096, 2048x2048, 1024x1024, 512x512

- Reading pixel attributes encoded according to the UTFGrid specification :

      $ gdallocationinfo /vsicurl/http://a.tiles.mapbox.com/v3/mapbox.geography-class.mbtiles -wgs84 2 49 -b 1 -xml

  Output:

      <Report pixel="33132" line="22506">
        <BandReport band="1">
          <LocationInfo>
            <Key>74</Key>
            <JSon>{"admin":"France","flag_png":" "}</JSon>
          </LocationInfo>
          <Value>238</Value>
        </BandReport>
      </Report>

See Also:

- MBTiles specification
- UTFGrid specification