# SEG-P1 / UKOOA P1/90

(GDAL/OGR >= 1.9.0)

This driver reads files in SEG-P1 and UKOOA P1/90 formats. Those files are simple ASCII files that contain seismic shotpoints. Two layers are reported : one with the points, and another ones where sequential points with same line name are merged together in a single feature with a line geometry.

### See Also

- Description of SEG-P1 format

- Description of UKOOA P1/90 format