# UK .NTF

The National Transfer Format, mostly used by the UK Ordnance Survey, is supported for read access.

This driver treats a directory as a dataset and attempts to merge all the .NTF files in the directory, producing a layer for each type of feature (but generally not for each source file). Thus a directory containing several Landline files will have three layers (LANDLINE_POINT, LANDLINE_LINE and LANDLINE_NAME) regardless of the number of landline files.

NTF features are always returned with the British National Grid coordinate system. This may be inappropriate for NTF files written by organizations other than the UK Ordnance Survey.

### See Also

- General UK NTF Information

## Implementation Notes

### Products (and Layers) Supported

    Landline (and Landline Plus):
    	LANDLINE_POINT
    	LANDLINE_LINE
    	LANDLINE_NAME

    Panorama Contours:
    	PANORAMA_POINT
    	PANORAMA_CONTOUR

    	HEIGHT attribute holds elevation.

    Strategi:
    	STRATEGI_POINT
    	STRATEGI_LINE
    	STRATEGI_TEXT
    	STRATEGI_NODE

    Meridian:
    	MERIDIAN_POINT
    	MERIDIAN_LINE
    	MERIDIAN_TEXT
    	MERIDIAN_NODE

    Boundaryline:
    	BOUNDARYLINE_LINK
    	BOUNDARYLINE_POLY
    	BOUNDARYLINE_COLLECTIONS

    	The _POLY layer has links to links allowing true polygons to
            be formed (otherwise the _POLY's only have a seed point for geometry.
    	The collections are collections of polygons (also without geometry
    	as read).  This is the only product from which polygons can be
    	constructed.

    BaseData.GB:
    	BASEDATA_POINT
    	BASEDATA_LINE
    	BASEDATA_TEXT
    	BASEDATA_NODE

    OSCAR Asset/Traffic:
    	OSCAR_POINT
    	OSCAR_LINE
    	OSCAR_NODE

    OSCAR Network:
    	OSCAR_NETWORK_POINT
    	OSCAR_NETWORK_LINE
    	OSCAR_NETWORK_NODE

    Address Point:
    	ADDRESS_POINT

    Code Point:
    	CODE_POINT

    Code Point Plus:
    	CODE_POINT_PLUS

The dataset as a whole will also have a FEATURE_CLASSES layer containing a pure table relating FEAT_CODE numbers with feature class names (FC_NAME). This applies to all products in the dataset. A few layer types (such as the Code Point, and Address Point products) don't include feature classes. Some products use features classes that are not defined in the file, and so they will not appear in the FEATURE_CLASSES layer.

### Product Schemas

The approach taken in this reader is to treat one file, or a directory of files as a single dataset. All files in the dataset are scanned on open. For each particular product (listed above) a set of layers are created; however, these layers may be extracted from several files of the same product.

The layers are based on a low level feature type in the NTF file, but will generally contain features of many different feature codes (FEAT_CODE attribute). Different features within a given layer may have a variety of attributes in the file; however, the schema is established based on the union of all attributes possible within features of a particular type (i.e. POINT) of that product family (i.e. OSCAR Network).

If an NTF product is read that doesn't match one of the known schema's it will go through a different generic handler which has only layers of type GENERIC_POINT and GENERIC_LINE. The features only have a FEAT_CODE attribute.

Details of what layers of what products have what attributes can be found in the NTFFileReader::EstablishLayers() method at the end of ntf_estlayers.cpp. This file also contains all the product specific translation code.

### Special Attributes

    FEAT_CODE: General feature code integer, can be used to lookup a name in the
               FEATURE_CLASSES layer/table.

    TEXT_ID/POINT_ID/LINE_ID/NAME_ID/COLL_ID/POLY_ID/GEOM_ID:
              Unique identifier for a feature of the appropriate type.

    TILE_REF: All layers (except FEATURE_CLASSES) contain a TILE_REF attribute
              which indicates which tile (file) the features came from.  Generally
              speaking the id numbers are only unique within the tile and so
              the TILE_REF can be used restrict id links within features from
              the same file.

    FONT/TEXT_HT/DIG_POSTN/ORIENT:
    	Detailed information on the font, text height, digitizing position,
            and orientation of text or name objects.  Review the OS product
            manuals to understand the units, and meaning of these codes.

    GEOM_ID_OF_POINT:
    	For _NODE features this defines the POINT_ID of the point layer object
            to which this node corresponds.  Generally speaking the nodes don't
            carry a geometry of their own.  The node must be related to a point
            to establish its position.

    GEOM_ID_OF_LINK:
    	A _list_ of _LINK or _LINE features to end/start at a node.  Nodes,
            and this field are generally only of value when establishing
            connectivity of line features for network analysis.   Note that this
            should be related to the target features GEOM_ID, not its LINE_ID.

            On the BOUNDARYLINE_POLY layer this attribute contains the GEOM_IDs
            of the lines which form the edge of the polygon.

    POLY_ID:
    	A list of POLY_ID's from the BOUNDARYLINE_POLY layer associated with
            a given collection in the BOUNDARYLINE_COLLECTIONS layer.

### Generic Products

In situations where a file is not identified as being part of an existing known product it will be treated generically. In this case the entire dataset is scanned to establish what features have what attributes. Because of this, opening a generic dataset can be much slower than opening a recognised dataset. Based on this scan a list of generic features (layers) are defined from the following set:

     GENERIC_POINT
     GENERIC_LINE
     GENERIC_NAME
     GENERIC_TEXT
     GENERIC_POLY
     GENERIC_NODE
     GENERIC_COLLECTION

Generic products are primarily handled by the ntf_generic.cpp module whereas specific products are handled in ntf_estlayers.cpp.

Because some data products (OSNI datasets) not from the Ordnance Survey were found to have record groups in unusual orders compared to what the UK Ordnance Survey does, it was found necessary to cache all the records of level 3 and higher generic products, and construct record groups by id reference from within this cache rather than depending on convenient record orderings. This is accomplished by the NTFFileReader "indexing" capability near the bottom of ntffilereader.cpp. Because of this in memory indexing accessing generic datasets can be much more memory intensive than accessing known data products, though it isn't necessary for generic level 1 and 2 products.

It is possible to force a known product to be treated as generic by setting the FORCE_GENERIC option to "ON" using OGRNTFDataSource::SetOptionsList() as is demonstrated in ntfdump.cpp. This may also be accomplished from outside OGR applications by setting the OGR_NTF_OPTIONS environment variable to "FORCE_GENERIC=ON".