# GRASS Raster Format

Driver short name

GRASS

Build dependencies

libgrass

GDAL optionally supports reading of existing GRASS raster maps or imagery groups, but not writing or export. The support for GRASS raster format is determined when the library is configured, and requires libgrass to be pre-installed (see Notes below).

GRASS raster maps/imagery groups can be selected in several ways.

1. The full path to the `cellhd` file can be specified. This is not a relative path, or at least it must contain all the path components within the GRASS database including the database root itself. The following example opens the raster map “proj_tm” within the GRASS mapset “PERMANENT” of the GRASS location “proj_tm” in the GRASS database located at `/u/data/grassdb`.

   For example:

       gdalinfo /u/data/grassdb/proj_tm/PERMANENT/cellhd/proj_tm

2. The full path to the directory containing information about an imagery group (or the REF file within it) can be specified to refer to the whole group as a single dataset. The following examples do the same thing.

   For example:

       gdalinfo /usr2/data/grassdb/imagery/raw/group/testmff/REF
       gdalinfo /usr2/data/grassdb/imagery/raw/group/testmff

3. If there is a correct `.grassrc5` (GRASS 5), `.grassrc6` (GRASS 6) `.grass7/rc` (GRASS 7) setup file in the users home directory then raster maps or imagery groups may be opened just by the cell name. This only works for raster maps or imagery groups in the current GRASS location and mapset as defined in the GRASS setup file.

The following features are supported by the GDAL/GRASS link.

- Up to 256 entries from raster colormaps are read (0-255).

- Compressed and uncompressed integer (CELL), floating point (FCELL) and double precision (DCELL) raster maps are all supported. Integer raster maps are classified with a band type of “Byte” if the 1-byte per pixel format is used, or “UInt16” if the two byte per pixel format is used. Otherwise integer raster maps are treated as “UInt32”.

- Georeferencing information is properly read from GRASS format.

- An attempt is made to translate coordinate systems, but some conversions may be flawed, in particular in handling of datums and units.

## Driver capabilities

Supports Georeferencing

This driver supports georeferencing

## Notes on driver variations

For GRASS 5.7 Radim Blazek has moved the driver to using the GRASS shared libraries directly instead of using libgrass. Currently (GDAL 1.2.2 and later) both version of the driver are available and can be configured using “–with-libgrass” for the libgrass variant or “–with-grass=<dir>” for the new GRASS 5.7+ library based version. The GRASS 5.7+ driver version is currently not supporting coordinate system access, though it is hoped that will be corrected at some point.

## See Also

- GRASS GIS home page

- libgrass page