.. _raster.gtiff:

================================================================================
GTiff -- GeoTIFF File Format
================================================================================

.. shortname:: GTiff

.. built_in_by_default::

Most forms of TIFF and GeoTIFF files are supported by GDAL for reading,
and somewhat less varieties can be written.

GDAL also supports reading and writing BigTIFF files (evolution of the TIFF format
to support files larger than 4 GB).

Currently band types of Byte, UInt16, Int16, UInt32, Int32, Float32,
Float64, CInt16, CInt32, CFloat32 and CFloat64 are supported for reading
and writing. Paletted images will return palette information associated
with the band. The compression formats listed below should be supported
for reading as well.

As well, one bit files, and some other unusual formulations of GeoTIFF
file, such as YCbCr color model files, are automatically translated into
RGBA (red, green, blue, alpha) form, and treated as four eight bit
bands.

For an alternative which offers thread-safe read-only capabilities, consult
:ref:`raster.libertiff`.

Driver capabilities
-------------------

.. supports_createcopy::

.. supports_create::

.. supports_georeferencing::

.. supports_virtualio::

Georeferencing
--------------

Most GeoTIFF projections should be supported, with the caveat that in
order to translate uncommon Projected, and Geographic coordinate systems
into OGC WKT it is necessary to have the PROJ proj.db database
available. It must be found at the location pointed to by the PROJ_LIB
environment variable, or at one of the locations set programmatically
via OSRSetPROJSearchPaths().

Georeferencing from GeoTIFF is supported in the form of one tiepoint and
pixel size, a transformation matrix, or a list of GCPs.

If no georeferencing information is available in the TIFF file itself,
GDAL will also check for, and use an ESRI :ref:`world
file <raster.wld>` with the extension .tfw, .tifw/.tiffw or
.wld, as well as a MapInfo .tab file.

By default, information is fetched in following order (first listed is
the highest priority): PAM (Persistent Auxiliary metadata) .aux.xml
sidecar file, INTERNAL (GeoTIFF keys and tags), TABFILE (.tab),
WORLDFILE (.tfw, .tifw/.tiffw or .wld), XML (.xml)

Starting with GDAL 2.2, the allowed sources and their priority order can
be changed with the :config:`GDAL_GEOREF_SOURCES` configuration option (or
:oo:`GEOREF_SOURCES` open option) whose value is a comma-separated list of the
following keywords : PAM, INTERNAL, TABFILE, WORLDFILE, XML (added in 3.7), NONE.
Earlier mentioned sources take priority over later ones. A non
mentioned source will be ignored.

For example setting it to "WORLDFILE,PAM,INTERNAL" will make a
geotransformation matrix from a potential worldfile priority over PAM
or GeoTIFF.

Minimum support for extracting the CRS from ESRI .xml side car files has been
added in GDAL 3.7, using the metadata.refSysInfo.RefSystem.refSysID.identCode.code
CRS code.

GDAL can read and write the *RPCCoefficientTag* as described in the
`RPCs in GeoTIFF <http://geotiff.maptools.org/rpc_prop.html>`__ proposed
extension. The tag is written only for files created with the default
profile GDALGeoTIFF. For other profiles, a .RPB file is created. In GDAL
data model, the RPC coefficients are stored into the RPC metadata
domain. For more details, see the :ref:`rfc-22`. If .RPB or \_RPC.TXT
files are found, they will be used to read the RPCs, even if the
*RPCCoefficientTag* tag is set.

Internal nodata masks
---------------------

TIFF files can contain internal transparency masks. The GeoTIFF driver
recognizes an internal directory as being a transparency mask when the
FILETYPE_MASK bit value is set on the TIFFTAG_SUBFILETYPE tag. According
to the TIFF specification, such internal transparency masks contain 1
sample of 1-bit data. Although the TIFF specification allows for higher
resolutions for the internal transparency mask, the GeoTIFF driver only
supports internal transparency masks of the same dimensions as the main
image. Transparency masks of internal overviews are also supported.

When the :config:`GDAL_TIFF_INTERNAL_MASK` configuration option is set to YES
(which is the case starting with GDAL 3.9 when CreateMaskBand() is invoked on
the dataset, or when it is invoked on a raster band with the GMF_PER_DATASET flag), and
the GeoTIFF file is opened in update mode, the CreateMaskBand() method
on a TIFF dataset or rasterband will create an internal transparency
mask. Otherwise, the default behavior of nodata mask creation will be
used, that is to say the creation of a .msk file, as per :ref:`rfc-15`.

1-bit internal mask band are deflate compressed. When reading them back,
to make conversion between mask band and alpha band easier, mask bands
are exposed to the user as being promoted to full 8 bits (i.e. the value
for unmasked pixels is 255) unless the :config:`GDAL_TIFF_INTERNAL_MASK_TO_8BIT`
configuration option is set to NO. This does not affect the way the mask
band is written (it is always 1-bit).

Overviews
---------

The GeoTIFF driver supports reading, creation and update of internal
overviews. Internal overviews can be created on GeoTIFF files opened in
update mode (with gdaladdo for instance). If the GeoTIFF file is opened
as read only, the creation of overviews will be done in an external .ovr
file. Overview are only updated on request with the BuildOverviews()
method.

The block size (tile width and height) used for overviews (internal or
external) can be specified by setting the GDAL_TIFF_OVR_BLOCKSIZE
environment variable to a power-of-two value between 64 and 4096. The
default is 128, or starting with GDAL 3.1 to use the same block size
as the full-resolution dataset if possible (i.e. block height and width
are equal, a power-of-two, and between 64 and 4096).

Overviews and nodata masks
--------------------------

The following configurations can be encountered depending if overviews
and nodata masks are internal or not.

-  Internal overviews, internal nodata mask: If a GeoTIFF file has a
   internal transparency mask and the GeoTIFF file is opened
   in update mode, BuildOverviews() will automatically create overviews
   for the internal transparency mask.
-  External overviews, external nodata mask: When opened in read-only
   mode, BuildOverviews() will automatically create overviews for the
   external transparency mask (in a .msk.ovr file)
-  Internal overviews, external nodata mask: when running
   BuildOverviews() in update mode on the .tif file, starting with GDAL 3.9,
   overviews of the main bands and of the external .msk will be generated (
   as internal overview of the .msk).
   Prior to GDAL 3.9, only the overviews of the main bands are generated.
   Overviews of the external .msk file had to be explicitly generated by running
   BuildOverviews() on the .msk.

For the remaining configuration, behavior is less obvious:

-  External overviews, internal nodata mask: when running
   BuildOverviews() in read-only mode on the .tif file, only the
   overviews of the main bands will be generated. Generating the
   overviews of the internal nodata mask is not currently supported by
   the driver.

Practical note: for a command line point of view, BuildOverview() in
update mode means "gdaladdo the.tiff" (without -ro). Whereas
BuildOverviews() in read-only mode means "gdaladdo -ro the.tiff".

Metadata
--------

GDAL can deal with the following baseline TIFF tags as dataset-level
metadata :

-  TIFFTAG_DOCUMENTNAME
-  TIFFTAG_IMAGEDESCRIPTION
-  TIFFTAG_SOFTWARE
-  TIFFTAG_DATETIME
-  TIFFTAG_ARTIST
-  TIFFTAG_HOSTCOMPUTER
-  TIFFTAG_COPYRIGHT
-  TIFFTAG_XRESOLUTION
-  TIFFTAG_YRESOLUTION
-  TIFFTAG_RESOLUTIONUNIT
-  TIFFTAG_MINSAMPLEVALUE (read only)
-  TIFFTAG_MAXSAMPLEVALUE (read only)
-  `GEO_METADATA <https://portal.dgiwg.org/files/70843>`__:
   This tag may be used for embedding XML-encoded instance documents
   prepared using 19139-based schema (GeoTIFF DGIWG) (GDAL >= 2.3)
-  `TIFF_RSID <https://www.awaresystems.be/imaging/tiff/tifftags/tiff_rsid.html>`__:
   This tag specifies a File Universal Unique Identifier, or RSID,
   according to DMF definition (GeoTIFF DGIWG) (GDAL >= 2.3)

The name of the metadata item to use is one of the above names
("TIFFTAG_DOCUMENTNAME", ...). On creation, those tags can for example
be set with

::

   gdal_translate in.tif out.tif -mo {TAGNAME}=VALUE

Other non standard metadata items can be stored in a TIFF file created
with the profile GDALGeoTIFF (the default, see below in the Creation
issues section). Those metadata items are grouped together into a XML
string stored in the non standard TIFFTAG_GDAL_METADATA ASCII tag (code
42112). When BASELINE or GeoTIFF profile are used, those non standard
metadata items are stored into a PAM .aux.xml file.

The value of GDALMD_AREA_OR_POINT ("AREA_OR_POINT") metadata item is
stored in the GeoTIFF key RasterPixelIsPoint for GDALGeoTIFF or GeoTIFF
profiles.

XMP metadata can be extracted from the file,
and will be reported as XML raw content in the xml:XMP metadata domain.

EXIF metadata can be extracted from the file,
and will be reported in the EXIF metadata domain.

Color Profile Metadata
----------------------

GDAL can deal with the following color profile
metadata in the COLOR_PROFILE domain:

-  SOURCE_ICC_PROFILE (Base64 encoded ICC profile embedded in file. If
   available, other tags are ignored.)
-  SOURCE_PRIMARIES_RED (xyY in "x,y,1" format for red primary.)
-  SOURCE_PRIMARIES_GREEN (xyY in "x,y,1" format for green primary)
-  SOURCE_PRIMARIES_BLUE (xyY in "x,y,1" format for blue primary)
-  SOURCE_WHITEPOINT (xyY in "x,y,1" format for whitepoint)
-  TIFFTAG_TRANSFERFUNCTION_RED (Red table of TIFFTAG_TRANSFERFUNCTION)
-  TIFFTAG_TRANSFERFUNCTION_GREEN (Green table of
   TIFFTAG_TRANSFERFUNCTION)
-  TIFFTAG_TRANSFERFUNCTION_BLUE (Blue table of
   TIFFTAG_TRANSFERFUNCTION)
-  TIFFTAG_TRANSFERRANGE_BLACK (Min range of TIFFTAG_TRANSFERRANGE)
-  TIFFTAG_TRANSFERRANGE_WHITE (Max range of TIFFTAG_TRANSFERRANGE)

Note that these metadata properties can only be used on the original raw
pixel data. If automatic conversion to RGB has been done, the color
profile information cannot be used.

All these metadata tags can be overridden and/or used as creation
options.

Nodata value
------------

GDAL stores band nodata value in the non standard TIFFTAG_GDAL_NODATA
ASCII tag (code 42113) for files created with the default profile
GDALGeoTIFF. Note that all bands must use the same nodata value. When
BASELINE or GeoTIFF profile are used, the nodata value is stored into a
PAM .aux.xml file.

Raster Attribute Table
----------------------

Starting with GDAL 3.11, Raster attribute tables stored in auxiliary
.tif.vat.dbf files, as written by ArcGIS, can be read as GDAL Raster Attribute
Table.

Sparse files
------------

GDAL makes a special interpretation of a TIFF tile or strip whose offset
and byte count are set to 0, that is to say a tile or strip that has no
corresponding allocated physical storage. On reading, such tiles or
strips are considered to be implicitly set to 0 or to the nodata value
when it is defined. On writing, it is possible to enable generating such
files through the Create() interface by setting the :co:`SPARSE_OK` creation
option to YES. Then, blocks that are never written through the
IWriteBlock()/IRasterIO() interfaces will have their offset and byte
count set to 0. This is particularly useful to save disk space and time
when the file must be initialized empty before being passed to a further
processing stage that will fill it. To avoid ambiguities with another
sparse mechanism discussed in the next paragraphs, we will call such
files with implicit tiles/strips "TIFF sparse files". They will be
likely **not** interoperable with TIFF readers that are not GDAL based
and would consider such files with implicit tiles/strips as defective.

Starting with GDAL 2.2, this mechanism is extended to the CreateCopy()
and Open() interfaces (for update mode) as well. If the :co:`SPARSE_OK`
creation option (or the :oo:`SPARSE_OK` open option for Open()) is set to YES,
even an attempt to write a all 0/nodata block will be detected so that
the tile/strip is not allocated (if it was already allocated, then its
content will be replaced by the 0/nodata content).

Starting with GDAL 2.2, in the case where :co:`SPARSE_OK` is **not** defined
(or set to its default value FALSE), for uncompressed files whose nodata
value is not set, or set to 0, in Create() and CreateCopy() mode, the
driver will delay the allocation of 0-blocks until file closing, so as
to be able to write them at the very end of the file, and in a way
compatible of the filesystem sparse file mechanisms (to be distinguished
from the TIFF sparse file extension discussed earlier). That is that all
the empty blocks will be seen as properly allocated from the TIFF point
of view (corresponding strips/tiles will have valid offsets and byte
counts), but will have no corresponding physical storage. Provided that
the filesystem supports such sparse files, which is the case for most
Linux popular filesystems (ext2/3/4, xfs, btfs, ...) or NTFS on Windows.
If the file system does not support sparse files, physical storage will
be allocated and filled with zeros.

Raw mode
--------

For some TIFF formulations that have "odd" photometric color spaces,
on-the-fly decoding as RGBA is done. This might not be desirable in some
use cases. This behavior can be disabled by prefixing the filename with
GTIFF_RAW:

For example to translate a CMYK file to another one :

::

   gdal_translate GTIFF_RAW:in.tif out.tif -co PHOTOMETRIC=CMYK

Open options
------------

|about-open-options|
This driver supports the following open options:

.. oo:: NUM_THREADS
   :choices: <number_of_threads>, ALL_CPUS
   :since: 2.1

   Enable
   multi-threaded compression by specifying the number of worker
   threads. Worth it for slow compression algorithms such as DEFLATE or
   LZMA. Default is compression in the main thread.
   Starting with GDAL 3.6, this option also enables multi-threaded decoding
   when RasterIO() requests intersect several tiles/strips.
   The :config:`GDAL_NUM_THREADS` configuration option can also
   be used as an alternative to setting the open option.

.. oo:: GEOREF_SOURCES
   :choices: comma-separated list with one or several of PAM\, INTERNAL\, TABFILE\, WORLDFILE or XML (XML added in 3.7)
   :since: 2.2

   Define which georeferencing
   sources are allowed and their priority order. See
   `Georeferencing <#georeferencing>`__ paragraph.

.. oo:: SPARSE_OK
   :choices: TRUE, FALSE
   :since: 2.2
   :default: FALSE

   Should empty blocks be
   omitted on disk? When this option is set, any attempt of writing a
   block whose all pixels are 0 or the nodata value will cause it not to
   be written at all (unless there is a corresponding block already
   allocated in the file). Sparse files have 0 tile/strip offsets for
   blocks never written and save space; however, most non-GDAL packages
   cannot read such files.

.. oo:: IGNORE_COG_LAYOUT_BREAK
   :choices: YES, NO
   :since: 3.8
   :default: NO

   Updating a COG (Cloud Optimized GeoTIFF) file generally breaks part of the
   optimizations, but still produces a valid GeoTIFF file.
   Starting with GDAL 3.8, to avoid undesired loss of the COG characteristics,
   opening such a file in update mode will be rejected, unless this option is
   also set to YES (default is NO).
   This option has only effect on COG files and when opening in update mode,
   and is ignored on regular (Geo)TIFF files.

.. oo:: COLOR_TABLE_MULTIPLIER
   :choices: AUTO, 1, 256, 257
   :since: 3.10.0

   Specifies the value by which to multiply GDAL color table entry values, usually
   in [0,255] range, to obtain a TIFF color map value, or on reading by which
   to divide TIFF color map values to get a GDAL color table entry. Since GDAL 2.3.0,
   GDAL consistently uses 257, but it might be necessary to use 256 for
   compatibility with files generated by other software.
   In AUTO mode, GDAL 3.10 or later can automatically detect the 256 multiplication
   factor when all values in the TIFF color map are multiple of that value.

Creation Issues
---------------

GeoTIFF files can be created with any GDAL defined band type, including
the complex types. Created files may have any number of bands. Files of
type Byte with exactly 3 bands will be given a photometric
interpretation of RGB, files of type Byte with exactly four bands will
have a photometric interpretation of RGBA, while all other combinations
will have a photometric interpretation of MIN_IS_BLACK. Starting with
GDAL 2.2, non-standard (regarding to the intrinsics TIFF capabilities)
band color interpretation, such as BGR ordering, will be handled in
creation and reading, by storing them in the GDAL internal metadata TIFF
tag.

The TIFF format only supports R,G,B components for palettes / color
tables. Thus on writing the alpha information will be silently
discarded.

Creation Options
~~~~~~~~~~~~~~~~

|about-creation-options|
This driver supports the following creation options:

-  .. co:: TFW
      :choices: YES, NO

      Force the generation of an associated ESRI world file
      (.tfw). See the :ref:`World Files <raster.wld>` page for details.

-  .. co:: RPB
      :choices: YES, NO

      Force the generation of an associated .RPB file to
      describe RPC (Rational Polynomial Coefficients), if RPC information
      is available. If not specified, this file is automatically generated
      if there's RPC information and that the PROFILE is not the default
      GDALGeoTIFF.

-  .. co:: RPCTXT
      :choices: YES, NO

      Force the generation of an associated
      \_RPC.TXT file to describe RPC (Rational Polynomial Coefficients), if
      RPC information is available.

-  .. co:: INTERLEAVE
      :choices: BAND, PIXEL

      Set the interleaving to use

      * ``PIXEL``: for each spatial block, one TIFF tile/strip gathering values for
        all bands is used . This matches the ``contiguous`` planar configuration in
        TIFF terminology.
        This is also known as a ``BIP (Band Interleaved Per Pixel)`` organization.
        Such method is the default, and may be slightly less
        efficient than BAND interleaving for some purposes, but some applications
        only support pixel interleaved TIFF files. On the other hand, image-based
        compression methods may perform better using PIXEL interleaving. For JPEG
        PHOTOMETRIC=YCbCr, pixel interleaving is required. It is also required for
        WebP compression.

        Assuming a pixel[band][y][x] indexed array, when using CreateCopy(),
        the pseudo code for the file disposition is:

        ::

          for y in 0 ... numberOfBlocksInHeight - 1:
              for x in 0 ... numberOfTilesInWidth - 1:
                  for j in 0 ... blockHeight - 1:
                      for i in 0 ... blockWidth -1:
                          start_new_strip_or_tile()
                          for band in 0 ... numberBands -1:
                              write(pixel[band][y*blockHeight+j][x*blockWidth+i])
                          end_new_strip_or_tile()
                      end_for
                  end_for
              end_for
          end_for


      * ``BAND``: for each spatial block, one TIFF tile/strip is used for each band.
        This matches the contiguous ``separate`` configuration in TIFF terminology.
        This is also known as a ``BSQ (Band SeQuential)`` organization.

        In addition to that, when using CreateCopy(), data for the first band is
        written first, followed by data for the second band, etc.
        The pseudo code for the file disposition is:

        ::

          for y in 0 ... numberOfBlocksInHeight - 1:
              for x in 0 ... numberOfTilesInWidth - 1:
                  start_new_strip_or_tile()
                  for band in 0 ... numberBands -1:
                      for j in 0 ... blockHeight - 1:
                          for i in 0 ... blockWidth -1:
                              write(pixel[band][y*blockHeight+j][x*blockWidth+i])
                          end_for
                      end_for
                  end_new_strip_or_tile()
              end_for
          end_for


      Starting with GDAL 3.5, when copying from a source dataset with multiple bands
      which advertises a INTERLEAVE metadata item, if the INTERLEAVE creation option
      is not specified, the source dataset INTERLEAVE will be automatically taken
      into account, unless the COMPRESS creation option is specified.

      .. note::

          Starting with GDAL 3.11, a ``TILE`` interleaving is available,
          but only when using the :ref:`raster.cog` driver.

-  .. co:: TILED
      :choices: YES, NO
      :default: NO

      By default striped TIFF files are created. This
      option can be used to force creation of tiled TIFF files.

-  .. co:: BLOCKXSIZE
      :choices: <integer>
      :default: 256

      Sets tile width. Must be divisible by 16.

-  .. co:: BLOCKYSIZE
      :choices: <integer>

      Set tile or strip height. Tile height defaults to
      256, strip height defaults to a value such that one strip is 8K or
      less. Must be divisible by 16 when :co:`TILED`\ =YES.

-  .. co:: NBITS
      :choices: <value>

      Create a file with less than 8 bits per sample by
      passing a value from 1 to 7. The apparent pixel type should be Byte.
      Values of n=9...15 (UInt16 type) and n=17...31
      (UInt32 type) are also accepted. From GDAL 2.2, n=16 is accepted for
      Float32 type to generate half-precision floating point values.

-  .. co:: COMPRESS
      :choices: JPEG, LZW, PACKBITS, DEFLATE, CCITTRLE, CCITTFAX3, CCITTFAX4, LZMA, ZSTD, LERC, LERC_DEFLATE, LERC_ZSTD, WEBP, JXL, NONE

      Set the compression to use.

      * ``JPEG`` should generally only be used with Byte data (8 bit per channel).
        Better compression for RGB images can be obtained by using the PHOTOMETRIC=YCBCR
        colorspace with a 4:2:2 subsampling of the Y,Cb,Cr components.

        Starting with GDAL 3.4, if GDAL is built with its internal libtiff,
        read and write support for JPEG-in-TIFF compressed images with 12-bit sample
        is enabled by default (if JPEG support is also enabled), using GDAL internal libjpeg
        (based on IJG libjpeg-6b, with additional changes for 12-bit sample support).
        Support for JPEG with 12-bit sample is independent of whether
        8-bit JPEG support is enabled through internal IJG libjpeg-6b or external libjpeg
        (like libjpeg-turbo)

      * ``CCITTFAX3``, ``CCITTFAX4`` or ``CCITRLE`` compression should only be used with 1bit (NBITS=1) data

      * ``LZW``, ``DEFLATE`` and ``ZSTD`` compressions can be used with the PREDICTOR creation option.

      * ``ZSTD`` is available since GDAL 2.3 when using internal libtiff and if GDAL
        built against libzstd >=1.0, or if built against external libtiff with zstd support.

      * ``LERC`` and ``LERC_DEFLATE`` are available only when using internal libtiff for GDAL < 3.3.0.
        Since GDAL 3.3.0, LERC compression is also available when building GDAL
        against external libtiff >= 4.3.0, built itself against https://github.com/esri/lerc

      * ``LERC_ZSTD`` is available when ``LERC`` and ``ZSTD`` are available.

      * ``JXL`` is for JPEG-XL, and is only available when using internal libtiff and building GDAL against
        https://github.com/libjxl/libjxl . It is recommended to use JXL compression with the ``TILED=YES`` creation
        option and block size of 256x256, 512x512, or 1024x1024 pixels. Supported data types are ``Byte``,
        ``UInt16`` and ``Float32`` only. For GDAL < 3.6.0, JXL compression may only be used alongside
        ``INTERLEAVE=PIXEL`` (the default) on datasets with 4 bands or less.

      * ``NONE`` is the default.

-  .. co:: NUM_THREADS
      :choices: <integer>, ALL_CPUS
      :default: 1
      :since: 2.1

      Enable multi-threaded compression by specifying the number of worker
      threads. Worthwhile for slow compression algorithms such as DEFLATE or LZMA.
      Will be ignored for JPEG. Default is compression in the main thread.

-  .. co:: PREDICTOR
      :choices: 1, 2, 3
      :default: 1

      Set the predictor for LZW, DEFLATE and ZSTD
      compression. The default is 1 (no predictor), 2 is horizontal
      differencing and 3 is floating point prediction.
      PREDICTOR=2 is only supported for 8, 16, 32 and 64 bit samples (support
      for 64 bit was added in libtiff > 4.3.0).
      PREDICTOR=3 is only supported for 16, 32 and 64 bit floating-point data.

-  .. co:: DISCARD_LSB
      :choices: <nbits>, nbits_band1\,nbits_band2\,...nbits_bandN

      Set the number of least-significant bits to clear,
      possibly different per band. Lossy compression scheme to be best used
      with PREDICTOR=2 and LZW/DEFLATE/ZSTD compression.

-  .. co:: SPARSE_OK
      :choices: TRUE, FALSE

      Should newly created
      files (through Create() interface) be allowed to be sparse? Sparse
      files have 0 tile/strip offsets for blocks never written and save
      space; however, most non-GDAL packages cannot read such files.
      Starting with GDAL 2.2, SPARSE_OK=TRUE is also supported through the
      CreateCopy() interface. Starting with GDAL 2.2, even an attempt to
      write a block whose all pixels are 0 or the nodata value will cause
      it not to be written at all (unless there is a corresponding block
      already allocated in the file). The default is FALSE.

-  .. co:: JPEG_QUALITY
      :choices: 1-100
      :default: 75

      Set the JPEG quality when using JPEG compression.

      Low values result in higher compression ratios, but poorer image quality
      with strong blocking artifacts.
      Values above 95 are not meaningfully better quality but can be
      substantially larger.

-  .. co:: JPEGTABLESMODE
      :choices: 0, 1, 2, 3
      :default: 1

      Configure how and where
      JPEG quantization and Huffman tables are written in the TIFF
      JpegTables tag and strip/tile.

      -  0: JpegTables is not written. Each strip/tile contains its own
         quantization tables and use optimized Huffman coding.
      -  1: JpegTables is written with only the quantization tables. Each
         strip/tile refers to those quantized tables and use optimized
         Huffman coding. This is generally the optimal choice for smallest
         file size, and consequently is the default.
      -  2: JpegTables is written with only the default Huffman tables.
         Each strip/tile refers to those Huffman tables (thus no optimized
         Huffman coding) and contains its own quantization tables
         (identical). This option has no anticipated practical value.
      -  3: JpegTables is written with the quantization and default Huffman
         tables. Each strip/tile refers to those tables (thus no optimized
         Huffman coding). This option could perhaps with some data be more
         efficient than 1, but this should only occur in rare
         circumstances.

-  .. co:: ZLEVEL
      :choices: [1-9] or [1-12]
      :default: 6

      Set the level of compression when using DEFLATE
      compression (or LERC_DEFLATE). A value of 9 (resp. 12) is best/slowest when
      using zlib (resp. libdeflate), and 1 is least/fastest compression.

-  .. co:: ZSTD_LEVEL
      :choices: [1-22]
      :default: 9

      Set the level of compression when using ZSTD
      compression (or LERC_ZSTD). A value of 22 is best (very slow), and 1
      is least compression.

-  .. co:: MAX_Z_ERROR
      :choices: <threshold>
      :default: 0

      Set the maximum error threshold on values
      for LERC/LERC_DEFLATE/LERC_ZSTD compression. The default is 0
      (lossless).

-  .. co:: MAX_Z_ERROR_OVERVIEW
      :choices: <threshold>
      :since: 3.8

      Set the maximum error threshold on values
      for LERC/LERC_DEFLATE/LERC_ZSTD compression, on overviews.
      The default is the value of :co:`MAX_Z_ERROR`

-  .. co:: WEBP_LEVEL
      :choices: [1-100]
      :default: 75

      Set the WEBP quality level when using WEBP
      compression. A value of 100 is best quality (least compression), and
      1 is worst quality (best compression).

-  .. co:: WEBP_LOSSLESS
      :choices: TRUE, FALSE
      :since: 2.4.0

      Requires libwebp >= 0.1.4.
      By default, lossy compression is used. If set to True, lossless
      compression will be used. There is a significant time penalty for each
      tile/strip with lossless WebP compression, so you may want to increase the
      :co:`BLOCKYSIZE` value for strip layout.

-  .. co:: JXL_LOSSLESS
      :choices: YES, NO
      :default: YES

      Set whether JPEG-XL compression should be lossless
      (YES) or lossy (NO). For lossy compression, the underlying data
      should be either gray, gray+alpha, rgb or rgb+alpha. For lossy compression,
      the pixel data should span the whole range of the underlying pixel type (i.e.
      0-255 for Byte, 0-65535 for UInt16)

-  .. co:: JXL_EFFORT
      :choices: [1-9]
      :default: 5

      Level of effort for JPEG-XL compression.
      The higher, the smaller file and slower compression time.

-  .. co:: JXL_DISTANCE
      :choices: [0.01-25]
      :default: 1.0

      (Only applies when JXL_LOSSLESS=NO)
      Distance level for lossy JPEG-XL compression.
      It is specified in multiples of a just-noticeable difference.
      (cf `butteraugli <https://github.com/google/butteraugli>`__ for the definition
      of the distance)
      That is, 0 is mathematically lossless, 1 should be visually lossless, and
      higher distances yield denser and denser files with lower and lower fidelity.
      The recommended range is [0.5,3].

-  .. co:: JXL_ALPHA_DISTANCE
      :choices: -1,0,[0.01-25]
      :default: -1
      :since: 3.7

      (Only applies when JXL_LOSSLESS=NO)
      Requires libjxl > 0.8.1.
      Distance level for alpha channel for lossy JPEG-XL compression.
      It is specified in multiples of a just-noticeable difference.
      (cf `butteraugli <https://github.com/google/butteraugli>`__ for the definition
      of the distance)
      That is, 0 is mathematically lossless, 1 should be visually lossless, and
      higher distances yield denser and denser files with lower and lower fidelity.
      For lossy compression, the recommended range is [0.5,3].
      The default value is the special value -1.0, which means to use the same
      distance value as non-alpha channel (ie JXL_DISTANCE).

-  .. co:: PHOTOMETRIC
      :choices: MINISBLACK, MINISWHITE, RGB, CMYK, YCBCR, CIELAB, ICCLAB, ITULAB

      Set the photometric interpretation tag. Default is MINISBLACK, but if
      the input image has 3 or 4 bands of Byte type, then RGB will be
      selected. You can override default photometric using this option.

-  .. co:: ALPHA
      :choices: YES, NON-PREMULTIPLIED, PREMULTIPLIED, UNSPECIFIED

      The
      first "extrasample" is marked as being alpha if there are any extra
      samples. This is necessary if you want to produce a greyscale TIFF
      file with an alpha band (for instance). YES is an alias
      for NON-PREMULTIPLIED alpha.

-  .. co:: PROFILE
      :choices: GDALGeoTIFF, GeoTIFF, BASELINE
      :default: GDALGeoTIFF

      Control what non-baseline tags are emitted by GDAL.

      -  With ``GDALGeoTIFF`` (the default) various GDAL custom tags may be
         written.
      -  With ``GeoTIFF`` only GeoTIFF tags will be added to the baseline.
      -  With ``BASELINE`` no GDAL or GeoTIFF tags will be written.
         BASELINE is occasionally useful when writing files to be read by
         applications intolerant of unrecognized tags.

-  .. co:: BIGTIFF
      :choices: YES, NO, IF_NEEDED, IF_SAFER
      :default: IF_NEEDED

      Control whether the created file is a BigTIFF or a classic TIFF.

      -  ``YES`` forces BigTIFF.
      -  ``NO`` forces classic TIFF.
      -  ``IF_NEEDED`` will only create a BigTIFF if it is clearly needed (in
         the uncompressed case, and image larger than 4GB. So no effect
         when using a compression).
      -  ``IF_SAFER`` will create BigTIFF if the resulting file \*might\*
         exceed 4GB. Note: this is only a heuristic that might not always
         work depending on compression ratios.

      BigTIFF is a TIFF variant which can contain more than 4GiB of data
      (size of classic TIFF is limited by that value). This option is
      available if GDAL is built with libtiff library version 4.0 or
      higher.

      When creating a new GeoTIFF with no compression, GDAL computes in
      advance the size of the resulting file. If that computed file size is
      over 4GiB, GDAL will automatically decide to create a BigTIFF file.
      However, when compression is used, it is not possible in advance to
      known the final size of the file, so classical TIFF will be chosen.
      In that case, the user must explicitly require the creation of a
      BigTIFF with :co:`BIGTIFF=YES` if the final file is anticipated to be too
      big for classical TIFF format. If BigTIFF creation is not explicitly
      asked or guessed and the resulting file is too big for classical
      TIFF, libtiff will fail with an error message like
      "TIFFAppendToStrip:Maximum TIFF file size exceeded".

-  .. co:: PIXELTYPE
      :choices: DEFAULT, SIGNEDBYTE

      By setting this to ``SIGNEDBYTE``, a
      new Byte file can be forced to be written as signed byte.
      Starting with GDAL 3.7, this option is deprecated and Int8 should rather
      be used.

-  .. co:: COPY_SRC_OVERVIEWS
      :choices: YES, NO
      :default: NO

      Used by (:cpp:func:`CreateCopy` only)
      By setting this to YES, the potential existing
      overviews of the source dataset will be copied to the target dataset
      without being recomputed. This option is typically used to generate
      Cloud Optimized Geotiff (starting with GDAL 3.1, the :ref:`raster.cog` driver
      can be used as a convenient shortcut). If overviews of mask band also exist,
      provided that the :config:`GDAL_TIFF_INTERNAL_MASK` configuration option is set
      to YES (which is the case starting with GDAL 3.9), they will also be copied.
      Note that this creation option will
      have `no effect <http://trac.osgeo.org/gdal/ticket/3917>`__ if
      general options (i.e. options which are not creation options) of
      gdal_translate are used. Creation options related to compression are
      also applied to the output overviews.

-  .. co:: STREAMABLE_OUTPUT
      :choices: YES, NO

      Generate a file with an Image File Directory and block order that allow
      streaming. See `Streaming operations`_.

-  .. co:: GEOTIFF_KEYS_FLAVOR
      :choices: STANDARD, ESRI_PE
      :since: 2.1.0
      :default: STANDARD

      Determine which "flavor" of GeoTIFF keys must be used to write the SRS
      information. The STANDARD way (default choice) will use the general
      accepted formulations of GeoTIFF keys, including extensions of the
      values accepted for ProjectedCSTypeGeoKey to new EPSG codes. The
      ESRI_PE flavor will write formulations that are (more) compatible of
      ArcGIS. At the time of writing, the ESRI_PE choice has mostly an
      effect when writing the EPSG:3857 (Web Mercator) SRS. For other SRS,
      the standard way will be used, with the addition of a ESRI_PE WKT
      string as the value of PCSCitationGeoKey.

-  .. co:: GEOTIFF_VERSION
      :choices: AUTO, 1.0, 1.1
      :since: 3.1.0
      :default: AUTO

      Select the version of
      the GeoTIFF standard used to encode georeferencing information. ``1.0``
      corresponds to the original
      `1995, GeoTIFF Revision 1.0, by Ritter & Ruth <http://geotiff.maptools.org/spec/geotiffhome.html>`_.
      ``1.1`` corresponds to the OGC standard 19-008, which is an evolution of 1.0,
      which clear ambiguities and fix inconsistencies mostly in the processing of
      the vertical part of a CRS.
      ``AUTO`` mode (default value) will generally select 1.0, unless the CRS to
      encode has a vertical component or is a 3D CRS, in which case 1.1 is used.

      .. note:: Write support for GeoTIFF 1.1 requires libgeotiff 1.6.0 or later.

-  .. co:: COLOR_TABLE_MULTIPLIER
      :choices: 1, 256, 257
      :since: 3.10.0
      :default: 257

      Specifies the value by which to multiply GDAL color table entry values, usually
      in [0,255] range, to obtain a TIFF color map value. Since GDAL 2.3.0,
      GDAL consistently uses 257, but it might be necessary to use 256 for
      compatibility with files generated by other software.

Subdatasets
~~~~~~~~~~~

Multi-page TIFF files are exposed as subdatasets. On opening, a
subdataset name is GTIFF_DIR:{index}:filename.tif, where {index} starts
at 1.

Starting with GDAL 3.0, subdataset creation is possible by using the
APPEND_SUBDATASET=YES creation option. The filename passed to Create() /
CreateCopy() should be the regular filename (not with GTIFF_DIR: syntax.
Creating overviews on a multi-page TIFF is not supported.

Starting with GDAL 3.2, read-only access to subdataset overviews and masks
is possible provided that they are referenced by their parent IFD through
the `TIFFTAG_SUBIFD <https://www.awaresystems.be/imaging/tiff/tifftags/subifds.html>`__ tag.

About JPEG compression of RGB images
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

When translating a RGB image to JPEG-In-TIFF, using PHOTOMETRIC=YCBCR
can make the size of the image typically 2 to 3 times smaller than the
default photometric value (RGB). When using PHOTOMETRIC=YCBCR, the
INTERLEAVE option must be kept to its default value (PIXEL), otherwise
libtiff will fail to compress the data.

Note also that the dimensions of the tiles or strips must be a multiple
of 8 for PHOTOMETRIC=RGB or 16 for PHOTOMETRIC=YCBCR

Lossless conversion of JPEG into JPEG-in-TIFF
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

The conversion of a JPEG file (but *not* a JPEG-in-TIFF file) to a JPEG-in-TIFF
file without decompression and compression cycles, and thus without any additional
quality loss, can be done with gdal_translate (or the CreateCopy() API),
if all the following conditions are met:

- the source dataset is a JPEG file (or a VRT with a JPEG as a single SimpleSource)
- the target dataset is a JPEG-in-TIFF file
- no explicitly target JPEG quality is specified
- no change in colorspace is specified
- no sub-windowing is requested
- and more generally, no change that alters pixel values

The generation of a tiled JPEG-in-TIFF from the original JPEG image is possible.
Explicit assignment of target SRS and bounds are also possible.

So, the following commands will use the lossless copy method :

::

    gdal_translate in.jpg out.tif -co COMPRESS=JPEG

    gdal_translate in.jpg out.tif -co COMPRESS=JPEG -co TILED=YES

    gdal_translate in.jpg out.tif -co COMPRESS=JPEG -a_srs EPSG:4326 -a_ullr -180 90 180 -90


whereas the following commands will *not* (and thus cause JPEG decompression and
compression):

::

    gdal_translate in.jpg out.tif -co COMPRESS=JPEG -co JPEG_QUALITY=60

    gdal_translate in.jpg out.tif -srcwin 0 0 500 500 -co COMPRESS=JPEG


Streaming operations
~~~~~~~~~~~~~~~~~~~~

The GeoTIFF driver can support reading or
writing TIFF files (with some restrictions detailed below) in a
streaming compatible way.

When reading a file from /vsistdin/, a named pipe (on Unix), or if
forcing streamed reading by setting the :config:`TIFF_READ_STREAMING`
configuration option to YES, the GeoTIFF driver will assume that the
TIFF Image File Directory (IFD) is at the beginning of the file, i.e. at
offset 8 for a classical TIFF file or at offset 16 for a BigTIFF file.
The values of the tags of array type must be contained at the beginning
of file, after the end of the IFD and before the first image strip/tile.
The reader must read the strips/tiles in the order they are written in
the file. For a pixel interleaved file (PlanarConfiguration=Contig), the
recommended order for a writer, and thus for a reader, is from top to
bottom for a strip-organized file or from top to bottom, which a chunk
of a block height, and left to right for a tile-organized file. For a
band organized file (PlanarConfiguration=Separate), the above order is
recommended with the content of the first band, then the content of the
second band, etc... Technically this order corresponds to increasing
offsets in the TileOffsets/StripOffsets tag. This is the order that the
GDAL raster copy routine will assume.

If the order is not the one described above, the UNORDERED_BLOCKS=YES
dataset metadata item will be set in the TIFF metadata domain. Each
block offset can be determined by querying the
"BLOCK_OFFSET_[xblock]_[yblock]" band metadata items in the TIFF
metadata domain (where xblock, yblock is the coordinate of the block),
and a reader could use that information to determine the appropriate
reading order for image blocks.

The files that are streamed into the GeoTIFF driver may be compressed,
even if the GeoTIFF driver cannot produce such files in streamable
output mode (regular creation of TIFF files will produce such compatible
files for streamed reading).

When writing a file to /vsistdout/, a named pipe (on Unix), or when
defining the :co:`STREAMABLE_OUTPUT=YES` creation option, the CreateCopy()
method of the GeoTIFF driver will generate a file with the above defined
constraints (related to position of IFD and block order), and this is
only supported for a uncompressed file. The Create() method also
supports creating streamable compatible files, but the writer must be
careful to set the projection, geotransform or metadata before writing
image blocks (so that the IFD is written at the beginning of the file).
And when writing image blocks, the order of blocks must be the one of
the above paragraph, otherwise errors will be reported.

Some examples :

::

   gdal_translate in.tif /vsistdout/ -co TILED=YES | gzip | gunzip | gdal_translate /vsistdin/ out.tif -co TILED=YES -co COMPRESS=DEFLATE

or

::

   mkfifo my_fifo
   gdalwarp in.tif my_fifo -t_srs EPSG:3857
   gdal_translate my_fifo out.png -of PNG

Note: not all utilities are compatible with such input or output
streaming operations, and even those which may deal with such files may
not manage to deal with them in all circumstances, for example if the
reading driver driven by the output file is not compatible with the
block order of the streamed input.

Configuration options
~~~~~~~~~~~~~~~~~~~~~

|about-config-options|
This paragraph lists the configuration options that can be set to alter
the default behavior of the GTiff driver.

-  .. config:: GTIFF_IGNORE_READ_ERRORS
      :choices: TRUE, FALSE

      Can be set to TRUE to avoid turning libtiff errors into GDAL errors. Can
      help reading partially corrupted TIFF files.

-  .. config:: ESRI_XML_PAM
      :choices: TRUE, FALSE

      Can be set to TRUE to force metadata in the xml:ESRI
      domain to be written to PAM.

-  .. config:: BIGTIFF_OVERVIEW

      Control whether BigTIFF should be used for overviews. Options are the same as :co:`BIGTIFF` creation option.

-  .. config:: COMPRESS_OVERVIEW

      See :co:`COMPRESS` creation option.
      Set the compression type to use for overviews. For internal overviews, only honoured since GDAL 3.6.

-  .. config:: INTERLEAVE_OVERVIEW
      :choices: BAND, PIXEL

      Control whether pixel or band interleaving is used for overviews.

-  .. config:: PHOTOMETRIC_OVERVIEW

      Set the photometric color space for overview creation

-  .. config:: PREDICTOR_OVERVIEW
      :choices: 1, 2, 3

      Set the predictor to use for overviews with LZW, DEFLATE and ZSTD compression.

-  .. config:: JPEG_QUALITY_OVERVIEW
      :choices: Integer between 0 and 100
      :default: 75

      Quality of JPEG compressed overviews, either internal or external.

-  .. config:: WEBP_LEVEL_OVERVIEW
      :choices: Integer between 0 and 100
      :default: 75

      WEBP quality level of overviews, either internal or external.

-  .. config:: WEBP_LOSSLESS_OVERVIEW
      :choices: YES, NO
      :default: NO
      :since: 3.6

      Whether WEBP compression is lossless or not.

-  .. config:: ZLEVEL_OVERVIEW
      :choices: Integer between 1 and 9 (or 12 when libdeflate is used)
      :default: 6
      :since: 3.4.1

      Deflate compression level of overviews, for COMPRESS_OVERVIEW=DEFLATE or LERC_DEFLATE, either internal or external.

-  .. config:: ZSTD_LEVEL_OVERVIEW
      :choices: Integer between 1 and 22
      :default: 9
      :since: 3.4.1

      ZSTD compression level of overviews, for COMPRESS_OVERVIEW=DEFLATE or LERC_ZSTD, either internal or external.

-  .. config:: MAX_Z_ERROR_OVERVIEW
      :default: 0 (lossless)
      :since: 3.4.1

      Maximum error threshold on values for LERC/LERC_DEFLATE/LERC_ZSTD compression of overviews, either internal or external.

-  .. config:: SPARSE_OK_OVERVIEW
      :choices: ON, OFF
      :default: OFF
      :since: 3.4.1

      When set to ON, blocks whose pixels are all at nodata (or 0 if no nodata is defined)

-  .. config:: GDAL_TIFF_INTERNAL_MASK
      :choices: TRUE, FALSE
      :default: TRUE (since GDAL 3.9), FALSE (GDAL 3.8 or earlier)

      See `Internal nodata masks`_ section

-  .. config:: GDAL_TIFF_INTERNAL_MASK_TO_8BIT
      :choices: TRUE, FALSE
      :default: TRUE

      See `Internal nodata masks`_ section.

-  :config:`USE_RRD`: Can be set to TRUE to force external overviews in the RRD
   format.

-  .. config:: TIFF_USE_OVR
      :choices: TRUE, FALSE
      :default: FALSE

      Can be set to TRUE to force external overviews in the GeoTIFF (.ovr) format.

-  .. config:: TIFF_READ_STREAMING
      :choices: YES, NO

      If ``YES``, assume that Image File Directory is at the beginning of the file.
      See `Streaming operations`_.

-  .. config:: GTIFF_POINT_GEO_IGNORE
      :choices: TRUE, FALSE
      :default: FALSE

      Can be set to TRUE to revert back to the
      behavior of ancient GDAL versions regarding how PixelIsPoint is interpreted
      w.r.t geotransform. See :ref:`rfc-33` for more details.

-  .. config:: GTIFF_REPORT_COMPD_CS
      :choices: TRUE, FALSE

      Can be set to TRUE to avoid
      stripping the vertical CRS of compound CRS when reading the SRS of a
      file. Does not affect the writing side. Default value : FALSE for GeoTIFF 1.0
      files, or TRUE (starting with GDAL 3.1) for GeoTIFF 1.1 files.

-  .. config:: GDAL_ENABLE_TIFF_SPLIT
      :choices: TRUE, FALSE
      :default: TRUE

      Can be set to FALSE to avoid
      all-in-one-strip files being presented as having.

-  .. config:: GDAL_TIFF_OVR_BLOCKSIZE

      See `Overviews`_ section.

-  .. config:: GTIFF_LINEAR_UNITS

      Can be set to BROKEN to read GeoTIFF files that
      have false easting/northing improperly set in meters when it ought to
      be in coordinate system linear units. (`Ticket
      #3901 <http://trac.osgeo.org/gdal/ticket/3901>`__).

-  .. config:: TAB_APPROX_GEOTRANSFORM
      :choices: YES, NO
      :default: NO

      To decide if an approximate geotransform is acceptable when reading a .tab
      file.

-  .. config:: GTIFF_DIRECT_IO
      :choices: YES, NO
      :default: NO

      Can be set to YES to use
      specialized RasterIO() implementations when reading un-compressed
      TIFF files (un-tiled only in GDAL 2.0, both un-tiled and tiled in
      GDAL 2.1) to avoid using the block cache. Setting it to YES even when
      the optimized cases do not apply should be safe (generic
      implementation will be used).

-  .. config:: GTIFF_VIRTUAL_MEM_IO
      :choices: YES, NO, IF_ENOUGH_RAM
      :default: NO

      Can be set
      to YES to use specialized RasterIO() implementations when reading
      un-compressed TIFF files to avoid using the block cache. This
      implementation relies on memory-mapped file I/O, and is currently
      only supported on Linux (64-bit build strongly recommended) or,
      starting with GDAL 2.1, on other POSIX-like systems. Setting it to
      YES even when the optimized cases do not apply should be safe
      (generic implementation will be used), but if the file exceeds RAM,
      disk swapping might occur if the whole file is read. Setting it to
      IF_ENOUGH_RAM will first check if the uncompressed file size is no
      bigger than the physical memory. If both
      :config:`GTIFF_VIRTUAL_MEM_IO` and :config:`GTIFF_DIRECT_IO` are enabled, the former is
      used in priority, and if not possible, the later is tried.

-  :config:`GDAL_NUM_THREADS` enables multi-threaded compression by specifying the number of worker
   threads. Worth it for slow compression algorithms such as DEFLATE or
   LZMA. Will be ignored for JPEG. Default is compression in the main
   thread. Note: this configuration option also apply to other parts to
   GDAL (warping, gridding, ...).
   Starting with GDAL 3.6, this option also enables multi-threaded decoding
   when RasterIO() requests intersect several tiles/strips.

-  .. config:: GTIFF_WRITE_TOWGS84
      :choices: AUTO, YES, NO
      :since: 3.0.3

      When set to AUTO, a
      GeogTOWGS84GeoKey geokey will be written with TOWGS84 3 or 7-parameter
      Helmert transformation, if the CRS has no EPSG code attached to it, or if
      the TOWGS84 transformation attached to the CRS doesn't match the one imported
      from the EPSG code.
      If set to YES, then the TOWGS84 transformation attached to the CRS will be
      always written. If set to NO, then the transformation will not be written in
      any situation.

-  .. config:: CHECK_DISK_FREE_SPACE
      :choices: YES, NO
      :default: YES

      If ``YES``, ensure that enough disk space is available before attempting to
      write an uncompressed, non-sparse GeoTIFF. Disabling this check is not
      expected to be necessary, unless GDAL is incorrectly determining the disk
      space available on the destination file system.

-  .. config:: GTIFF_READ_ANGULAR_PARAMS_IN_DEGREE
      :choices: YES, NO
      :default: NO
      :since: 3.9.1

      Conformant GeoTIFF files should have the values of angular projection
      parameters written in the unit of the GeogAngularUnitsGeoKey. But some
      non-conformant implementations, such as GDAL <= 3.9.0, always wrote them
      in degrees.
      This option can be set to YES when reading such non-conformant GeoTIFF
      files (typically using grads), to instruct GDAL (>= 3.9.1) that the projection
      parameters are in degrees, instead of being expressed in the unit of the
      GeogAngularUnitsGeoKey.

-  .. config:: GTIFF_WRITE_ANGULAR_PARAMS_IN_DEGREE
      :choices: YES, NO
      :default: NO
      :since: 3.9.1

      Conformant GeoTIFF files should have the values of angular projection
      parameters written in the unit of the GeogAngularUnitsGeoKey. But some
      non-conformant implementations, such as GDAL >= 3.0 and <= 3.9.0, assumed
      those values to be in degree.
      This option can be set to YES to force writing such non-conformant GeoTIFF
      files. It should *not* be nominally used, except to workaround interoperability
      issues.


Codec Recommendations
---------------------


LZW
~~~

If you don't know what to choose, choose this one.

DEFLATE
~~~~~~~

The most commonly supported TIFF codec, especially with older non-geo software.

LERC
~~~~

Used for storing quantized floating point data. https://github.com/esri/lerc


ZSTD
~~~~

Smaller and faster than DEFLATE, but not as commonly supported.

WEBP
~~~~

A smaller and faster JPEG.

JXL
~~~

Next-gen JPG from the JPG group.


LZMA
~~~~

Slow but storage efficient.

CCITTRLE/CCITTFAX3/CCITTFAX4
~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Did you happen to have fax files from the 1990s? Use these.

See Also
--------

-  `GeoTIFF Information Page <https://trac.osgeo.org/geotiff>`__
-  `libtiff Page <http://www.simplesystems.org/libtiff/>`__
-  `Details on BigTIFF file
   format <http://www.awaresystems.be/imaging/tiff/bigtiff.html>`__
- :ref:`raster.cog` driver

.. toctree::
   :maxdepth: 1
   :hidden:

   wld
