# SIGDEM -- Scaled Integer Gridded DEM

Driver short name

SIGDEM

Added in version 2.4.

Driver built-in by default

This driver is built-in by default

The SIGDEM driver supports reading and writing Scaled Integer Gridded DEM files.

SIGDEM files contain exactly 1 band. The in-memory band data is stored using GDT_Float64.

SIGDEM prefers use of an EPSG ID inside the file for coordinate systems. Only if the spatial reference doesn't have an EPSG ID will a .prj file be written or read.

NOTE: Implemented as sigdemdataset.cpp.

## Driver capabilities

Supports CreateCopy()

This driver supports the `GDALDriver::CreateCopy()` operation

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)