# `gdal raster pixel-info`

Added in version 3.11.

Return information on a pixel of a raster dataset

## Synopsis

    Usage: gdal raster pixel-info [OPTIONS] <INPUT> [<column,line> or <X,Y>]

    Return information on a pixel of a raster dataset.

    Positional arguments:
      -i, --dataset, --input <INPUT>                       Input raster dataset [required]
      -p, --pos, --position <column,line> or <X,Y>         Pixel position [may be repeated]

    Common Options:
      -h, --help                                           Display help message and exit
      --json-usage                                         Display usage as JSON document and exit
      --config <KEY>=<VALUE>                               Configuration option [may be repeated]

    Options:
      -f, --of, --format, --output-format <OUTPUT-FORMAT>  Output format. OUTPUT-FORMAT=geojson|csv (default: geojson)
      -b, --band <BAND>                                    Input band(s) (1-based index) [may be repeated]
      --overview <OVERVIEW>                                Which overview level of source file must be used
      --position-crs <POSITION-CRS>                        CRS of position (default: pixel)
      -r, --resampling <RESAMPLING>                        Resampling algorithm for interpolation. RESAMPLING=nearest|bilinear|cubic|cubicspline (default: nearest)

    Advanced Options:
      --oo, --open-option <KEY>=<VALUE>                    Open options [may be repeated]
      --if, --input-format <INPUT-FORMAT>                  Input formats [may be repeated]

## Description

gdal raster pixel-info provide a mechanism to query information about a pixel given its location in one of a variety of coordinate systems.

It supports outputting either as GeoJSON or CSV.

The following items will be reported (when known):

- Input coordinates

- Input coordinates converted to column, line

- Pixel value per selected band(s), with unscaled value

- For VRT files, which file(s) contribute to the pixel value.

The following options are available:

### Standard options

-f, --of, --format, --output-format geojson|csv

  Which output format to use. Default is GeoJSON.

--oo, --open-option <NAME>=<VALUE>

  Dataset open option (format specific).

  May be repeated.

--if, --input-format <format>

  Format/driver name to be attempted to open the input file(s). It is generally not necessary to specify it, but it can be used to skip automatic driver detection, when it fails to select the appropriate driver. This option can be repeated several times to specify several candidate drivers. Note that it does not force those drivers to open the dataset. In particular, some drivers have requirements on file extensions.

  May be repeated.

-b <band>

  Selects a band to query. Multiple bands can be listed. By default all bands are queried.

-p, --pos, --position <column,line> or <X,Y>

  Required. This can be specified either as an option, a positional value after the dataset name, or when called from gdal, as (space separated) values provided on the standard input.

  By default, when `--position-crs` is not specified, or set to `pixel`, this is a column, line tuple (possibly with fractional part). If `--position-crs` is set to `dataset`, this is a georeferenced coordinate expressed in the CRS of the dataset. If `--position-crs` is specified to a CRS definition, this is a georeferenced coordinate expressed in this CRS.

  X means always longitude or easting, Y means always latitude or northing.

  Several x,y tuples may be specified.

--position-crs pixel|dataset|<crs-def>

  CRS of position, or one of two following special values:

  - `pixel` means that the position is set as column, line (default)

  - `dataset` means that the position is a georeferenced coordinate expressed in the CRS of the dataset.

-r, --resampling nearest|bilinear|cubic|cubicspline

  Select a sampling algorithm. The default is `nearest`.

  The available methods are:

  - `nearest` applies a nearest neighbour.

  - `bilinear` applies a bilinear convolution kernel.

  - `cubic` applies a cubic convolution kernel.

  - `cubicspline` applies a B-Spline convolution kernel.

--ovr, --overview <index>

  Query the (overview_level)th overview (overview_level=0 is the 1st overview), instead of the base band. Note that the x,y location (if the coordinate system is pixel/line) must still be given with respect to the base band.

## Examples

### Example 1: Reporting on pixel column=5, line=10 on the file `byte.tif`

    $ gdal raster pixel-info byte.tif 5 10
    {
      "type":"FeatureCollection",
      "crs":{
        "type":"name",
        "properties":{
          "name":"urn:ogc:def:crs:EPSG::26711"
        }
      },
      "features":[
        {
          "type":"Feature",
          "properties":{
            "input_coordinate":[
              5.0,
              10.0
            ],
            "column":5.0,
            "line":10.0,
            "bands":[
              {
                "band_number":1,
                "raw_value":132,
                "unscaled_value":132.0
              }
            ]
          },
          "geometry":{
            "type":"Point",
            "coordinates":[
              441020.0,
              3750720.0
            ]
          }
        }
      ]
    }

### Example 2: Reporting on point at UTM 11N coordinates easting=441320 and northing=3750720 on the file `byte.tif`

    $ gdal raster pixel-info --position-crs=dataset byte.tif 441320 3750720
    {
      "type":"FeatureCollection",
      "crs":{
        "type":"name",
        "properties":{
          "name":"urn:ogc:def:crs:EPSG::26711"
        }
      },
      "features":[
        {
          "type":"Feature",
          "properties":{
            "input_coordinate":[
              441320.0,
              3750720.0
            ],
            "column":10.0,
            "line":10.0,
            "bands":[
              {
                "band_number":1,
                "raw_value":115,
                "unscaled_value":115.0
              }
            ]
          },
          "geometry":{
            "type":"Point",
            "coordinates":[
              441320.0,
              3750720.0
            ]
          }
        }
      ]
    }

### Example 3: Reporting on point at WGS84 coordinates longitude=-117.6355 and latitude=33.8970 on the file `byte.tif`, with CSV output format

    $ gdal raster pixel-info --of=csv --position-crs=WGS84 byte.tif -117.6355 33.8970
    input_x,input_y,extra_input,column,line,band_1_raw_value,band_1_unscaled_value
    -117.63549999999999,33.896999999999998,"",10.020546288988044,9.9833047347492538,115,115

### Example 4: Reporting on point at WGS84 coordinates provided on the standard input with longitude, latitude order.

    $ echo -117.6355 33.8970 | gdal raster pixel-info --of=csv --position-crs=WGS84 byte.tif
    -117.6355 33.8970 | gdal raster pixel-info --of=csv --position-crs=WGS84 byte.tif