# gdal_fillnodata

Fill raster regions by interpolation from edges.

## Synopsis

    gdal_fillnodata [--help] [--help-general] [-q] [-md <max_distance>]
               [-si <smoothing_iterations>] [-o <name>=<value> [<name>=<value> ...]]
               [-mask <filename>] [-interp {inv_dist,nearest}] [-b <band>]
               [-of <gdal_format>] [-co <name>=<value>]
               <src_file> <dst_file>

## Description

gdal_fillnodata fills selection regions (usually nodata areas) by interpolating from valid pixels around the edges of the area.

Additional details on the algorithm are available in the `GDALFillNodata()` docs.

Tip

Equivalent in new "gdal" command line interface:

See gdal raster fill-nodata.

Note

gdal_fillnodata is a Python utility, and is only available if GDAL Python bindings are available.

--help

  Show this help message and exit

--help-general

  Gives a brief usage message for the generic GDAL commandline options and exit.

-q

  The script runs in quiet mode. The progress monitor is suppressed and routine messages are not displayed.

-md <max_distance>

  The maximum distance (in pixels) that the algorithm will search out for values to interpolate. The default is 100 pixels.

-si <smooth_iterations>

  The number of 3x3 average filter smoothing iterations to run after the interpolation to dampen artifacts. The default is zero smoothing iterations.

-o <name>=<value>

  Specify a special argument to the algorithm. Currently none are supported.

-b <band>

  The band to operate on, by default the first band is operated on.

-mask <filename>

  Use the first band of the specified file as a validity mask (zero is invalid, non-zero is valid).

-of <format>

  Select the output format. The default is GTiff -- GeoTIFF File Format. Use the short format name.

-interp {inv_dist,nearest}

  Added in version 3.9.

  By default, pixels are interpolated using an inverse distance weighting (`inv_dist`). It is also possible to choose a nearest neighbour (`nearest`) strategy.

<srcfile>

  The source raster file used to identify target pixels. Only one band is used.

<dstfile>

  The new file to create with the interpolated result.