# RFC 108: Driver removals for GDAL 3.11

Author: | Even Rouault
Contact: | even.rouault @ spatialys.com
Started: | 2025-02-18
Status: | Adopted, implemented
Target: | GDAL 3.11

## Summary

This RFC communicates about the partial or total removal of obsolete drivers for GDAL 3.11.

## Motivation

GDAL is an ever growing code base, with probably more than 50% of the code base being used by less of 1% of users. This is isn't very sustainable, and quite demotivating for current maintainers who know nothing/little about most drivers, have no evidence that they are used, and regularly stumble upon them when doing whole codebase enhancements. The decision of which driver to removal comes from a mix of "intuition" and community feedback from https://docs.google.com/spreadsheets/d/12yk0p8rRK4rAYO_VwXboatWkiILAjE2Cepu32lsHhM8/edit?gid=0#gid=0

## Technical solution

Fully removed drivers:

- raster:

  - JP2Lura: JPEG2000-capable driver. Was based on a proprietary SDK. Initial proponents of that driver no longer use it.

  - OZI OZF2/OZFX3: OZI now uses a new format v4 that has not been reverse engineered.

  - BLX (Magellan BLX Topo File Format). No activity in this driver from non-GDAL team. No obvious sign in issue tracker it is used.

  - XPM driver: Not relevant in a geospatial context. Obsolete image format. Users can probably use ImageMagick if support for it is needed.

  - SGI driver: same as above

  - FIT driver: No idea what it is about (not to be confused by FITS, which is actively used by astronomic/planetary community)

  - DIPEx: No idea what it is about

  - CTable2 driver: obsolete PROJ.4 grid format. There was just one file ("null") known to use that format.

  - R (R Object Data Store (`*.rda`)): not known to be used. Not to be confused with the RRaster driver which is used in the R ecosystem.

  - GSAG (Golden Software ASCII) and GSBG (Golden Software 6.0 binary): likely obsolete. GS7B (Golden Software 7.0 binary) kept as there are signs it is used.

  - Rasterlite: Rasterlite 1.0 format. Obsolete/no longer maintained by the Spatialite crew. The SQLite driver has support for Rasterlite 2

  - BT (VTP .bt Binary Terrain Format). The VTP project seems abandoned since 2015.

  - SDTS: obsolete

  - RDB (RIEGL Laser Measurement Systems GmbH): Not CI tested. Depends on proprietary SDK. Removed with agreement from RIEGL.

- vector:

  - Geoconcept export .txt: no sign it is used. Feedback from a French GIS forum when asking if someone still uses the driver: "It is not clear who still uses Geoconcept (the software) at all"

  - OGDI: Vector Product Format / DGN / VMap. All obsolete formats. The problematic part is that it depends on libogdi, which is an obsolete C code base nobody sane would want to maintain anymore.

  - SDTS: obsolete

  - SVG: only supported files from Cloudmade Vector Stream Server, which no longer exists. The code could probably be re-enabled to be made more generic and handle arbitrary SVG, if the needs arises.

  - Tiger: pre-2006 format for US Census. New datasets are in shapefile.

Write-support removal:

- raster:

  - ADRG: defense-related format. Write support was mostly to test the read side of the driver

  - ELAS: not sure what it is about and that this is actively used

  - PAux: not sure what it is about and that this is actively used

  - MFF: not sure what it is about and that this is actively used

  - MFF2/HKV: not sure what it is about and that this is actively used

  - LAN: old ERDAS format before HFA (.img). "raw format", does not support compression. Write support doesn't seem useful.

  - BYN: Canadian grid-related format. Write support doesn't seem useful

  - NTv2: read-support definitely useful. Write support obsolete since PROJ 7 and use of Geodetic TIFF Grid format.

  - USGSDEM: obsolete format. There might be historic datasets to read, but write support doesn't seem useful

  - ISIS2: Planetary format. Obsoleted by ISIS3. ISIS2 write support not used by USGS.

About/only 50,000 lines of code removed.

## Discussion

- Q. Are we sure they are not used? A. No, we aren't. We could also have used a more progressive deprecation mechanism (like requiring a runtime configuration option to be set), but we don't think it is worth the extra burden. Let's see if we get massive complaints from users, and use git revert if needed. We add a similar phase around GDAL 3.5 and as far as I remember, we just got a couple of remarks, but did not end up reviving deleted drivers.

- Q. Would a dedicated per-driver maintainer model help? A. Maybe, although in most of the above cases, most of those drivers are not problematic per-se. They are just sitting there, contributing to the overall weight of the library, and occasionally getting into our legs.

- Q: I don't see the logic in the above removals. That seems a bit random at times. A. Yes, it is. Like cognitive processes are sometimes. This is also a way to scare people contributing drivers to GDAL that we might scrap them when that becomes inconvenient.

- Q. GDAL is all about support for odd formats! Don't do this! A. Feel free to create a gdal-legacy-drivers project.

- Should we consider in the future adding telemetry in GDAL? Have looked at https://opentelemetry.io a bit. Seems a bit impressive...

## Documentation

Removed drivers will be mentioned at bottom of https://gdal.org/en/latest/drivers/raster/index.html and https://gdal.org/en/latest/drivers/vector/index.html with the mention of the version where they have been removed. This gives a way for users that would need them to use the appropriate past version(s).

## Related issues and PRs

- Candidate implementation: https://github.com/OSGeo/gdal/pull/11758 (JP2Lura and OZI have already been removed in master)

## Funding

Funded by GDAL Sponsorship Program (GSP) (this RFC text)

## Voting history

+1 from PSC members JukkaR, JavierJS, KurtS, HowardB, DanielM, and -0 from DanB.