# RFC 58: Removing Dataset Nodata Value

Authors: Sean Gillies

Contact: sean at mapbox.com

Status: Adopted, implemented

Implementation version: 2.1

## Summary

This RFC concerns addition of a `DeleteNoDataValue()` function to the C++ GDALRasterBand API. This function removes the nodata value of a raster band. When it succeeds, the raster band will have no nodata value. When it fails, the nodata value will be unchanged.

## Rationale

The nodata value has accessors `GetNoDataValue()` and `SetNoDataValue()`. For GeoTIFFs, the value is stored in a TIFFTAG_GDAL_NODATA TIFF tag. Newly created GeoTIFF files can have no nodata value (no tag), but once a nodata value is set and stored it can only be given new values, it can not be removed. Nor can it be set to a value outside the range of the data type; for 8-bit data passing `nan`, `-inf`, or `256` to `GDALSetNoDataValue()` has the same effect as passing 0.

The problem with un-removable nodata values is this:

- Nodata masks (see GDAL RFC 15) can cover up a nodata value but if the .msk file gets lost (and this is ever the problem with sidecar files), the nodata value you were hiding is exposed again.

- Nodata masks are not available everywhere in GDAL, nodata values are the only definition of valid data in some parts of GDAL.

The current recommended practice for removing a nodata value is to copy the GeoTIFF using gdal_translate, specifying that the nodata tag not be copied over along with the data. By making the nodata value fully editable and removable we could avoid copying unnecessarily.

## Changes

The `virtual CPLErr DeleteNoDataValue()` method will be added to the GDALRasterBand method in gdal_priv.h (C++ API), and `CPLErr GDALDeleteRasterNoDataValue()` to gdal.h (C API)

### Updated drivers

The following drivers will be updated: GTiff, MEM, VRT and KEA.

For GTiff, the TIFFTAG_GDAL_NODATA TIFF tag is unset if GDAL is built against libtiff 4.X, which is the appropriate behavior. For libtiff 3.X where TIFFUnsetField() does not exist, the tag is set to the empty string : GDAL 2.0 will detect that as the absence of a nodata value, older versions will parse it as 0.

The `GDALPamRasterBand` class will also be updated (for drivers that have no built-in mechanism nodata mechanism and rely on .aux.xml sidecars). Note that this only removes the tag from the .aux.xml, so in the situation where a driver would have a internal way of storing nodata, but would be opened in read-only mode (so defaulting to PAM), DeleteNoData() would have no effect.

## SWIG bindings (Python / Java / C# / Perl) changes

The DeleteNoDataValue() method is added to the RasterBand object.

## Utilities

The gdal_edit.py script is enhanced with a -unsetnodata option.

## Documentation

The new method and function are documented.

## Test Suite

The tests of the updated drivers test the effect of the new method.

## Compatibility Issues

None for the C API. ABI change for the C++ API because of introduction of a new virtual method.

## Related ticket

#2020 mentions the issue.

## Implementation

Implementation will be done by Even Rouault and be sponsored by Mapbox.

A proposed implementation is available in https://github.com/OSGeo/gdal/compare/trunk...rouault:rfc58_removing_nodata_value

## Voting history

+1 from EvenR, HowardB, DanielM and JukkaR