# DODS – OPeNDAP Grid Client

Driver short name

DODS

Build dependencies

libdap

GDAL optionally includes read support for 2D grids and arrays via the OPeNDAP (DODS) protocol.

## Driver capabilities

Supports Georeferencing

This driver supports georeferencing

## Dataset Naming

The full dataset name specification consists of the OPeNDAP dataset url, the full path to the desired array or grid variable, and an indicator of the array indices to be accessed.

For instance, if the url http://maps.gdal.org/daac-bin/nph-hdf/3B42.HDF.dds returns a DDS definition like this:

    Dataset {
      Structure {
        Structure {
          Float64 precipitate[scan = 5][longitude = 360][latitude = 80];
          Float64 relError[scan = 5][longitude = 360][latitude = 80];
        } PlanetaryGrid;
      } DATA_GRANULE;
    } 3B42.HDF;

then the precipitate grid can be accessed using the following GDAL dataset name:

http://maps.gdal.org/daac-bin/nph-hdf/3B42.HDF?DATA_GRANULE.PlanetaryGrid.precipitate[0][x][y]

The full path to the grid or array to be accessed needs to be specified (not counting the outer Dataset name). GDAL needs to know which indices of the array to treat as x (longitude or easting) and y (latitude or northing). Any other dimensions need to be restricted to a single value.

In cases of data servers with only 2D arrays and grids as immediate children of the Dataset it may not be necessary to name the grid or array variable.

In cases where there are a number of 2D arrays or grids at the dataset level, they may be each automatically treated as separate bands.

## Specialized AIS/DAS Metadata

A variety of information will be transported via the DAS describing the dataset. Some DODS drivers (such as the GDAL based one!) already return the following DAS information, but in other cases it can be supplied locally using the AIX mechanism. See the DODS documentation for details of how the AIS mechanism works.

    Attributes {

        GLOBAL {
            Float64 Northernmost_Northing 71.1722;
        Float64 Southernmost_Northing  4.8278;
        Float64 Easternmost_Easting  -27.8897;
        Float64 Westernmost_Easting -112.11;
            Float64 GeoTransform "71.1722 0.001 0.0 -112.11 0.0 -0.001";
        String spatial_ref "GEOGCS[\"WGS 84\",DATUM[\"WGS_1984\",SPHEROID[\"WGS 84\",6378137,298.257223563]],PRIMEM[\"Greenwich\",0],UNIT[\"degree\",0.0174532925199433]]";
            Metadata {
              String TIFFTAG_XRESOLUTION "400";
              String TIFFTAG_YRESOLUTION "400";
              String TIFFTAG_RESOLUTIONUNIT "2 (pixels/inch)";
            }
        }

        band_1 {
            String Description "...";
            String
        }
    }

### Dataset

There will be an object in the DAS named GLOBAL containing attributes of the dataset as a whole.

It will have the following subitems:

- Northernmost_Northing: The latitude or northing of the north edge of the image.

- Southernmost_Northing: The latitude or northing of the south edge of the image.

- Easternmost_Easting: The longitude or easting of the east edge of the image.

- Westernmost_Easting: The longitude or easting of the west edge of the image.

- GeoTransform: The six parameters defining the affine transformation between pixel/line space and georeferenced space if applicable. Stored as a single string with values separated by spaces. Note this allows for rotated or sheared images. (optional)

- SpatialRef: The OpenGIS WKT description of the coordinate system. If not provided it will be assumed that the coordinate system is WGS84. (optional)

- Metadata: a container with a list of string attributes for each available metadata item. The metadata item keyword name will be used as the attribute name. Metadata values will always be strings. (optional)

- address GCPs

Note that the edge northing and easting values can be computed based on the grid size and the geotransform. They are included primarily as extra documentation that is easier to interpret by a user than the GeoTransform. They will also be used to compute a GeoTransform internally if one is note provided, but if both are provided the GeoTransform will take precedence.

### Band

There will be an object in the DAS named after each band containing attribute of the specific band.

It will have the following subitems:

- Metadata: a container with a list of string attributes for each available metadata item. The metadata item keyword name will be used as the attribute name. Metadata values will always be strings. (optional)

- PhotometricInterpretation: Will have a string value that is one of “Undefined”, “GrayIndex”, “PaletteIndex”, “Red”, “Green”, “Blue”, “Alpha”, “Hue”, “Saturation”, “Lightness”, “Cyan”, “Magenta”, “Yellow” or “Black”. (optional)

- units: name of units (one of “ft” or “m” for elevation data). (optional)

- add_offset: Offset to be applied to pixel values (after scale_factor) to compute a “real” pixel value. Defaults to 0.0. (optional)

- scale_factor: Scale to be applied to pixel values (before add_offset) to compute “real” pixel value. Defaults to 1.0. (optional)

- Description: Descriptive text about the band. (optional)

- missing_value: The nodata value for the raster. (optional)

- Colormap: A container with a subcontainer for each color in the color table, looking like the following. The alpha component is optional and assumed to be 255 (opaque) if not provided.

      Colormap {
        Color_0 {
          Byte red 0;
          Byte green 0;
          Byte blue 0;
          Byte alpha 255;
        }
        Color_1 {
          Byte red 255;
          Byte green 255;
          Byte blue 255;
          Byte alpha 255;
        }
        ...
      }

## See Also

- OPeNDAP Website