# ARG – Azavea Raster Grid

Driver short name

ARG

Driver built-in by default

This driver is built-in by default

Driver implementation for a raw format that is used in GeoTrellis and called ARG. ARG format specification. Format is essentially a raw format, with a companion .JSON file.

NOTE: Implemented as `gdal/frmts/arg/argdataset.cpp`.

## Driver capabilities

Supports CreateCopy()

This driver supports the `GDALDriver::CreateCopy()` operation

Supports Create()

This driver supports the `GDALDriver::Create()` operation

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)