# SEG-P1 / UKOOA P1/90

Driver short name

SEGUKOOA

Driver built-in by default

This driver is built-in by default

This driver reads files in SEG-P1 and UKOOA P1/90 formats. Those files are simple ASCII files that contain seismic shotpoints. Two layers are reported : one with the points, and another ones where sequential points with same line name are merged together in a single feature with a line geometry.

## Driver capabilities

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)

## See Also

- Description of SEG-P1 format

- Description of UKOOA P1/90 format