.. _raster.db2:

================================================================================
DB2 raster
================================================================================

.. shortname:: DB2

.. build_dependencies:: ODBC (and any or all of PNG, JPEG, WEBP drivers)

.. note::

    The DB2 driver is based largely on the source code for the OGR/DB2
    GeoPackage (GPKG) driver, replaceing SQLITE functionality with
    corresponding DB2 functionality. Appreciation is expressed for the major
    development required to produce the GeoPackage driver which dramatically
    reduced the effort to produce the DB2 driver. At some point it may be
    worthwhile to explore whether refactoring of the class structure to
    share common functionality is practical.

    The DB2 driver largely implements the GeoPackage standard, with the main
    difference that the "gpkg\_" prefix is replaced with "gpkg." in the DB2
    table name, assigning them to a distinct database schema.

    The documentation below is largely copied from the
    :ref:`raster.gpkg` documentation. References to the GeoPackage
    standard have been left as such. References to the implementation have
    been changed to DB2. In some cases it isn't clear whether we should
    refer to "DB2 tiles" or "GeoPackage tiles".

This driver implements full read/creation/update
of tables containing raster tiles in the `OGC GeoPackage format
standard <http://www.geopackage.org/spec/>`__. The GeoPackage standard
uses a SQLite database file as a generic container, and the standard
defines:

-  Expected metadata tables (``gpkg.contents``,
   ``gpkg.spatial_ref_sys``, ``gpkg.tile_matrix``,
   ``gpkg.tile_matrix_set``, ...)
-  Tile format encoding (PNG and JPEG for base specification, WebP as
   extension) and tiling conventions
-  Naming and conventions for extensions

This driver reads and writes DB2 tables in the DB2 database, so it must
be run by a user with create authority on the database it is working
with.

The driver can also handle DB2 vectors. See :ref:`DB2
vector <vector.db2>` documentation page

Various kind of input datasets can be converted to DB2 raster :

-  Single band grey level
-  Single band with R,G,B or R,G,B,A color table
-  Two bands: first band with grey level, second band with alpha channel
-  Three bands: Red, Green, Blue
-  Four band: Red, Green, Blue, Alpha

DB2 rasters only support Byte data type.

All raster extensions standardized by the GeoPackage specification are
supported in read and creation :

-  *gpkg.webp*: when storing WebP tiles, provided that GDAL is compiled
   against libwebp.
-  *gpkg.zoom_other*: when resolution of consecutive zoom levels does
   not vary with a factor of 2.

Driver capabilities
-------------------

.. supports_createcopy::

.. supports_create::

.. supports_georeferencing::

Opening options
---------------

By default, the driver will expose a DB2 dataset as a four band
(Red,Green, Blue,Alpha) dataset, which gives the maximum compatibility
with the various encodings of tiles that can be stored. It is possible
to specify an explicit number of bands with the BAND_COUNT opening
option.

The driver will use the geographic/projected extent indicated in the
`gpkg.contents <http://www.geopackage.org/spec/#_contents>`__ table, and
do necessary clipping, if needed, to respect that extent. However that
information being optional, if omitted, the driver will use the extent
provided by the
`gpkg.tile_matrix_set <http://www.geopackage.org/spec/#_tile_matrix_set>`__,
which covers the extent at all zoom levels. The user can also specify
the USE_TILE_EXTENT=YES open option to use the actual extent of tiles at
the maximum zoom level. Or it can specify any of MINX/MINY/MAXX/MAXY to
have a custom extent.

The following open options are available:

-  **TABLE**\ =table_name: Name of the table containing the tiles
   (called `"Tile Pyramid User Data
   Table" <http://www.geopackage.org/spec/#tiles_user_tables>`__ in the
   GeoPackage specification language). If the DB2 dataset only contains
   one table, this option is not necessary. Otherwise, it is required.
-  **ZOOM_LEVEL**\ =value: Integer value between 0 and the maximum
   filled in the *gpkg.tile_matrix* table. By default, the driver will
   select the maximum zoom level, such as at least one tile at that zoom
   level is found in the raster table.
-  **BAND_COUNT**\ =1/2/3/4: Number of bands of the dataset exposed
   after opening. Some conversions will be done when possible and
   implemented, but this might fail in some cases, depending on the
   BAND_COUNT value and the number of bands of the tile. Defaults to 4
   (which is the always safe value).
-  **MINX**\ =value: Minimum longitude/easting of the area of interest.
-  **MINY**\ =value: Minimum latitude/northing of the area of interest.
-  **MAXX**\ =value: Maximum longitude/easting of the area of interest.
-  **MAXY**\ =value: Maximum latitude/northing of the area of interest.
-  **USE_TILE_EXTENT**\ =YES/NO: Whether to use the extent of actual
   existing tiles at the zoom level of the full resolution dataset.
   Defaults to NO.
-  **TILE_FORMAT**\ =PNG_JPEG/PNG/PNG8/JPEG/WEBP: Format used to store
   tiles. See `Tile format <#tile_format>`__ section. Only used in
   update mode. Defaults to PNG_JPEG.
-  **QUALITY**\ =1-100: Quality setting for JPEG and WEBP compression.
   Only used in update mode. Default to 75.
-  **ZLEVEL**\ =1-9: DEFLATE compression level for PNG tiles. Only used
   in update mode. Default to 6.
-  **DITHER**\ =YES/NO: Whether to use Floyd-Steinberg dithering (for
   TILE_FORMAT=PNG8). Only used in update mode. Defaults to NO.

Note: open options are typically specified with "-oo name=value" syntax
in most GDAL utilities, or with the GDALOpenEx() API call.

Creation issues
---------------

Depending of the number of bands of the input dataset and the tile
format selected, the driver will do the necessary conversions to be
compatible with the tile format.

To add several tile tables to a DB2 dataset (seen as GDAL subdatasets),
or to add a tile table to an existing vector-only DB2, the generic
APPEND_SUBDATASET=YES creation option must be provided.

Fully transparent tiles will not be written to the database, as allowed
by the format.

The driver implements the Create() and IWriteBlock() methods, so that
arbitrary writing of raster blocks is possible, enabling the direct use
of DB2 as the output dataset of utilities such as gdalwarp.

On creation, raster blocks can be written only if the geotransformation
matrix has been set with SetGeoTransform() This is effectively needed to
determine the zoom level of the full resolution dataset based on the
pixel resolution, dataset and tile dimensions.

Technical/implementation note: when a dataset is opened with a
non-default area of interest (i.e. use of MINX,MINY,MAXX,MAXY or
USE_TILE_EXTENT open option), or when creating/ opening a dataset with a
non-custom tiling scheme, it is possible that GDAL blocks do not exactly
match a single DB2 tile. In which case, each GDAL block will overlap
four DB2 tiles. This is easily handled on the read side, but on
creation/update side, such configuration could cause numerous
decompression/ recompression of tiles to be done, which might cause
unnecessary quality loss when using lossy compression (JPEG, WebP). To
avoid that, the driver will create a temporary database next to the main
DB2 table to store partial DB2 tiles in a lossless (and uncompressed)
way. Once a tile has received data for its four quadrants and for all
the bands (or the dataset is closed or explicitly flushed with
FlushCache()), those uncompressed tiles are definitely transferred to
the DB2 table with the appropriate compression. All of this is
transparent to the user of GDAL API/utilities

Tile formats
~~~~~~~~~~~~

DB2 can store tiles in different formats, PNG and/or JPEG for the
baseline specification, and WebP for extended DB2. Support for those
tile formats depend if the underlying drivers are available in GDAL,
which is generally the case for PNG and JPEG, but not necessarily for
WebP since it requires GDAL to be compiled against the optional libwebp.

By default, GDAL will use a mix of PNG and JPEG tiles. PNG tiles will be
used to store tiles that are not completely opaque, either because input
dataset has an alpha channel with non fully opaque content, or because
tiles are partial due to clipping at the right or bottom edges of the
raster, or when a dataset is opened with a non-default area of interest,
or with a non-custom tiling scheme. On the contrary, for fully opaque
tiles, JPEG format will be used.

It is possible to select one unique tile format by setting the
creation/open option TILE_FORMAT to one of PNG, JPEG or WEBP. When using
JPEG, the alpha channel will not be stored. When using WebP, the
`gpkg.webp <http://www.geopackage.org/spec/#extension_tiles_webp>`__
extension will be registered. The lossy compression of WebP is used.
Note that a recent enough libwebp (>=0.1.4) must be used to support
alpha channel in WebP tiles.

PNG8 can be selected to use 8-bit PNG with a color table up to 256
colors. On creation, an optimized color table is computed for each tile.
The DITHER option can be set to YES to use Floyd/Steinberg dithering
algorithm, which spreads the quantization error on neighbouring pixels
for better rendering (note however than when zooming in, this can cause
non desirable visual artifacts). Setting it to YES will generally cause
less effective compression. Note that at that time, such an 8-bit PNG
formulation is only used for fully opaque tiles, as the median-cut
algorithm currently implemented to compute the optimal color table does
not support alpha channel (even if PNG8 format would potentially allow
color table with transparency). So when selecting PNG8, non fully opaque
tiles will be stored as 32-bit PNG.

Tiling schemes
~~~~~~~~~~~~~~

By default, conversion to DB2 will create a custom tiling scheme, such
that the input dataset can be losslessly converted, both at the pixel
and georeferencing level (if using a lossless tile format such as PNG).
That tiling scheme is such that its origin (*min_x*, *max_y*) in the
`gpkg.tile_matrix_set <http://www.geopackage.org/spec/#_tile_matrix_set>`__
table perfectly matches the top left corner of the dataset, and the
selected resolution (*pixel_x_size*, *pixel_y_size*) at the computed
maximum zoom_level of the
`gpkg.tile_matrix <http://www.geopackage.org/spec/#_tile_matrix>`__
table will match the pixel width and height of the raster.

However to ease interoperability with other implementations, and enable
use of DB2 with tile servicing software, it is possible to select a
predefined tiling scheme that has world coverage. The available tiling
schemes are :

-  *GoogleCRS84Quad*, as described in `OGC 07-057r7 WMTS
   1.0 <http://portal.opengeospatial.org/files/?artifact_id=35326>`__
   specification, Annex E.3. That tiling schemes consists of a single
   256x256 tile at its zoom level 0, in EPSG:4326 CRS, with extent in
   longitude and latitude in the range [-180,180]. Consequently, at zoom
   level 0, 64 lines are unused at the top and bottom of that tile. This
   may cause issues with some implementations of the specification, and
   there are some ambiguities about the exact definition of this tiling
   scheme. Using InspireCRS84Quad/PseudoTMS_GlobalGeodetic instead is
   therefore recommended.
-  *GoogleMapsCompatible*, as described in WMTS 1.0 specification, Annex
   E.4. That tiling schemes consists of a single 256x256 tile at its
   zoom level 0, in EPSG:3857 CRS, with extent in easting and northing
   in the range [-20037508.34,20037508.34].
-  *InspireCRS84Quad*, as described in `Inspire View
   Services <http://inspire.ec.europa.eu/documents/Network_Services/TechnicalGuidance_ViewServices_v3.0.pdf>`__.
   That tiling schemes consists of two 256x256 tiles at its zoom level
   0, in EPSG:4326 CRS, with extent in longitude in the range [-180,180]
   and in latitude in the range [-90,90].
-  *PseudoTMS_GlobalGeodetic*, based on the
   `global-geodetic <http://wiki.osgeo.org/wiki/Tile_Map_Service_Specification#global-geodetic>`__
   profile of OSGeo TMS (Tile Map Service) specification. This has
   exactly the same definition as *InspireCRS84Quad* tiling scheme. Note
   however that full interoperability with TMS is not possible due to
   the origin of numbering of tiles being the top left corner in DB2
   (consistently with WMTS convention), whereas TMS uses the bottom left
   corner as origin.
-  *PseudoTMS_GlobalMercator*, based on the
   `global-mercator <http://wiki.osgeo.org/wiki/Tile_Map_Service_Specification#global-mercator>`__
   profile of OSGeo TMS (Tile Map Service) specification. That tiling
   schemes consists of four 256x256 tiles at its zoom level 0, in
   EPSG:3857 CRS, with extent extent in easting and northing in the
   range [-20037508.34,20037508.34]. The same remark as with
   PseudoTMS_GlobalGeodetic applies regarding interoperability with TMS.

In all the above tiling schemes, consecutive zoom levels defer by a
resolution of a factor of two.

Creation options
~~~~~~~~~~~~~~~~

The following creation options are available:

-  **RASTER_TABLE**\ =string. Name of tile user table. By default, based
   on the source filename.
-  **APPEND_SUBDATASET**\ =YES/NO: If set to YES, an existing DB2 table
   will not be priorly destroyed, such as to be able to add new content
   to it. Defaults to NO.
-  **RASTER_IDENTIFIER**\ =string. Human-readable identifier (e.g. short
   name), put in the *identifier* column of the *gpkg.contents* table.
-  **RASTER_DESCRIPTION**\ =string. Human-readable description, put in
   the *description* column of the *gpkg.contents* table.
-  **BLOCKSIZE**\ =integer. Block size in width and height in pixels.
   Defaults to 256. Maximum supported is 4096. Should not be set when
   using a non-custom TILING_SCHEME.
-  **BLOCKXSIZE**\ =integer. Block width in pixels. Defaults to 256.
   Maximum supported is 4096.
-  **BLOCKYSIZE**\ =integer. Block height in pixels. Defaults to 256.
   Maximum supported is 4096.
-  **TILE_FORMAT**\ =PNG_JPEG/PNG/PNG8/JPEG/WEBP: Format used to store
   tiles. See `Tile formats <#tile_formats>`__ section. Defaults to
   PNG_JPEG.
-  **QUALITY**\ =1-100: Quality setting for JPEG and WEBP compression.
   Default to 75.
-  **ZLEVEL**\ =1-9: DEFLATE compression level for PNG tiles. Default to
   6.
-  **DITHER**\ =YES/NO: Whether to use Floyd-Steinberg dithering (for
   TILE_FORMAT=PNG8). Defaults to NO.
-  **TILING_SCHEME**\ =CUSTOM/GoogleCRS84Quad/GoogleMapsCompatible/InspireCRS84Quad/PseudoTMS_GlobalGeodetic/PseudoTMS_GlobalMercator.
   See `Tiling schemes <#tiling_schemes>`__ section. Defaults to CUSTOM.
-  **ZOOM_LEVEL_STRATEGY**\ =AUTO/LOWER/UPPER. Strategy to determine
   zoom level. Only used for TILING_SCHEME is different from CUSTOM.
   LOWER will select the zoom level immediately below the theoretical
   computed non-integral zoom level, leading to subsampling. On the
   contrary, UPPER will select the immediately above zoom level, leading
   to oversampling. Defaults to AUTO which selects the closest zoom
   level.
-  **RESAMPLING**\ =NEAREST/BILINEAR/CUBIC/CUBICSPLINE/LANCZOS/MODE/AVERAGE.
   Resampling algorithm. Only used for TILING_SCHEME is different from
   CUSTOM. Defaults to BILINEAR.

Overviews
---------

gdaladdo / BuildOverviews() can be used to compute overviews.
Power-of-two overview factors (2,4,8,16,...) should be favored to be
conformant with the baseline GeoPackage specification. Use of other
overview factors will work with the GDAL driver, and cause the
`gpkg.zoom_other <http://www.geopackage.org/spec/#extension_zoom_other_intervals>`__
extension to be registered, but that could potentially cause
interoperability problems with other implementations that do not support
that extension.

Overviews can also be cleared with the -clean option of gdaladdo (or
BuildOverviews() with nOverviews=0)

Metadata
--------

GDAL uses the standardized
```gpkg.metadata`` <http://www.geopackage.org/spec/#_metadata_table>`__
and
```gpkg.metadata_reference`` <http://www.geopackage.org/spec/#_metadata_reference_table>`__
tables to read and write metadata.

GDAL metadata, from the default metadata domain and possibly other
metadata domains, is serialized in a single XML document, conformant
with the format used in GDAL PAM (Persistent Auxiliary Metadata)
.aux.xml files, and registered with md_scope=dataset and
md_standard_uri=http://gdal.org in gpkg.metadata. In
gpkg.metadata_reference, this entry is referenced with a
reference_scope=table and table_name={name of the raster table}

It is possible to read and write metadata that applies to the global
DB2, and not only to the raster table, by using the *GEOPACKAGE*
metadata domain.

Metadata not originating from GDAL can be read by the driver and will be
exposed as metadata items with keys of the form gpkg.METADATA_ITEM_XXX
and values the content of the *metadata* columns of the gpkg.metadata
table. Update of such metadata is not currently supported through GDAL
interfaces ( although it can be through direct SQL commands).

The specific DESCRIPTION and IDENTIFIER metadata item of the default
metadata domain can be used in read/write to read from/update the
corresponding columns of the gpkg.contents table.

Examples
--------

-  Simple translation of a GeoTIFF into DB2. The table 'byte' will be
   created with the tiles.

   ::

      % gdal_translate -of DB2ODBC byte.tif DB2ODBC:database=sample;DSN=SAMPLE

-  Translation of a GeoTIFF into DB2 using WebP tiles

   ::

      % gdal_translate -of DB2ODBC byte.tif DB2ODBC:database=sample;DSN=SAMPLE -co TILE_FORMAT=WEBP

-  Translation of a GeoTIFF into DB2 using GoogleMapsCompatible tiling
   scheme (with reprojection and resampling if needed)

   ::

      % gdal_translate -of DB2ODBC byte.tif DB2ODBC:database=sample;DSN=SAMPLE -co TILING_SCHEME=GoogleMapsCompatible

-  Building of overviews of an existing DB2

   ::

      % gdaladdo -oo RASTER_TABLE=world -r cubic DB2ODBC:database=sample;DSN=SAMPLE 2 4 8 16 32 64

-  Addition of a new subdataset to an existing DB2, and choose a non
   default name for the raster table.

   ::

      % gdal_translate -of DB2ODBC new.tif DB2ODBC:database=sample;DSN=SAMPLE -co APPEND_SUBDATASET=YES -co RASTER_TABLE=new_table

-  Reprojection of an input dataset to DB2

   ::

      % gdalwarp -of DB2ODBC -co RASTER_TABLE=new_table in.tif DB2ODBC:database=sample;DSN=SAMPLE -t_srs EPSG:3857

-  Open a specific raster table in a DB2

   ::

      % gdalinfo DB2ODBC:database=sample;DSN=SAMPLE -oo TABLE=a_table

See Also
--------

-  :ref:`DB2 vector <vector.db2>` documentation page
-  :ref:`PNG driver <raster.png>` documentation page
-  :ref:`JPEG driver <raster.jpeg>` documentation page
-  :ref:`WEBP driver <raster.webp>` documentation page
-  `OGC 07-057r7 WMTS
   1.0 <http://portal.opengeospatial.org/files/?artifact_id=35326>`__
   specification
-  `OSGeo TMS (Tile Map
   Service) <http://wiki.osgeo.org/wiki/Tile_Map_Service_Specification>`__
   specification
