Short name | Long name | Creation | Copy | Geo-referencing | Build requirements
--- | --- | --- | --- | --- | ---
AAIGrid | Arc/Info ASCII Grid | No | Yes | Yes | Built-in by default
ACE2 | ACE2 | No | No | Yes | Built-in by default
ADRG | ADRG/ARC Digitized Raster Graphics (.gen/.thf) | Yes | Yes | Yes | Built-in by default
AIG | Arc/Info Binary Grid | No | No | Yes | Built-in by default
AIRSAR | AIRSAR Polarimetric Format | No | No | No | Built-in by default
ARG | Azavea Raster Grid | Yes | Yes | Yes | Built-in by default
BAG | Bathymetry Attributed Grid | Yes | Yes | Yes | libhdf5
BLX | Magellan BLX Topo File Format | No | Yes | Yes | Built-in by default
BMP | Microsoft Windows Device Independent Bitmap | Yes | Yes | Yes | Built-in by default
BPG | Better Portable Graphics | No | No | No | libbpg (manual build required for now)
BSB | Maptech/NOAA BSB Nautical Chart Format | No | No | Yes | Built-in by default
BT | VTP .bt Binary Terrain Format | Yes | Yes | Yes | Built-in by default
BYN | Natural Resources Canada’s Geoid file format (.byn) | Yes | Yes | Yes | Built-in by default
CAD | AutoCAD DWG raster layer | No | No | Yes | (internal libopencad provided)
CALS | CALS Type 1 | No | Yes | No | Built-in by default
CEOS | CEOS Image | No | Yes | No | Built-in by default
COASP | DRDC COASP SAR Processor Raster | No | No | No | Built-in by default
COG | Cloud Optimized GeoTIFF generator | No | Yes | Yes | Built-in by default
COSAR | TerraSAR-X Complex SAR Data Product | No | No | No | Built-in by default
CPG | Convair PolGASP data | No | No | Yes | Built-in by default
CTable2 | CTable2 Datum Grid Shift | Yes | Yes | Yes | Built-in by default
CTG | USGS LULC Composite Theme Grid | No | No | Yes | Built-in by default
DAAS | DAAS (Airbus DS Intelligence Data As A Service driver) | No | No | Yes | libcurl
DB2 | DB2 raster | Yes | Yes | Yes | ODBC (and any or all of PNG, JPEG, WEBP drivers)
DDS | DirectDraw Surface | No | Yes | No | Crunch Lib
DERIVED | Derived subdatasets driver | No | No | No | Built-in by default
DIMAP | Spot DIMAP | No | No | Yes | Built-in by default
DIPEx | ELAS DIPEx | No | No | Yes | Built-in by default
DODS | OPeNDAP Grid Client | No | No | Yes | libdap
DOQ1 | First Generation USGS DOQ | No | No | Yes | Built-in by default
DOQ2 | New Labelled USGS DOQ | No | No | Yes | Built-in by default
DTED | Military Elevation Data | No | Yes | Yes | Built-in by default
E00GRID | Arc/Info Export E00 GRID | No | No | Yes | Built-in by default
ECRGTOC | ECRG Table Of Contents (TOC.xml) | No | No | Yes | Built-in by default
ECW | Enhanced Compressed Wavelets (.ecw) | Yes | Yes | Yes | ECW SDK
EEDAI | Google Earth Engine Data API Image | No | No | Yes | libcurl
EHdr | ESRI .hdr Labelled | Yes | Yes | Yes | Built-in by default
EIR | Erdas Imagine Raw | No | No | Yes | Built-in by default
ELAS | Earth Resources Laboratory Applications Software | Yes | Yes | Yes | Built-in by default
ENVI | ENVI .hdr Labelled Raster | Yes | Yes | Yes | Built-in by default
EPSILON | Wavelet compressed images | No | Yes | No | epsilon 0.9.1
ERS | ERMapper .ERS | Yes | Yes | Yes | Built-in by default
ESAT | Envisat Image Product | No | No | No | Built-in by default
ESRIC | Esri Compact Cache | No | No | Yes | Built-in by default
EXR | Extended Dynamic Range Image File Format | Yes | Yes | Yes | libopenexr
FAST | EOSAT FAST Format | No | No | Yes | Built-in by default
FIT | FIT | No | Yes | Yes | Built-in by default
FITS | Flexible Image Transport System | Yes | Yes | Yes | libcfitsio
FujiBAS | Fuji BAS Scanner Image | No | No | No | Built-in by default
GenBin | Generic Binary (.hdr labelled) | No | No | No | Built-in by default
GeoRaster | Oracle Spatial GeoRaster | Yes | Yes | Yes | Oracle client libraries
GFF | Sandia National Laboratories GSAT File Format | No | No | No | Built-in by default
GIF | Graphics Interchange Format | No | Yes | No | (internal GIF library provided)
GMT | GMT Compatible netCDF | No | Yes | Yes | libnetcdf
GPKG | GeoPackage raster | Yes | Yes | Yes | libsqlite3 (and any or all of PNG, JPEG, WEBP drivers)
GRASS | GRASS Raster Format | No | No | Yes | libgrass
GRASSASCIIGrid | GRASS ASCII Grid | No | No | Yes | Built-in by default
GRIB | WMO General Regularly-distributed Information in Binary form | No | No | Yes | Built-in by default
GS7BG | Golden Software Surfer 7 Binary Grid File Format | Yes | Yes | Yes | Built-in by default
GSAG | Golden Software ASCII Grid File Format | No | No | Yes | Built-in by default
GSBG | Golden Software Binary Grid File Format | Yes | Yes | Yes | Built-in by default
GSC | GSC Geogrid | No | No | No | Built-in by default
GTA | Generic Tagged Arrays | No | Yes | Yes | libgta
GTiff | GeoTIFF File Format | Yes | Yes | Yes | Built-in by default
GXF | Grid eXchange File | No | No | Yes | Built-in by default
HDF4 | Hierarchical Data Format Release 4 (HDF4) | Yes | Yes | Yes | libdf
HDF5 | Hierarchical Data Format Release 5 (HDF5) | No | No | Yes | libhdf5
HEIF | ISO/IEC 23008-12:2017 High Efficiency Image File Format | No | No | No | libheif (>= 1.1), built against libde265
HF2 | HF2/HFZ heightfield raster | No | Yes | Yes | Built-in by default
HFA | Erdas Imagine .img | Yes | Yes | Yes | Built-in by default
IDA | Image Display and Analysis | Yes | Yes | Yes | Built-in by default
RST | Idrisi Raster Format | Yes | Yes | Yes | Built-in by default
IGNFHeightASCIIGrid | IGN-France height correction ASCII grids | No | No | Yes | Built-in by default
ILWIS | Raster Map | Yes | Yes | Yes | Built-in by default
INGR | Intergraph Raster Format | Yes | Yes | Yes | Built-in by default
IRIS | Vaisala’s weather radar software format | No | No | Yes | Built-in by default
ISCE | ISCE | Yes | Yes | Yes | Built-in by default
ISG | International Service for the Geoid | No | No | Yes | Built-in by default
ISIS2 | USGS Astrogeology ISIS Cube (Version 2) | Yes | Yes | Yes | Built-in by default
ISIS3 | USGS Astrogeology ISIS Cube (Version 3) | Yes | Yes | Yes | Built-in by default
JDEM | Japanese DEM (.mem) | No | No | Yes | Built-in by default
JP2ECW | ERDAS JPEG2000 (.jp2) | Yes | Yes | Yes | ECW SDK
JP2KAK | JPEG-2000 (based on Kakadu) | No | Yes | Yes | Kakadu library
JP2LURA | JPEG2000 driver based on Lurawave library | No | Yes | Yes | Lurawave library
JP2MrSID | JPEG2000 via MrSID SDK | No | Yes | Yes | MrSID SDK
JP2OpenJPEG | JPEG2000 driver based on OpenJPEG library | No | Yes | Yes | openjpeg >= 2.1
JPEG | JPEG JFIF File Format | No | Yes | Yes | (internal libjpeg provided)
JPEG2000 | Implementation of the JPEG-2000 part 1 | No | Yes | Yes | libjasper
JPEGLS | JPEGLS | No | Yes | No | CharLS library
JPIPKAK | JPIP Streaming | No | No | Yes | Kakadu library
KEA | KEA | Yes | Yes | Yes | libkea and libhdf5 libraries
KMLSuperoverlay | KMLSuperoverlay | No | Yes | Yes | Built-in by default
KRO | KOLOR Raw format | Yes | Yes | No | Built-in by default
L1B | NOAA Polar Orbiter Level 1b Data Set (AVHRR) | No | No | Yes | Built-in by default
LAN | Erdas 7.x .LAN and .GIS | No | No | Yes | Built-in by default
LCP | FARSITE v.4 LCP Format | No | Yes | Yes | Built-in by default
Leveller | Daylon Leveller Heightfield | Yes | Yes | Yes | Built-in by default
LOSLAS | NADCON .los/.las Datum Grid Shift | No | No | Yes | Built-in by default
MAP | OziExplorer .MAP | No | No | Yes | Built-in by default
MRF | Meta Raster Format | Yes | Yes | Yes | Built-in by default
MBTiles | MBTiles | Yes | Yes | Yes | libsqlite3
MEM | In Memory Raster | Yes | Yes | Yes | Built-in by default
MFF | Vexcel MFF Raster | Yes | Yes | Yes | Built-in by default
MFF2 | Vexcel MFF2 Image | Yes | Yes | Yes | Built-in by default
MG4Lidar | MrSID/MG4 LiDAR Compression / Point Cloud View files | No | No | No | LIDAR SDK
MrSID | Multi-resolution Seamless Image Database | No | No | Yes | MrSID SDK
MSG | Meteosat Second Generation | No | No | Yes | msg library
MSGN | Meteosat Second Generation (MSG) Native Archive Format (.nat) | No | No | Yes | Built-in by default
NDF | NLAPS Data Format | No | No | Yes | Built-in by default
netCDF | NetCDF: Network Common Data Form | Yes | Yes | Yes | libnetcdf
NGSGEOID | NOAA NGS Geoid Height Grids | No | No | Yes | Built-in by default
NGW | NextGIS Web | No | No | Yes | libcurl
NITF | National Imagery Transmission Format | Yes | Yes | Yes | Built-in by default
NTv1 | NTv1 Datum Grid Shift | No | No | Yes | Built-in by default
NTv2 | NTv2 Datum Grid Shift | Yes | Yes | Yes | Built-in by default
NWT_GRD | Northwood/Vertical Mapper File Format | Yes | Yes | Yes | Built-in by default
NWT_GRC | Northwood/Vertical Mapper File Format | Yes | Yes | Yes | Built-in by default
OGCAPI | OGC API Tiles / Maps | No | No | Yes | libcurl
OZI | OZF2/OZFX3 raster | No | No | Yes | Built-in by default
JAXAPALSAR | JAXA PALSAR Processed Products | No | No | Yes | Built-in by default
PAux | PCI .aux Labelled Raw Format | Yes | Yes | No | Built-in by default
PCIDSK | PCI Geomatics Database File | Yes | Yes | Yes | Built-in by default
PCRaster | PCRaster raster file format | Yes | Yes | Yes | (internal libcf provided)
PDF | Geospatial PDF | No | Yes | Yes | none for write support, Poppler/PoDoFo/PDFium for read support
PDS | Planetary Data System v3 | No | No | Yes | Built-in by default
PDS4 | NASA Planetary Data System (Version 4) | Yes | Yes | Yes | Built-in by default
PLMosaic | PLMosaic (Planet Labs Mosaics API) | No | No | Yes | libcurl
PNG | Portable Network Graphics | No | Yes | Yes | Built-in by default
PNM | Netpbm (.pgm, .ppm) | No | Yes | No | Built-in by default
PostGISRaster | PostGIS Raster driver | No | Yes | Yes | PostgreSQL library
PRF | PHOTOMOD Raster File | No | No | No | Built-in by default
R | R Object Data Store | No | Yes | No | Built-in by default
Rasdaman | Rasdaman GDAL driver | No | No | No | raslib
Rasterlite | Rasters in SQLite DB | No | Yes | Yes | libsqlite3
SQLite | Rasters in SQLite DB | No | Yes | Yes | libsqlite3, librasterlite2, libspatialite
RDA | RDA (DigitalGlobe Raster Data Access) | No | No | Yes | libcurl
RDB | RIEGL Database | No | No | Yes | rdblib >= 2.2.0.
RIK | Swedish Grid Maps | No | No | Yes | (internal zlib is used if necessary)
RMF | Raster Matrix Format | Yes | Yes | Yes | Built-in by default
ROI_PAC | ROI_PAC | Yes | Yes | Yes | Built-in by default
RPFTOC | Raster Product Format/RPF (a.toc) | No | No | Yes | Built-in by default
RRASTER | R Raster | Yes | Yes | Yes | Built-in by default
RS2 | RadarSat 2 XML Product | No | No | Yes | Built-in by default
SAFE | Sentinel-1 SAFE XML Product | No | No | Yes | Built-in by default
SAR_CEOS | CEOS SAR Image | No | No | Yes | Built-in by default
SAGA | SAGA GIS Binary Grid File Format | Yes | Yes | Yes | Built-in by default
SDTS | USGS SDTS DEM | No | No | Yes | Built-in by default
SENTINEL2 | Sentinel-2 Products | No | No | Yes | Built-in by default
SGI | SGI Image Format | Yes | Yes | No | Built-in by default
SIGDEM | Scaled Integer Gridded DEM | No | Yes | Yes | Built-in by default
SNODAS | Snow Data Assimilation System | No | No | Yes | Built-in by default
SRP | Standard Product Format (ASRP/USRP) (.gen) | No | No | Yes | Built-in by default
SRTMHGT | SRTM HGT Format | No | No | Yes | Built-in by default
Terragen | Terragen™ Terrain File | Yes | Yes | Yes | Built-in by default
TGA | TARGA Image File Format | No | No | No | Built-in by default
TIL | EarthWatch/DigitalGlobe .TIL | No | No | Yes | Built-in by default
TileDB | TileDB | Yes | Yes | Yes | TileDB
TSX | TerraSAR-X Product | No | No | Yes | Built-in by default
USGSDEM | USGS ASCII DEM (and CDED) | Yes | No | Yes | Built-in by default
VICAR | VICAR | Yes | Yes | Yes | Built-in by default
VRT | GDAL Virtual Format | Yes | Yes | Yes | Built-in by default
WCS | OGC Web Coverage Service | No | No | Yes | libcurl
WEBP | WEBP | No | Yes | No | libwebp
WMS | Web Map Services | No | Yes | Yes | libcurl
WMTS | OGC Web Map Tile Service | No | No | Yes | libcurl
XPM | X11 Pixmap | No | Yes | No | Built-in by default
XYZ | ASCII Gridded XYZ | No | Yes | Yes | Built-in by default
ZMAP | ZMap Plus Grid | No | Yes | Yes | Built-in by default