# LOSLAS – NADCON .los/.las Datum Grid Shift

Driver short name

LOSLAS

Driver built-in by default

This driver is built-in by default

Starting with GDAL 3.1, can also open geoid models of extension .geo such as https://geodesy.noaa.gov/GEOID/MEXICO97/

NOTE: Implemented as `gdal/frmts/raw/loaslasdataset.cpp`.

## Driver capabilities

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)