# VICAR – VICAR

Driver short name

VICAR

Driver built-in by default

This driver is built-in by default

Note

PDS3 datasets can incorporate a VICAR header. By default, GDAL will use the PDS driver in that situation. Starting with GDAL 3.1, if the `GDAL_TRY_PDS3_WITH_VICAR` configuration option is set to YES, the dataset will be opened by the VICAR driver.

## Driver capabilities

Supports CreateCopy()

This driver supports the `GDALDriver::CreateCopy()` operation

Supports Create()

This driver supports the `GDALDriver::Create()` operation

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)

## Metadata

Starting with GDAL 3.1, the VICAR label can be retrieved as JSon-serialized content in the json:VICAR metadata domain.

For example:

    $ python
    from osgeo import gdal
    ds = gdal.Open('../autotest/gdrivers/data/test_vicar_truncated.bin')
    print(ds.GetMetadata_List('json:VICAR')[0])
    {
     "LBLSIZE":9680,
     "FORMAT":"BYTE",
     "TYPE":"IMAGE",
     "BUFSIZ":2097152,
     "DIM":3,
     "EOL":0,
     "RECSIZE":4840,
     "ORG":"BSQ",
     "NL":1000,
     "NS":400,
     "NB":1,
     "N1":4000,
     "N2":1000,
     "N3":1,
     "N4":0,
     "NBB":0,
     "NLB":0,
     "HOST":"X86-64-LINX",
     "INTFMT":"LOW",
     "REALFMT":"RIEEE",
     "BHOST":"X86-LINUX",
     "BINTFMT":"LOW",
     "BREALFMT":"RIEEE",
     "BLTYPE":"M94_HRSC",
     "COMPRESS":"NONE",
     "EOCI1":0,
     "EOCI2":0,
     "PROPERTY":{
         "M94_ORBIT":{
             "ORBIT_NUMBER":5273,
             "ASCENDING_NODE_LONGITUDE":118.46,
             "ORBITAL_ECCENTRICITY":1.23,
             "ORBITAL_INCLINATION":4.56,
             "PERIAPSIS_ARGUMENT_ANGLE":7.89,
             "PERIAPSIS_TIME":"PERIAPSIS_TIME",
             "PERIAPSIS_ALTITUDE":333.16,
             "ORBITAL_SEMIMAJOR_AXIS":1.23,
             "SPACECRAFT_SOLAR_DISTANCE":4.56,
             "SPACECRAFT_CLOCK_START_COUNT":"1\/1",
             "SPACECRAFT_CLOCK_STOP_COUNT":"1\/2",
             "START_TIME":"start_time",
             "STOP_TIME":"stop_time",
             "SPACECRAFT_POINTING_MODE":"NADIR",
             "RIGHT_ASCENSION":-1.0000000000000001e+32,
             "DECLINATION":-1.0000000000000001e+32,
             "OFFSET_ANGLE":-1.0000000000000001e+32,
             "SPACECRAFT_ORIENTATION":[
                 0.000000,
                 -1.000000,
                 0.000000
             ]
         },
         [...]
         "PHOT":{
             "PHO_FUNC":"NONE"
         }
     },
     "TASK":{
         "HRCONVER":{
             "USER":"mexsyst",
             "DAT_TIM":"DAT_TIM",
             "SPICE_FILE_NAME":[
                 "foo"
             ],
             "SPICE_FILE_ID":"(LSK,SCLK,ON)",
             "DETECTOR_TEMPERATURE":1.23,
             "DETECTOR_TEMPERATURE__UNIT":"degC",
             "FOCAL_PLANE_TEMPERATURE":8.5833,
             "FOCAL_PLANE_TEMPERATURE__UNIT":"degC",
             "INSTRUMENT_TEMPERATURE":2.34,
             "INSTRUMENT_TEMPERATURE__UNIT":"degC",
             "LENS_TEMPERATURE":4.56,
             "LENS_TEMPERATURE__UNIT":"degC",
             "SOURCE_FILE_NAME":"SOURCE_FILE_NAME",
             "MISSING_FRAMES":0,
             "OVERFLOW_FRAMES":0,
             "ERROR_FRAMES":1
         }
       }
     }

or

    $ gdalinfo -json ../autotest/gdrivers/data/test_vicar_truncated.bin -mdd all

## Binary prefixes

Starting with GDAL 3.1, if the VICAR label declares a non-zero binary prefix length (NBB label item), then GDAL will look in the vicar.json configuration file if there is an entry corresponding to the BLTYPE label item (currently only M94_HRSC is defined), and if there is a match, a OGR vector layer will be available on the dataset, with a feature for each image record.

For example:

    $ ogrinfo h0038_0000.bl2.16 -al -q

    Layer name: binary_prefixes
    OGRFeature(binary_prefixes):0
        EphTime (Real) = 127988268.646895
        Exposure (Real) = 40.1072692871094
        COT (Integer) = 28275
        FEETemp (Integer) = 28508
        FPMTemp (Integer) = 29192
        OBTemp (Integer) = 28295
        FERT (Integer) = 27001
        LERT (Integer) = 28435
        CmpDataLen (Integer) = 146
        FrameCount (Integer) = 486
        Pischel (Integer) = 5
        ActPixel (Integer) = 5120
        RSHits (Integer) = 0
        DceInput (Integer) = 0
        DceOutput (Integer) = 4
        FrameErr1 (Integer) = 0
        FrameErr2 (Integer) = 0
        Gob1 (Integer) = 0
        Gob2 (Integer) = 0
        Gob3 (Integer) = 0
        DSS (Integer) = 97
        DecmpErr1 (Integer) = 0
        DecmpErr2 (Integer) = 0
        DecmpErr3 (Integer) = 0
        FillerFlag (Integer) = 5

## Creation support

Starting with GDAL 3.1, the VICAR driver supports updating imagery of existing datasets, creating new datasets through the CreateCopy() and Create() interfaces.

When using CreateCopy(), gdal_translate or gdalwarp, an effort is made to preserve as much as possible of the original label when doing VICAR to VICAR conversions. This can be disabled with the USE_SRC_LABEL=NO creation option.

The available creation options are:

- GEOREF_FORMAT=MIPL/GEOTIFF. (GDAL >= 3.4) How to encode georeferencing information. Defaults to MIPL using the `MAP` property group. When setting to GEOTIFF, a `GEOTIFF` property group will be used using GeoTIFF keys and tags. The COORDINATE_SYSTEM_NAME, POSITIVE_LONGITUDE_DIRECTION and TARGET_NAME options will be ignored when selecting the GEOTIFF encoding.

- COORDINATE_SYSTEM_NAME=PLANETOCENTRIC/PLANETOGRAPHIC. Value of MAP.COORDINATE_SYSTEM_NAME. Defaults to PLANETOCENTRIC. If specified, and USE_SRC_MAP is in effect, this will be taken into account to override the source COORDINATE_SYSTEM_NAME.

- POSITIVE_LONGITUDE_DIRECTION=EAST/WEST. Value of MAP.override. Defaults to EAST. If specified, and USE_SRC_MAP is in effect, this will be taken into account to override the source POSITIVE_LONGITUDE_DIRECTION.

- TARGET_NAME=string. Value of MAP.TARGET_NAME. This is normally deduced from the SRS datum name. If specified, and USE_SRC_MAP is in effect, this will be taken into account to override the source TARGET_NAME.

- USE_SRC_LABEL=YES/NO. Whether to use source label in VICAR to VICAR conversions. Defaults to YES.

- LABEL=string. Label to use, either as a JSON string or a filename containing one. If defined, takes precedence over USE_SRC_LABEL.

- COMPRESS= NONE/BASIC/BASIC2. Compression method. Default to NONE. For maximum interoperability, do not use BASIC or BASIC2 which are not well specified and not always available in VICAR capable applications.

## See Also

- Implemented as `gdal/frmts/pds/vicardataset.cpp`.

- VICAR documentation

- VICAR file format