# FlatGeobuf

New in version 3.1.

Driver short name

FlatGeobuf

Driver built-in by default

This driver is built-in by default

This driver implements read/write support for access to features encoded in FlatGeobuf format, a performant binary encoding for geographic data based on flatbuffers that can hold a collection of Simple Features.

## Driver capabilities

Supports Create()

This driver supports the `GDALDriver::Create()` operation

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)

## Multi layer support

A single .fgb file only contains one single layer. For multiple layer support, it is possible to put several .fgb files in a directory, and use that directory name as the connection string.

On creation, passing a filename without a .fgb suffix will instruct the driver to create a directory of that name, and create layers as .fgb files in that directory.

## Open options

- VERIFY_BUFFERS=YES/NO: Set to YES to verify buffers when reading. This can provide some protection for invalid/corrupt data with a performance trade off. Defaults to YES.

## Dataset Creation Options

None

## Layer Creation Options

- SPATIAL_INDEX=YES/NO: Set to YES to create a spatial index. Defaults to YES.

- TEMPORARY_DIR=path: Path to an existing directory where temporary files should be created. Only used if SPATIAL_INDEX=YES. If not specified, the directory of the output file will be used for regular filenames. For other VSI file systems, the temporary directory will be the one decided by the `CPLGenerateTempFilename()` function. “/vsimem/” can be used for in-memory temporary files.

## Creation Issues

Currently, NULL geometries are not supported with SPATIAL_INDEX=YES.

More background and dicussion on this issue at

## Examples

- Simple translation of a single shapefile into a FlatGeobuf file. The file ‘filename.fgb’ will be created with the features from abc.shp and attributes from abc.dbf. The file `filename.fgb` must not already exist, as it will be created.

      ogr2ogr -f FlatGeobuf filename.fgb abc.shp

- Conversion of a Geopackage file with multiple layers:

      ogr2ogr -f FlatGeobuf my_fgb_dataset input.gpkg

## See Also

- FlatGeobuf at GitHub