# ogrlineref

Create linear reference and provide some calculations using it.

## Synopsis

    ogrlineref [--help-general] [-progress] [-quiet]
           [-f format_name] [[-dsco NAME=VALUE] ...] [[-lco NAME=VALUE]...]
           [-create]
           [-l src_line_datasource_name] [-ln layer_name] [-lf field_name]
           [-p src_repers_datasource_name] [-pn layer_name] [-pm pos_field_name] [-pf field_name]
           [-r src_parts_datasource_name] [-rn layer_name]
           [-o dst_datasource_name] [-on layer_name]  [-of field_name] [-s step]
           [-get_pos] [-x long] [-y lat]
           [-get_coord] [-m position]
           [-get_subline] [-mb position] [-me position]

## Description

The ogrlineref program can be used for:

- create linear reference file from input data

- return the “linear referenced” distance for the projection of the input coordinates (point) on the path

- return the coordinates (point) on the path according to the “linear referenced” distance

- return the portion of the path according to the “linear referenced” begin and end distances

The ogrlineref creates a linear reference - a file containing a segments of special length (e.g. 1 km in reference units) and get coordinates, linear referenced distances or sublines (subpaths) from this file. The utility not required the `M` or `Z` values in geometry. The results can be stored in any OGR supported format. Also some information is written to the stdout.

--help-general

  Show the usage.

-progress

  Show progress.

-quiet

  Suppress all messages except errors and results.

-f <format_name>

  Select an output format name. The default is to create a shapefile.

-dsco <NAME=VALUE>

  Dataset creation option (format specific)

-lco <NAME=VALUE>

  Layer creation option (format specific).

-create

  Create the linear reference file (linestring of parts).

-l <src_line_datasource_name>

  The path to input linestring datasource (e.g. the road)

-ln <layer_name>

  The layer name in datasource

-lf <field_name>

  The field name of unique values to separate the input lines (e.g. the set of roads).

-p <src_repers_datasource_name>

  The path to linear references points (e.g. the road mile-stones)

-pn <layer_name>

  The layer name in datasource

-pm <pos_field_name>

  The field name of distances along path (e.g. mile-stones values)

-pf <field_name>

  The field name of unique values to map input reference points to lines.

-r <src_parts_datasource_name>

  The path to linear reference file.

-rn <layer_name>

  The layer name in datasource

-o <dst_datasource_name>

  The path to output linear reference file (linestring datasource)

-on <layer_name>

  The layer name in datasource

-of <field_name>

  The field name for storing the unique values of input lines

-s <step>

  The part size in linear units

-get_pos

  Return linear referenced position for input X, Y

-x <long>

  Input X coordinate

-y <lat>

  Input Y coordinate

-get_coord

  Return point on path for input linear distance

-m <position>

  The input linear distance

-get_subline

  Return the portion of the input path from and to input linear positions.

-mb <position>

  The input begin linear distance

-me <position>

  The input end linear distance

## Example

This example would create a shapefile (`parts.shp`) containing a data needed for linear referencing (1 km parts):

    ogrlineref -create -l roads.shp -p references.shp -pm dist -o parts.shp -s 1000 -progress