.. raster_driver_summary:

..
  This file is generated by build_driver_summary.py. DO NOT EDIT !!!
  Do not put in git !!!
..
.. list-table::
   :widths: 10 35 10 10 10 25
   :header-rows: 1

   * - Short name
     - Long name
     - Creation
     - Copy
     - Geo-referencing
     - Build requirements
   * - :ref:`AAIGrid <raster.aaigrid>`
     - Arc/Info ASCII Grid
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ACE2 <raster.ace2>`
     - ACE2
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`ADRG <raster.adrg>`
     - ADRG/ARC Digitized Raster Graphics (.gen/.thf)
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`AIG <raster.aig>`
     - Arc/Info Binary Grid
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`AIRSAR <raster.airsar>`
     - AIRSAR Polarimetric Format
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`ARG <raster.arg>`
     - Azavea Raster Grid
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`BAG <raster.bag>`
     - Bathymetry Attributed Grid
     - **Yes**
     - **Yes**
     - **Yes**
     - libhdf5
   * - :ref:`BASISU <raster.basisu>`
     - Basis Universal
     - No
     - **Yes**
     - No
     - Basis Universal
   * - :ref:`BLX <raster.blx>`
     - Magellan BLX Topo File Format
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`BMP <raster.bmp>`
     - Microsoft Windows Device Independent Bitmap
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`BSB <raster.bsb>`
     - Maptech/NOAA BSB Nautical Chart Format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`BT <raster.bt>`
     - VTP .bt Binary Terrain Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`BYN <raster.byn>`
     - Natural Resources Canada's Geoid file format (.byn)
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`CAD <raster.cad>`
     - AutoCAD DWG raster layer
     - No
     - No
     - **Yes**
     - (internal libopencad provided)
   * - :ref:`CALS <raster.cals>`
     - CALS Type 1
     - No
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`CEOS <raster.ceos>`
     - CEOS Image
     - No
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`COASP <raster.coasp>`
     -  DRDC COASP SAR Processor Raster
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`COG <raster.cog>`
     - Cloud Optimized GeoTIFF generator
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`COSAR <raster.cosar>`
     - TerraSAR-X Complex SAR Data Product
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`CPG <raster.cpg>`
     - Convair PolGASP data
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`CTable2 <raster.ctable2>`
     - CTable2 Datum Grid Shift
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`CTG <raster.ctg>`
     - USGS LULC Composite Theme Grid
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`DAAS <raster.daas>`
     - DAAS (Airbus DS Intelligence Data As A Service driver)
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`DDS <raster.dds>`
     - DirectDraw Surface
     - No
     - **Yes**
     - No
     - Crunch Lib
   * - :ref:`DERIVED <raster.derived>`
     - Derived subdatasets driver
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`DIMAP <raster.dimap>`
     - Spot DIMAP
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`DIPEx <raster.dipex>`
     - ELAS DIPEx
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`DOQ1 <raster.doq1>`
     - First Generation USGS DOQ
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`DOQ2 <raster.doq2>`
     - New Labelled USGS DOQ
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`DTED <raster.dted>`
     - Military Elevation Data
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ECRGTOC <raster.ecrgtoc>`
     - ECRG Table Of Contents (TOC.xml)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`ECW <raster.ecw>`
     - Enhanced Compressed Wavelets (.ecw)
     - **Yes**
     - **Yes**
     - **Yes**
     - ECW SDK
   * - :ref:`EEDAI <raster.eedai>`
     - Google Earth Engine Data API Image
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`EHdr <raster.ehdr>`
     - ESRI .hdr Labelled
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`EIR <raster.eir>`
     - Erdas Imagine Raw
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`ELAS <raster.elas>`
     - Earth Resources Laboratory Applications Software
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ENVI <raster.envi>`
     - ENVI .hdr Labelled Raster
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ERS <raster.ers>`
     - ERMapper .ERS
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ESAT <raster.esat>`
     - Envisat Image Product
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`ESRIC <raster.esric>`
     - Esri Compact Cache
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`EXR <raster.exr>`
     - Extended Dynamic Range Image File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - libopenexr
   * - :ref:`FAST <raster.fast>`
     - EOSAT FAST Format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`FIT <raster.fit>`
     - FIT
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`FITS <raster.fits>`
     - Flexible Image Transport System
     - **Yes**
     - **Yes**
     - **Yes**
     - libcfitsio
   * - :ref:`GenBin <raster.genbin>`
     - Generic Binary (.hdr labelled)
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`GeoRaster <raster.georaster>`
     - Oracle Spatial GeoRaster
     - **Yes**
     - **Yes**
     - **Yes**
     - Oracle client libraries
   * - :ref:`GFF <raster.gff>`
     - Sandia National Laboratories GSAT File Format
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`GIF <raster.gif>`
     - Graphics Interchange Format
     - No
     - **Yes**
     - No
     - (internal GIF library provided)
   * - :ref:`GPKG <raster.gpkg>`
     - GeoPackage raster
     - **Yes**
     - **Yes**
     - **Yes**
     - libsqlite3 (and any or all of PNG, JPEG, WEBP drivers)
   * - :ref:`GRASS <raster.grass>`
     - GRASS Raster Format
     - No
     - No
     - No
     - gdal-grass-driver
   * - :ref:`GRASSASCIIGrid <raster.grassasciigrid>`
     - GRASS ASCII Grid
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`GRIB <raster.grib>`
     - WMO General Regularly-distributed Information in Binary form
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`GS7BG <raster.gs7bg>`
     - Golden Software Surfer 7 Binary Grid File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`GSAG <raster.gsag>`
     - Golden Software ASCII Grid File Format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`GSBG <raster.gsbg>`
     - Golden Software Binary Grid File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`GSC <raster.gsc>`
     - GSC Geogrid
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`GTA <raster.gta>`
     - Generic Tagged Arrays
     - No
     - **Yes**
     - **Yes**
     - libgta
   * - :ref:`GTiff <raster.gtiff>`
     - GeoTIFF File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`GXF <raster.gxf>`
     - Grid eXchange File
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`HDF4 <raster.hdf4>`
     - Hierarchical Data Format Release 4 (HDF4)
     - **Yes**
     - **Yes**
     - **Yes**
     - libdf
   * - :ref:`HDF5 <raster.hdf5>`
     - Hierarchical Data Format Release 5 (HDF5)
     - No
     - No
     - **Yes**
     - libhdf5
   * - :ref:`HEIF <raster.heif>`
     - ISO/IEC 23008-12:2017 High Efficiency Image File Format
     - No
     - No
     - No
     - libheif (>= 1.1), built against libde265
   * - :ref:`HF2 <raster.hf2>`
     - HF2/HFZ heightfield raster
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`HFA <raster.hfa>`
     - Erdas Imagine .img
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`RST <raster.Idrisi>`
     - Idrisi Raster Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ILWIS <raster.ilwis>`
     - Raster Map
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`IRIS <raster.iris>`
     - Vaisala's weather radar software format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`ISCE <raster.isce>`
     - ISCE
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ISG <raster.isg>`
     - International Service for the Geoid
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`ISIS2 <raster.isis2>`
     - USGS Astrogeology ISIS Cube (Version 2)
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ISIS3 <raster.isis3>`
     - USGS Astrogeology ISIS Cube (Version 3)
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`JDEM <raster.jdem>`
     - Japanese DEM (.mem)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`JP2ECW <raster.jp2ecw>`
     - ERDAS JPEG2000 (.jp2)
     - **Yes**
     - **Yes**
     - **Yes**
     - ECW SDK
   * - :ref:`JP2KAK <raster.jp2kak>`
     - JPEG-2000 (based on Kakadu)
     - No
     - **Yes**
     - **Yes**
     - Kakadu library
   * - :ref:`JP2LURA <raster.jp2lura>`
     - JPEG2000 driver based on Lurawave library
     - No
     - **Yes**
     - **Yes**
     - Lurawave library
   * - :ref:`JP2MrSID <raster.jp2mrsid>`
     - JPEG2000 via MrSID SDK
     - No
     - **Yes**
     - **Yes**
     - MrSID SDK
   * - :ref:`JP2OpenJPEG <raster.jp2openjpeg>`
     - JPEG2000 driver based on OpenJPEG library
     - No
     - **Yes**
     - **Yes**
     - openjpeg >= 2.1
   * - :ref:`JPEG <raster.jpeg>`
     - JPEG JFIF File Format
     - No
     - **Yes**
     - **Yes**
     - (internal libjpeg provided)
   * - :ref:`JPEGXL <raster.jpegxl>`
     - JPEG-XL File Format
     - No
     - **Yes**
     - **Yes**
     - libjxl
   * - :ref:`JPIPKAK <raster.jpipkak>`
     - JPIP Streaming
     - No
     - No
     - **Yes**
     - Kakadu library
   * - :ref:`KEA <raster.kea>`
     - KEA
     - **Yes**
     - **Yes**
     - **Yes**
     - libkea and libhdf5 libraries
   * - :ref:`KMLSuperoverlay <raster.kmlsuperoverlay>`
     - KMLSuperoverlay
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`KRO <raster.kro>`
     - KOLOR Raw format
     - **Yes**
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`KTX2 <raster.ktx2>`
     - KTX2
     - No
     - **Yes**
     - No
     - Basis Universal
   * - :ref:`L1B <raster.l1b>`
     - NOAA Polar Orbiter Level 1b Data Set (AVHRR)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`LAN <raster.lan>`
     - Erdas 7.x .LAN and .GIS
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`LCP <raster.lcp>`
     - FARSITE v.4 LCP Format
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`Leveller <raster.leveller>`
     - Daylon Leveller Heightfield
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`LOSLAS <raster.loslas>`
     - NADCON .los/.las Datum Grid Shift
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`MAP <raster.map>`
     - OziExplorer .MAP
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`MRF <raster.marfa>`
     - Meta Raster Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`MBTiles <raster.mbtiles>`
     - MBTiles
     - **Yes**
     - **Yes**
     - **Yes**
     - libsqlite3
   * - :ref:`MEM <raster.mem>`
     - In Memory Raster
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`MFF <raster.mff>`
     - Vexcel MFF Raster
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`MFF2 <raster.mff2>`
     - Vexcel MFF2 Image
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`MrSID <raster.mrsid>`
     - Multi-resolution Seamless Image Database
     - No
     - No
     - **Yes**
     - MrSID SDK
   * - :ref:`MSG <raster.msg>`
     - Meteosat Second Generation
     - No
     - No
     - **Yes**
     - msg library
   * - :ref:`MSGN <raster.msgn>`
     - Meteosat Second Generation (MSG) Native Archive Format (.nat)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`NDF <raster.ndf>`
     - NLAPS Data Format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`netCDF <raster.netcdf>`
     - NetCDF: Network Common Data Form
     - **Yes**
     - **Yes**
     - **Yes**
     - libnetcdf
   * - :ref:`NGSGEOID <raster.ngsgeoid>`
     - NOAA NGS Geoid Height Grids
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`NGW <raster.ngw>`
     - NextGIS Web
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`NITF <raster.nitf>`
     - National Imagery Transmission Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`NOAA_B <raster.noaa_b>`
     - NOAA GEOCON/NADCON5 .b format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`NSIDCbin <raster.nsidcbin>`
     - National Snow and Ice Data Centre Sea Ice Concentrations
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`NTv2 <raster.ntv2>`
     - NTv2 Datum Grid Shift
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`NWT_GRD <raster.nwtgrd>`
     - Northwood/Vertical Mapper File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`NWT_GRC <raster.nwtgrd>`
     - Northwood/Vertical Mapper File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`OGCAPI <raster.ogcapi>`
     - OGC API Tiles / Maps / Coverage
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`OpenFileGDB <raster.openfilegdb>`
     - ESRI File Geodatabase raster (OpenFileGDB)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`OZI <raster.ozi>`
     - OZF2/OZFX3 raster
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`JAXAPALSAR <raster.palsar>`
     - JAXA PALSAR Processed Products
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`PAux <raster.paux>`
     - PCI .aux Labelled Raw Format
     - **Yes**
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`PCIDSK <raster.pcidsk>`
     - PCI Geomatics Database File
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`PCRaster <raster.pcraster>`
     - PCRaster raster file format
     - **Yes**
     - **Yes**
     - **Yes**
     - (internal libcf provided)
   * - :ref:`PDF <raster.pdf>`
     - Geospatial PDF
     - No
     - **Yes**
     - **Yes**
     - none for write support, Poppler/PoDoFo/PDFium for read support
   * - :ref:`PDS <raster.pds>`
     - Planetary Data System v3
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`PDS4 <raster.pds4>`
     - NASA Planetary Data System (Version 4)
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`PLMosaic <raster.plmosaic>`
     - PLMosaic (Planet Labs Mosaics API)
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`PNG <raster.png>`
     - Portable Network Graphics
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`PNM <raster.pnm>`
     - Netpbm (.pgm, .ppm)
     - No
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`PostGISRaster <raster.postgisraster>`
     - PostGIS Raster driver
     - No
     - **Yes**
     - **Yes**
     - PostgreSQL library
   * - :ref:`PRF <raster.prf>`
     - PHOTOMOD Raster File
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`R <raster.r>`
     - R Object Data Store
     - No
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`Rasterlite <raster.rasterlite>`
     - Rasters in SQLite DB
     - No
     - **Yes**
     - **Yes**
     - libsqlite3
   * - :ref:`SQLite <raster.rasterlite2>`
     - Rasters in SQLite DB
     - No
     - **Yes**
     - **Yes**
     - libsqlite3, librasterlite2, libspatialite
   * - :ref:`RDB <raster.rdb>`
     - *RIEGL* Database
     - No
     - No
     - **Yes**
     - rdblib >= 2.2.0.
   * - :ref:`RIK <raster.rik>`
     - Swedish Grid Maps
     - No
     - No
     - **Yes**
     - (internal zlib is used if necessary)
   * - :ref:`RMF <raster.rmf>`
     - Raster Matrix Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`ROI_PAC <raster.roi_pac>`
     - ROI_PAC
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`RPFTOC <raster.rpftoc>`
     - Raster Product Format/RPF (a.toc)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`RRASTER <raster.rraster>`
     - R Raster
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`RS2 <raster.rs2>`
     - RadarSat 2 XML Product
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`S102 <raster.s102>`
     - S-102 Bathymetric Surface Product
     - No
     - No
     - **Yes**
     - libhdf5
   * - :ref:`SAFE <raster.safe>`
     - Sentinel-1 SAFE XML Product
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SAR_CEOS <raster.sar_ceos>`
     - CEOS SAR Image
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SAGA <raster.sdat>`
     - SAGA GIS Binary Grid File Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`SDTS <raster.sdts>`
     - USGS SDTS DEM
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SENTINEL2 <raster.sentinel2>`
     - Sentinel-2 Products
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SGI <raster.sgi>`
     - SGI Image Format
     - **Yes**
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`SIGDEM <raster.sigdem>`
     - Scaled Integer Gridded DEM
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`SNODAS <raster.snodas>`
     - Snow Data Assimilation System
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SRP <raster.srp>`
     - Standard Product Format (ASRP/USRP) (.gen)
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`SRTMHGT <raster.srtmhgt>`
     - SRTM HGT Format
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`STACIT <raster.stacit>`
     - Spatio-Temporal Asset Catalog Items
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`STACTA <raster.stacta>`
     - Spatio-Temporal Asset Catalog Tiled Assets
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`Terragen <raster.terragen>`
     - Terragen™ Terrain File
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`TGA <raster.tga>`
     - TARGA Image File Format
     - No
     - No
     - No
     - Built-in by default
   * - :ref:`TIL <raster.til>`
     - EarthWatch/DigitalGlobe .TIL
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`TileDB <raster.tiledb>`
     - TileDB raster
     - **Yes**
     - **Yes**
     - **Yes**
     - TileDB (>= 2.7 starting with GDAL 3.7)
   * - :ref:`TSX <raster.tsx>`
     -  TerraSAR-X Product
     - No
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`USGSDEM <raster.usgsdem>`
     - USGS ASCII DEM (and CDED)
     - **Yes**
     - No
     - **Yes**
     - Built-in by default
   * - :ref:`VICAR <raster.vicar>`
     - VICAR
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`VRT <raster.vrt>`
     - GDAL Virtual Format
     - **Yes**
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`WCS <raster.wcs>`
     - OGC Web Coverage Service
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`WEBP <raster.webp>`
     - WEBP
     - No
     - **Yes**
     - No
     - libwebp
   * - :ref:`WMS <raster.wms>`
     - Web Map Services
     - No
     - **Yes**
     - **Yes**
     - libcurl
   * - :ref:`WMTS <raster.wmts>`
     - OGC Web Map Tile Service
     - No
     - No
     - **Yes**
     - libcurl
   * - :ref:`XPM <raster.xpm>`
     - X11 Pixmap
     - No
     - **Yes**
     - No
     - Built-in by default
   * - :ref:`XYZ <raster.xyz>`
     - ASCII Gridded XYZ
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
   * - :ref:`Zarr <raster.zarr>`
     - Zarr
     - **Yes**
     - No
     - **Yes**
     - Built-in by default, but liblz4, libxz (lzma), libzstd and libblosc
   * - :ref:`ZMAP <raster.zmap>`
     - ZMap Plus Grid
     - No
     - **Yes**
     - **Yes**
     - Built-in by default
