# GPX - GPS Exchange Format

Driver short name

GPX

Build dependencies

(read support needs libexpat)

GPX (the GPS Exchange Format) is a light-weight XML data format for the interchange of GPS data (waypoints, routes, and tracks) between applications and Web services on the Internet.

OGR has support for GPX reading (if GDAL is build with expat library support) and writing.

Version supported are GPX 1.0 and 1.1 for reading, GPX 1.1 for writing.

The OGR driver supports reading and writing of all the GPX feature types:

- waypoints : layer of features of OGR type wkbPoint

- routes : layer of features of OGR type wkbLineString

- tracks : layer of features of OGR type wkbMultiLineString

It also supports reading of route points and track points in standalone layers (route_points and track_points), so that their own attributes can be used by OGR.

In addition to its GPX attributes, each route point of a route has a route_fid (foreign key to the FID of its belonging route) and a route_point_id which is its sequence number in the route.
The same applies for track points with track_fid, track_seg_id and track_seg_point_id. All coordinates are relative to the WGS84 datum (EPSG:4326).

The OGR GPX driver reads and writes the GPX attributes for the waypoints, routes and tracks.

Starting with GDAL 3.7, metadata from the top <metadata> element is reported at dataset level.

## Driver capabilities

Supports Create()

This driver supports the `GDALDriver::Create()` operation

Supports Georeferencing

This driver supports georeferencing

Supports VirtualIO

This driver supports virtual I/O operations (/vsimem/, etc.)

## Configuration options

The following configuration options are available:

- GPX_USE_EXTENSIONS=value: See Extensions element reading.

- GPX_SHORT_NAMES=[TRUE/FALSE]: Defaults to `FALSE`. If `TRUE`, the following fields will be renamed:

  - "track_seg_id" to "trksegid"

  - "track_seg_point_id" to "trksegptid"

  - "route_point_id" to "rteptid"

  But note that no particular processing will be done for any extension field names.

- GPX_ELE_AS_25D=[YES/NO]: Defaults to `NO`. If `YES`, the elevation element will be used to set the Z coordinates of waypoints, route points and track points.

- GPX_N_MAX_LINKS=value: Defaults to `2`. Determines the number of <link> elements can be taken into account by feature.

## Open options

New in version 3.9.

The following open options are available:

- SHORT_NAMES=[YES/NO]: Defaults to `FALSE`. If `YES`, the following fields will be renamed:

  - "track_seg_id" to "trksegid"

  - "track_seg_point_id" to "trksegptid"

  - "route_point_id" to "rteptid"

  But note that no particular processing will be done for any extension field names.

- ELE_AS_25D=[YES/NO]: Defaults to `NO`. If `YES`, the elevation element will be used to set the Z coordinates of waypoints, route points and track points.

- N_MAX_LINKS=value: Defaults to `2`. Determines the number of <link> elements can be taken into account by feature.

## Encoding issues

Expat library supports reading the following built-in encodings :

- US-ASCII

- UTF-8

- UTF-16

- ISO-8859-1

- Windows-1252

The content returned by OGR will be encoded in UTF-8, after the conversion from the encoding mentioned in the file header is.

If your GPX file is not encoded in one of the previous encodings, it will not be parsed by the GPX driver. You may convert it into one of the supported encoding with the iconv utility for example and change accordingly the encoding parameter value in the XML header.

When writing a GPX file, the driver expects UTF-8 content to be passed in.

## Extensions element reading

If the <extensions> element is detected in a GPX file, OGR will expose the content of its sub elements as fields. Complex content of sub elements will be exposed as an XML blob.

The following sequence GPX content :

    <extensions>
        <navaid:name>TOTAL RF</navaid:name>
        <navaid:address>BENSALEM</navaid:address>
        <navaid:state>PA</navaid:state>
        <navaid:country>US</navaid:country>
        <navaid:frequencies>
        <navaid:frequency type="CTAF" frequency="122.900" name="CTAF"/>
        </navaid:frequencies>
        <navaid:runways>
        <navaid:runway designation="H1" length="80" width="80" surface="ASPH-G">
        </navaid:runway>
        </navaid:runways>
        <navaid:magvar>12</navaid:magvar>
    </extensions>

will be interpreted in the OGR SF model as :

    navaid_name (String) = TOTAL RF
    navaid_address (String) = BENSALEM
    navaid_state (String) = PA
    navaid_country (String) = US
    navaid_frequencies (String) = <navaid:frequency type="CTAF" frequency="122.900" name="CTAF" ></navaid:frequency>
    navaid_runways (String) = <navaid:runway designation="H1" length="80" width="80" surface="ASPH-G" ></navaid:runway>
    navaid_magvar (Integer) = 12

Note : the GPX driver will output content of the extensions element only if it is found in the first records of the GPX file. If extensions appear later, you can force an explicit parsing of the whole file with the `GPX_USE_EXTENSIONS` configuration option.

## Creation Issues

On export all layers are written to a single GPX file. Update of existing files is not currently supported.

If the output file already exits, the writing will not occur. You have to delete the existing file first.

Supported geometries :

- Features of type wkbPoint/wkbPoint25D are written in the wpt element.

- Features of type wkbLineString/wkbLineString25D are written in the rte element.

- Features of type wkbMultiLineString/wkbMultiLineString25D are written in the trk element.

- Other type of geometries are not supported.

For route points and tracks points, if there is a Z coordinate, it is used to fill the elevation element of the corresponding points.

If a layer is named "track_points" with wkbPoint/wkbPoint25D geometries, the tracks in the GPX file will be built from the sequence of features in that layer. This is the way of setting GPX attributes for each track point, in addition to the raw coordinates. Points belonging to the same track are identified thanks to the same value of the 'track_fid' field (and it will be broken into track segments according to the value of the 'track_seg_id' field). They must be written in sequence so that track objects are properly reconstructed. The 'track_name' field can be set on the first track point to fill the <name> element of the track. Similarly, if a layer is named "route_points" with wkbPoint/wkbPoint25D geometries, the routes in the GPX file will be built from the sequence of points with the same value of the 'route_fid' field. The 'route_name' field can be set on the first track point to fill the <name> element of the route.

## Layer creation options

- FORCE_GPX_TRACK=[YES/NO]: Defaults to `NO`. By default when writing a layer whose features are of type wkbLineString, the GPX driver chooses to write them as routes. If YES is specified, they will be written as tracks.

- FORCE_GPX_ROUTE=[YES/NO]: Defaults to `NO`. By default when writing a layer whose features are of type wkbMultiLineString, the GPX driver chooses to write them as tracks. If YES is specified, they will be written as routes, provided that the multilines are composed of only one single line.

## Dataset creation options

- GPX_USE_EXTENSIONS=[YES/NO]: Defaults to `NO`. By default, the GPX driver will discard attribute fields that do not match the GPX XML definition (name, cmt, etc...). If `GPX_USE_EXTENSIONS=YES` is specified, extra fields will be written inside the<extensions> tag.

- GPX_EXTENSIONS_NS=value: Defaults to `ogr`. The namespace value used for extension tags. Only used if `GPX_USE_EXTENSIONS=YES` and `GPX_EXTENSIONS_NS_URL` is set.

- GPX_EXTENSIONS_NS_URL=value: Defaults to `"http://osgeo.org/gdal"`. The namespace URI. Only used if `GPX_USE_EXTENSIONS=YES` and `GPX_EXTENSIONS_NS` is set.

- LINEFORMAT=[CRLF/LF]: By default files are created with the line termination conventions of the local platform (CR/LF on win32 or LF on all other systems). This may be overridden through use of this option.

- CREATOR=value: (GDAL >= 3.8) Name of creating application. Defaults to `GDAL `` followed by its version number.

Dataset creation options to fill the top <metadata> element have been added in GDAL 3.7:

- METADATA_AUTHOR_EMAIL=value: (GDAL >= 3.7)

- METADATA_AUTHOR_NAME=value: (GDAL >= 3.7)

- METADATA_AUTHOR_LINK_HREF=value: (GDAL >= 3.7)

- METADATA_AUTHOR_LINK_TEXT=value: (GDAL >= 3.7)

- METADATA_AUTHOR_LINK_TYPE=value: (GDAL >= 3.7)

- METADATA_COPYRIGHT_AUTHOR=value: (GDAL >= 3.7)

- METADATA_COPYRIGHT_LICENSE=value: (GDAL >= 3.7)

- METADATA_COPYRIGHT_YEAR=value: (GDAL >= 3.7)

- METADATA_DESCRIPTION=value: (GDAL >= 3.7)

- METADATA_KEYWORDS=value: (GDAL >= 3.7)

- METADATA_LINK_{N}_HREF=value: (GDAL >= 3.7) where {N} should be substituted with a serial number (1, 2, ...)

- METADATA_LINK_{N}_TEXT=value: (GDAL >= 3.7) where {N} should be substituted with a serial number (1, 2, ...)

- METADATA_LINK_{N}_TYPE=value: (GDAL >= 3.7) where {N} should be substituted with a serial number (1, 2, ...)

- METADATA_NAME=value: (GDAL >= 3.7)

- METADATA_TIME=value: (GDAL >= 3.7)

Waypoints, routes and tracks must be written into that order to be valid against the XML Schema.

When translating from a source dataset, it may be necessary to rename the field names from the source dataset to the expected GPX attribute names, such as <name>, <desc>, etc... This can be done with a OGR VRT dataset, or by using the "-sql" option of the ogr2ogr utility.

## Issues when translating to Shapefile

- When translating the track_points layer to a Shapefile, the field names "track_seg_id" and "track_seg_point_id" are truncated to 10 characters in the .DBF file, thus leading to duplicate names.

  To avoid this, you can define the `GPX_SHORT_NAMES` configuration option to TRUE.

  To translate the track_points layer of a GPX file to a set of shapefiles :

      ogr2ogr --config GPX_SHORT_NAMES YES out input.gpx track_points

- Shapefile does not support fields of type DateTime. It only supports fields of type Date. So by default, you will lose the hour:minute:second part of the Time elements of a GPX file.

  You can use the OGR SQL CAST operator to convert the time field to a string :

      ogr2ogr out input.gpx -sql "SELECT ele, CAST(time AS character(32)) FROM waypoints"

  There is a more convenient way to select all fields and ask for the conversion of the ones of a given type to strings:

      ogr2ogr out input.gpx -fieldTypeToString DateTime

## VSI Virtual File System API support

The driver supports reading and writing to files managed by VSI Virtual File System API, which include "regular" files, as well as files in the /vsizip/ (read-write) , /vsigzip/ (read-write) , /vsicurl/ (read-only) domains.

Writing to /dev/stdout or /vsistdout/ is also supported.

## Example

The ogrinfo utility can be used to dump the content of a GPX datafile :

    ogrinfo -ro -al input.gpx

The ogr2ogr utility can be used to do GPX to GPX translation :

    ogr2ogr -f GPX output.gpx input.gpx waypoints routes tracks

Note : in the case of GPX to GPX translation, you need to specify the layer names, in order to discard the route_points and track_points layers.

Use of the <extensions> tag for output :

    ogr2ogr -f GPX  -dsco GPX_USE_EXTENSIONS=YES output.gpx input

which will give an output like the following one :

    <?xml version="1.0"?>
    <gpx version="1.1" creator="GDAL 1.5dev"
    xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
    xmlns:ogr="http://osgeo.org/gdal"
    xmlns="http://www.topografix.com/GPX/1/1"
    xsi:schemaLocation="http://www.topografix.com/GPX/1/1 http://www.topografix.com/GPX/1/1/gpx.xsd">
    <wpt lat="1" lon="2">
    <extensions>
        <ogr:Primary_ID>PID5</ogr:Primary_ID>
        <ogr:Secondary_ID>SID5</ogr:Secondary_ID>
    </extensions>
    </wpt>
    <wpt lat="3" lon="4">
    <extensions>
        <ogr:Primary_ID>PID4</ogr:Primary_ID>
        <ogr:Secondary_ID>SID4</ogr:Secondary_ID>
    </extensions>
    </wpt>
    </gpx>

Use of -sql option to remap field names to the ones allowed by the GPX schema:

    ogr2ogr -f GPX output.gpx input.shp -sql "SELECT field1 AS name, field2 AS desc FROM input"

## FAQ

How to solve "ERROR 6: Cannot create GPX layer XXXXXX with unknown geometry type" ?

This error happens when the layer to create does not expose a precise geometry type, but just a generic wkbUnknown type. This is for example the case when using ogr2ogr with a SQL request to a PostgreSQL datasource. You must then explicitly specify -nlt POINT (or LINESTRING or MULTILINESTRING).

## See Also

- Home page for GPX format

- GPX 1.1 format documentation