# FAST -- EOSAT FAST Format

Supported reading from FAST-L7A format (Landsat TM data) and EOSAT Fast Format Rev. C (IRS-1C/1D data). If you want to read other datasets in this format (SPOT), write to me (Andrey Kiselev, dron@remotesensing.org). You should share data samples with me.

Datasets in FAST format represented by several files: one or more administrative headers and one or more files with actual image data in raw format. Administrative files contains different information about scene parameters including filenames of images. You can read files with administrative headers with any text viewer/editor, it is just plain ASCII text.

This driver wants administrative file for input. Filenames of images will be extracted and data will be imported, every file will be interpreted as band.

## Data

### FAST-L7A

FAST-L7A consists form several files: big ones with image data and three small files with administrative information. You should give to driver one of the administrative files:

- L7fppprrr_rrrYYYYMMDD_HPN.FST: panchromatic band header file with 1 band
- L7fppprrr_rrrYYYYMMDD_HRF.FST: VNIR/ SWIR bands header file with 6 bands
- L7fppprrr_rrrYYYYMMDD_HTM.FST: thermal bands header file with 2 bands

All raw images corresponded to their administrative files will be imported as GDAL bands.

From the `` Level 1 Product Output Files Data Format Control Book'':

`The file naming convention for the FAST-L7A product files is
L7fppprrr_rrrYYYYMMDD_AAA.FST
where
L7 = Landsat 7 mission
f = ETM+ format (1 or 2) (data not pertaining to a specific format defaults to 1)
ppp = starting path of the product
rrr_rrr = starting and ending rows of the product
YYYYMMDD = acquisition date of the image
AAA = file type:
HPN = panchromatic band header file
HRF = VNIR/ SWIR bands header file
HTM = thermal bands header file
B10 = band 1
B20 = band 2
B30 = band 3
B40 = band 4
B50 = band 5
B61 = band 6L
B62 = band 6H
B70 = band 7
B80 = band 8
FST = FAST file extension
`

So you should give to driver one of the `L7fppprrr_rrrYYYYMMDD_HPN.FST`, `L7fppprrr_rrrYYYYMMDD_HRF.FST` or `L7fppprrr_rrrYYYYMMDD_HTM.FST` files.

### IRS-1C/1D

Fast Format REV. C does not contain band filenames in administrative header. So we should guess band filenames, because different data distributors name their files differently. Several naming schemes hardcoded in GDAL's FAST driver. These are:

`<header>.<ext>
<header>.1.<ext>
<header>.2.<ext>
...
`

or

`<header>.<ext>
band1.<ext>
band2.<ext>
...
`

or

`<header>.<ext>
band1.dat
band2.dat
...
`

or

`<header>.<ext>
imagery1.<ext>
imagery2.<ext>
...
`

or

`<header>.<ext>
imagery1.dat
imagery2.dat
...
`

in lower or upper case. Header file could be named arbitrarily. This should cover majority of distributors fantasy in naming files. But if you out of luck and your datasets named differently you should rename them manually before importing data with GDAL.

## Georeference

All USGS projections should be supported (namely UTM, LCC, PS, PC, TM, OM). Contact me if you have troubles with proper projection extraction.

## Metadata

Calibration coefficients for each band reported as metadata items.

- ACQUISITION_DATE: First scene acquisition date in yyyyddmm format.

- SATELLITE: First scene satellite name.

- SENSOR: First scene sensor name.

- BIASn: Bias value for the channel n.

- GAINn: Gain value for the channel n.

## See Also:

- Implemented as `gdal/frmts/fast/fastdataset.cpp`.

- Landsat FAST L7A format description available from http://ltpwww.gsfc.nasa.gov/IAS/htmls/l7_review.html (see ESDIS Level 1 Product Generation System (LPGS) Output Files DFCB, Vol. 5, Book 2)

- EOSAT Fast Format REV. C description available from http://www.euromap.de/doc_001.htm