| OGR WCTS - Web Coordinate Transformation Service The Web Coordinate Transformation Service enables the transformation of geometries between different coordinate reference systems (CRS).
WCTS Server
Provide the WCTS server.
Server |
Coordinate Reference Systems (CRS)
Provide the original and target coordinate reference system (CRS) as EPSG PCS or GCS codes. Some examples are: • 4326: Lat/Long WGS84 • 4269: Lat/Long NAD83 • 4267: Lat/Long NAD27 • 32611: UTM 11 WGS84 • 26911: UTM 11 NAD83 • 26711: UTM 11 NAD27
Source | CRS / Projection
Target | CRS / Projection
Point / Location
Provide the X and Y coordinates for the point / location in decimal degrees. An example is: -117 44
Source | X / Longitude / Easting |
| Y / Latitude / Northing |
GML Dataset
Provide a URL to the GML dataset, or paste the GML directly into the textbox.
Source | URL:
| GML: