#ifndef DOXYGEN_SKIP
/* $Id: vb6_tutorial.dox 13528 2008-01-14 19:37:42Z warmerdam $ */
#endif /* DOXYGEN_SKIP */

/*!
\page vb6_tutorial GDAL VB6 Bindings Tutorial

\section Intro Introduction

A partial set of Visual Basic 6 bindings have been build for GDAL.  Internally 
these bindings use Declare based calls into the GDAL DLL C API but a set of
shadow classes are also provided to provide object oriented access to 
GDAL services in VB6 similar to those provided in C++. 

Note that the VB6 bindings are nowhere near comprehensive, nor are they 
documented.  However, in combination with the corresponding C++ class
documentation, and the following docs, it should be possible to use GDAL 
to accomplish a variety of operations.  It is not believed that the VB6
bindings will be of any utility with earlier version of VB nor with VB.Net. 

The classes for which access has been implemented includes 
GDALDriver, GDALDataset, GDALRasterBand, GDALColorTable, OGRSpatialReference
and OGRCoordinateTransformation.

A mailing list specifically on VB6 GDAL topics has been setup at
http://groups.yahoo.com/group/gdal-vb6-appdev .

\section UsingVB6 Using GDAL VB6 Classes

To use VB6 GDAL bindings it is necessary to ensure that GDAL has been
built with appropriate C entry points exported using the "stdcall" calling
convention.  This is the current default, but was not as recently as GDAL
1.2.6.  So ensure you get a version more recent than 1.2.6.  

Then add the GDAL VB6 class and module files to your VB6 project.  These
come from the <a href="http://svn.osgeo.org/gdal/trunk/gdal/vb6">gdal/vb6 directory</a>
and include the following key files:

<ul>
<li> GDAL.bas - The main user visible module. 
<li> GDALCore.bas - This module is for internal use. 
<li> GDALDriver.cls - The GDALDriver class. 
<li> GDALDataset.cls - The GDALDataset class.
<li> GDALRasterBand.cls - The GDALRasterBand class. 
<li> GDALColorTable.cls - The GDALColorTable class.
<li> OGRSpatialReference.cls - The OGRSpatialReference class. 
<li> OGRCoordinateTransformation.cls - The OGRCoordinateTransformation class.
</ul>

You may need to edit GDALCore.bas, and change occurrences of gdal12.dll 
to match what your GDAL DLL is called.  You can include a full path to the
DLL if it can't be guaranteed to be in the current working directory of the
application (or the windows system32 directory).  

You should also be able to load the "test" project from the gdal\\vb6\\test
directory.  The test project has test menu items roughly corresponding to
the tasks in the following tutorial topics.  

\section TutorialRead Tutorial - Read Dataset

This brief tutorial will demonstrate open a GDAL file, and fetching out
some information, about the dataset, and the individual bands.  The
results are printed to the default from in the following example for 
simplicity. 

Before opening the file we need to register the GDAL format drivers.
Normally we will just register all the drivers with GDALAllRegister().

\code
  Call GDAL.AllRegister()
\endcode

Then we need to try and open the dataset.  The GDAL.OpenDS() function
returns a GDALDataset object, so we dimension an appropriate object for
this.  GDAL.OpenDS() is the VB6 equivalent of the GDALDataset::GDALOpen() 
function.

\code
  Dim ds As GDALDataset

  Set ds = GDAL.OpenDS( "utm.tif", GDAL.GA_ReadOnly )
\endcode
  
Then we need to check if the open succeeded, and if not report an error. 

\code
  If not ds.IsValid() Then
    Call MsgBox( "Open failed: " & GDAL.GetLastErrorMsg() )
    Exit Sub
  End If
\endcode

If things succeeded, we query width of the image in pixels (XSize),
Height of the image in pixels (YSize) and number of bands (BandCount)
from the dataset properties.

\code
  Print "Size: " & ds.XSize & "x" & ds.YSize & "x" & ds.BandCount
\endcode

Next we read metadata from the dataset using the VB6 equivalent of the
GDALMajorObject::GetMetadata() method, and report it to the user.  Metadata
is returned as an array of strings of "name=value" items.  Array indices 
start at zero in the returned array.  The domain argument should normally
be vbNullString though in specialized circumstances other domains might
apply.

\code
  Dim MD As Variant
  MD = ds.GetMetadata(vbNullString)
  If (UBound(MD) > 0) Then
    Print "Metadata:"
    For i = 1 To UBound(MD)
      Print "  " & MD(i)
    Next i
  End If
\endcode

Parsing the "name=value" strings from GetMetadata() can be a bit of a bother,
so if we were looking for specific values we could use GetMetadataItem()
and provide a specific item we want to extract.  This would extract just
the value if it is found, or an empty string otherwise.  The GetMetadataItem()
is an analog of the C++ GDALMajorObject::GetMetadataItem() method. 

\code
  Dim MDValue As String

  MDValue = ds.GetMetadataItem( "TIFF_DATETIME", vbNullString )
  if MDValue <> "" Then
    Print "Creation Date: " & MDValue
  End If
\endcode  

The GDALDataset::GetGeoTransform() method is used to get fetch the affine
transformation used to relate pixel/line locations on the image to 
georeferenced locations in the current coordinate system.  In the most common
case (image is not rotated or sheared) you can just report the origin 
(upper left corner) and pixel size from these values.   The method returns
0 on success or an error class if it fails, so we only use the return result
(placed into the Geotransform array) on success.

\code
  Dim Geotransform(6) As Double

  If ds.GetGeoTransform( Geotransform ) = 0 Then 
    If Geotransform(2) = 0 and Geotransform(4) = 0 Then
      Print "Origin: " & Geotransform(0) & "," & Geotransform(3)
      Print "Pixel Size: " & Geotransform(1) & "x" & (-1 * Geotransform(5))
    End If
  End If
\endcode

The coordinate system can be fetched using the GDALDataset::GetProjectionRef()
analog, GDALDataset.GetProjection().  The returned string is in OpenGIS
Well Known Text format.   A later example will show how to use an 
OGRSpatialReference object to reformat the WKT into more readable format
and make other use of it. 

\code
  Dim WKT As String

  WKT = ds.GetProjection()
  If Len(WKT) > 0 Then
    Print "Projection: " & WKT
  End If
\endcode

GDALDataset objects have one or more raster bands associated with them.
GDALRasterBand objects can have metadata (accessed the same as on the
GDALDataset) as well as an array of pixel values, and various specialized
metadata items like data type, color interpretation, offset/scale.   Here
we report a few of the items.  

First we loop over all the bands, fetching a band object for each band
and report the band number, and block size. 

\code
  For i = 1 To ds.BandCount
    Dim band As GDALRasterBand
           
    Set band = ds.GetRasterBand(i)
    Print "Band " & i & " BlockSize: " & band.BlockXSize & "x" & band.BlockYSize
\endcode

The GDALRasterBand has a DataType property which has the value returned
by the C++ method GDALRasterBand::GetRasterDataType().  The returned value
is an integer, but may be compared to the predefined constants GDAL.GDT_Byte, 
GDAL.GDT_UInt16, GDAL.GDT_Int16, GDAL.GDT_UInt32, GDAL.GDT_Int32, 
GDAL.GDT_Float32, GDAL.GDT_Float64, GDAL.GDT_CInt16, GDAL.GDT_CInt32,
GDAL.GDT_CFloat32 and GDAL.GDT_CFloat64.   In this case we use the 
GDAL.GetDataTypeName() method to convert the data type into a name we
can show the user. 

\code
    Print "     DataType=" & GDAL.GetDataTypeName(band.DataType) _
\endcode

We also report the offset, scale, minimum and maximum for the band. 

\code
    Print " Offset=" & band.GetOffset() & " Scale=" & band.GetScale() _
        & " Min=" & band.GetMinimum() & " Max=" & band.GetMaximum()
\endcode

GDALRasterBands can also have GDALColorTable objects associated with them.  
They are read with the GDALRasterBand::GetColorTable() analog in VB6.  
Individual RGBA entries should be read into a 4 Integer array.

\code
    Dim ct As GDALColorTable
    Set ct = band.GetColorTable()
    If ct.IsValid() Then
      Dim CEntry(4) As Integer
      Print "    Has Color Table, " & ct.EntryCount & " entries"
      For iColor = 0 To ct.EntryCount - 1
        Call ct.GetColorEntryAsRGB(iColor, CEntry)
        Print "      " & iColor & ": " & CEntry(0) & "," & CEntry(1) & "," & CEntry(2) & "," & CEntry(3)
      Next iColor
    End If
\endcode

But of course, the most important contents of a GDAL file is the raster
pixel values themselves.  The C++ GDALRasterBand::RasterIO() method is
provided in a somewhat simplified form.  A predimensioned 1D or 2D 
array of type Byte, Int, Long, Float or Double is passed to the RasterIO()
method along with the band and window to be read.  Internally the "buffer
size" and datatype is extracted from the dimensions of the passed in buffer.

This example dimensions the RawData array to be the size of one scanline
of data (XSize x 1) and reads the first whole scanline of data from the
file, but only prints out the second and tenth values (since the buffer
indexes are zero based). 

\code
    Dim err As Long
    Dim RawData() As Double
    ReDim RawData(ds.XSize) As Double

    err = band.RasterIO(GDAL.GF_Read, 0, 0, ds.XSize, 1, RawData)
    if err = 0 Then
      Print "    Data: " & RawData(1) & " " & RawData(9)
    End If
\endcode

Finally, when done accessing a GDALDataset we can explicitly close
it using the CloseDS() method, or just let it fall out of scope in which
case it will be closed automatically. 

\code
    Call ds.CloseDS()
\endcode

\section TutorialCreate Tutorial - Creating Files

Next we address creating a new file from an existing file.  To create a
new file, you have to select a GDALDriver to do the creating.  The GDALDriver
is essentially an object representing a file format.   We fetch it with the
GetDriverByName() call from the GDAL module using the driver name.  

\code
    Dim Drv As GDALDriver

    Call GDAL.AllRegister
    Drv = GDALCore.GetDriverByName( "GTiff" )
    If Not Drv.IsValid() Then
        Call MsgBox( "GTiff driver not found " )
	Exit Sub
    End If
\endcode

You could get a list of registered drivers, and identify which support
creation something like this:

\code
    drvCount = GDAL.GetDriverCount
    For drvIndex = 0 To drvCount - 1
        Set Drv = GDAL.GetDriver(drvIndex)
        If Drv.GetMetadataItem(GDAL.DCAP_CREATE, "") = "YES" _
            Or Drv.GetMetadataItem(GDAL.DCAP_CREATECOPY, "") = "YES" Then
            xMsg = " (Read/Write)"
        Else
            xMsg = " (ReadOnly)"
        End If
              
        Print Drv.GetShortName() & ": " & Drv.GetMetadataItem(GDAL.DMD_LONGNAME, "") & xMsg
    Next drvIndex
\endcode

Once we have the driver object, the simplest way of creating a new file
is to use CreateCopy().  This tries to create a copy of the input file
in the new format.  A complete segment (without any error checking)
would look like the following.  The CreateCopy() method corresponds to the
C++ method GDALDriver::CreateCopy().  The VB6 implementation does not 
support the use of progress callbacks. 

\code
    Dim Drv As GDALDriver
    Dim SrcDS As GDALDataset, DstDS As GDALDataset

    Call GDAL.AllRegister
    Set Drv = GDALCore.GetDriverByName( "GTiff" )

    Set SrcDS = GDAL.Open( "in.tif", GDAL.GA_ReadOnly )
    Set DstDS = Drv.CreateCopy( "out.tif", SrcDS, True, Nothing )
\endcode

This is nice and simple, but sometimes we need to create a file with more
detailed control.  So, next we show how to create a file and then copy 
pieces of data to it "manually".   The GDALDriver::Create() analog is 
Create().  

\code
    Set DstDS = Drv.Create("out.tif", SrcDS.XSize, SrcDS.YSize, _
                           SrcDS.BandCount, GDAL.GDT_Byte, Nothing)
\endcode

In some cases we may want to provide some creation options,
which is demonstrated here.  Creation options (like metadata set through the
SetMetadata() method) are arrays of Strings.  

\code
    Dim CreateOptions(1) As String

    CreateOptions(1) = "PHOTOMETRIC=MINISWHITE"
    Set DstDS = Drv.Create("out.tif", SrcDS.XSize, SrcDS.YSize, _
                           SrcDS.BandCount, GDAL.GDT_Byte, CreateOptions)
\endcode

When copying the GeoTransform, we take care to check that reading the
geotransform actually worked.  Most methods which return CPLErr in C++
also return it in VB6.  A return value of 0 will indicate success, and non-zero
is failure. 

\code
    Dim err As Long
    Dim gt(6) As Double

    err = SrcDS.GetGeoTransform(gt)
    If err = 0 Then
        Call DstDS.SetGeoTransform(gt)
    End If
\endcode

Copy the projection.  Even if GetProjection() fails we get an empty string
which is safe enough to set on the target.   Similarly for metadata. 

\code
    Call DstDS.SetProjection(SrcDS.GetProjection())
    Call DstDS.SetMetadata(SrcDS.GetMetadata(""), "")
\endcode
    
Next we loop, processing bands, and copy some common data items.

\code
    For iBand = 1 To SrcDS.BandCount
        Dim SrcBand As GDALRasterBand, DstBand As GDALRasterBand
        
        Set SrcBand = SrcDS.GetRasterBand(iBand)
        Set DstBand = DstDS.GetRasterBand(iBand)
        
        Call DstBand.SetMetadata(SrcBand.GetMetadata(""), "")
        Call DstBand.SetOffset(SrcBand.GetOffset())
        Call DstBand.SetScale(SrcBand.GetScale())

        Dim NoDataValue As Double, Success As Long
        
        NoDataValue = SrcBand.GetNoDataValue(Success)
        If Success <> 0 Then
            Call DstBand.SetNoDataValue(NoDataValue)
        End If
\endcode

Then, if one is available, we copy the palette.

\code
        Dim ct As GDALColorTable
        Set ct = SrcBand.GetColorTable()
        If ct.IsValid() Then
            err = DstBand.SetColorTable(ct)
        End If
\endcode        

Finally, the meat and potatoes.  We copy the image data.  We do this one
scanline at a time so that we can support very large images without require
large amounts of RAM.   Here we use a Double buffer for the scanline, but
if we knew in advance the type of the image, we could dimension a buffer
of the appropriate type.  The RasterIO() method internally knows how to
convert pixel data types, so using Double ensures all data types (except
for complex) are properly preserved, though at the cost of some extra data
conversion internally.

\code
        Dim Scanline() As Double, iLine As Long
        ReDim Scanline(SrcDS.XSize) As Double

        ' Copy band raster data.
        For iLine = 0 To SrcDS.YSize - 1
            Call SrcBand.RasterIO(GDAL.GF_Read, 0, iLine, SrcDS.XSize, 1, _
				  Scanline)
            Call DstBand.RasterIO(GDAL.GF_Write, 0, iLine, SrcDS.XSize, 1, _
				  Scanline)
        Next iLine
\endcode

\section OSRTut Tutorial - Coordinate Systems and Reprojection

The GDAL VB6 bindings also include limited support for use of the
OGRSpatialReference and OGRCoordinateTransformation classes.  The 
OGRSpatialReference represents a coordinate system and can be used to 
parse, manipulate and form WKT strings, such as those returned by the
GDALDataset.GetProjection() method.   The OGRCoordinateTransformation 
class provides a way of reprojecting between two coordinate systems. 

The following example shows how to report the corners of an image in
georeferenced and geographic (lat/long) coordinates.   First, we open
the file, and read the geotransform. 

\code
    Dim ds As GDALDataset
    
    Call GDALCore.GDALAllRegister
    Set ds = GDAL.OpenDS(FileDlg.Filename, GDAL.GA_ReadOnly)
    
    If ds.IsValid() Then
        Dim Geotransform(6) As Double
        
        Call ds.GetGeoTransform(Geotransform)
\endcode

Next, we fetch the coordinate system, and if it is non-empty we try to 
instantiate an OGRSpatialReference from it. 

\code        
        ' report projection in pretty format.
        Dim WKT As String
        Dim srs As New OGRSpatialReference
        Dim latlong_srs As OGRSpatialReference
        Dim ct As New OGRCoordinateTransformation

        WKT = ds.GetProjection()
        If Len(WKT) > 0 Then
            Print "Projection: "
            Call srs.SetFromUserInput(WKT)

\endcode

If the coordinate system is projected it will have a PROJECTION node.  In
that case we build a new coordinate system which is the corresponding 
geographic coordinate system.  So for instance if the "srs" was UTM 11 WGS84
then it's corresponding geographic coordinate system would just be WGS84.
Once we have these two coordinate systems, we build a transformer to convert
between them. 

\code
            If srs.GetAttrValue("PROJECTION", 0) <> "" Then
                Set latlong_srs = srs.CloneGeogCS()
                Set ct = GDAL.CreateCoordinateTransformation(srs, latlong_srs)
            End If
        End If
\endcode

Next we call a helper function to report each corner, and the center. 
We pass in the name of the corner, the pixel/line location at the corner,
and the geotransform and transformer object.

\code
        Call ReportCorner("Top Left      ", 0, 0, _
                          Geotransform, ct)
        Call ReportCorner("Top Right     ", ds.XSize, 0, _
                          Geotransform, ct)
        Call ReportCorner("Bottom Left   ", 0, ds.YSize, _
                          Geotransform, ct)
        Call ReportCorner("Bottom Right  ", ds.XSize, ds.YSize, _
                          Geotransform, ct)
        Call ReportCorner("Center        ", ds.XSize / 2#, ds.YSize / 2#, _
                          Geotransform, ct)
\endcode

The ReportCorner subroutine starts by computing the corresponding 
georeferenced x and y location using the pixel/line coordinates and the
geotransform. 

\code
Private Sub ReportCorner(CornerName As String, pixel As Double, line As Double, _
                         gt() As Double, ct As OGRCoordinateTransformation)
                             
    Dim geox As Double, geoy As Double
    
    geox = gt(0) + pixel * gt(1) + line * gt(2)
    geoy = gt(3) + pixel * gt(4) + line * gt(5)
\endcode

Next, if we have a transformer, we use it to compute a corresponding 
latitude and longitude.

\code
    Dim longitude As Double, latitude As Double, Z As Double
    Dim latlong_valid As Boolean

    latlong_valid = False
    
    If ct.IsValid() Then
        Z = 0
        longitude = geox
        latitude = geoy
        latlong_valid = ct.TransformOne(longitude, latitude, Z)
    End If
\endcode

Then we report the corner location in georeferenced, and if we have it
geographic coordinates.  

\code                         
    If latlong_valid Then
        Print CornerName & geox & "," & geoy & "    " & longitude & "," & latitude
    Else
        Print CornerName & geox & "," & geoy
    End If
End Sub
\endcode

\htmlonly
<p>
$Id: vb6_tutorial.dox 13528 2008-01-14 19:37:42Z warmerdam $
</p>
\endhtmlonly

*/
