#ifndef DOXYGEN_SKIP
/* $Id: warptut.dox 33134 2016-01-23 23:10:03Z rouault $ */
#endif /* DOXYGEN_SKIP */

/*!
\page warptut GDAL Warp API Tutorial

\section warptut_overview Overview

The GDAL Warp API (declared in gdalwarper.h) provides services for high
performance image warping using application provided geometric transformation
functions (GDALTransformerFunc), a variety of resampling kernels, and 
various masking options.  Files much larger than can be held in memory can
be warped.

This tutorial demonstrates how to implement an application using the Warp API.
It assumes implementation in C++ as C and Python bindings are incomplete for
the Warp API.  It also assumes familiarity with the 
<a href="gdal_datamodel.html">GDAL Data Model</a>, and the general GDAL API.

Applications normally perform a warp by initializing a GDALWarpOptions 
structure with the options to be utilized, instantiating a GDALWarpOperation
based on these options, and then invoking the 
GDALWarpOperation::ChunkAndWarpImage() method to perform the warp options
internally using the GDALWarpKernel class.

\section warptut_simple A Simple Reprojection Case

First we will construct a relatively simple example for reprojecting an image,
assuming an appropriate output file already exists, and with minimal error
checking.

\code
#include "gdalwarper.h"

int main()
{
    GDALDatasetH  hSrcDS, hDstDS;

    // Open input and output files. 

    GDALAllRegister();

    hSrcDS = GDALOpen( "in.tif", GA_ReadOnly );
    hDstDS = GDALOpen( "out.tif", GA_Update );

    // Setup warp options. 
    
    GDALWarpOptions *psWarpOptions = GDALCreateWarpOptions();

    psWarpOptions->hSrcDS = hSrcDS;
    psWarpOptions->hDstDS = hDstDS;

    psWarpOptions->nBandCount = 1;
    psWarpOptions->panSrcBands = 
	(int *) CPLMalloc(sizeof(int) * psWarpOptions->nBandCount );
    psWarpOptions->panSrcBands[0] = 1;
    psWarpOptions->panDstBands = 
	(int *) CPLMalloc(sizeof(int) * psWarpOptions->nBandCount );
    psWarpOptions->panDstBands[0] = 1;

    psWarpOptions->pfnProgress = GDALTermProgress;   

    // Establish reprojection transformer. 

    psWarpOptions->pTransformerArg = 
        GDALCreateGenImgProjTransformer( hSrcDS, 
                                         GDALGetProjectionRef(hSrcDS), 
                                         hDstDS,
                                         GDALGetProjectionRef(hDstDS), 
                                         FALSE, 0.0, 1 );
    psWarpOptions->pfnTransformer = GDALGenImgProjTransform;

    // Initialize and execute the warp operation. 

    GDALWarpOperation oOperation;

    oOperation.Initialize( psWarpOptions );
    oOperation.ChunkAndWarpImage( 0, 0, 
		                  GDALGetRasterXSize( hDstDS ), 
			          GDALGetRasterYSize( hDstDS ) );

    GDALDestroyGenImgProjTransformer( psWarpOptions->pTransformerArg );
    GDALDestroyWarpOptions( psWarpOptions );

    GDALClose( hDstDS );
    GDALClose( hSrcDS );

    return 0;
}
\endcode

This example opens the existing input and output files (in.tif and out.tif).
A GDALWarpOptions structure is allocated (GDALCreateWarpOptions() sets lots
of sensible defaults for stuff, always use it for defaulting things), and
the input and output file handles, and band lists are set.  The panSrcBands and
panDstBands lists are dynamically allocated here and will be free automatically
by GDALDestroyWarpOptions().  The simple terminal output progress monitor
(GDALTermProgress) is installed for reporting completion progress to the user.

GDALCreateGenImgProjTransformer() is used to initialize the reprojection 
transformation between the source and destination images.  We assume that
they already have reasonable bounds and coordinate systems set.  Use of
GCPs is disabled. 

Once the options structure is ready, a GDALWarpOperation is instantiated using
them, and the warp actually performed with 
GDALWarpOperation::ChunkAndWarpImage().  Then the transformer, warp options
and datasets are cleaned up. 

Normally error check would be needed after opening files, setting up the 
reprojection transformer (returns NULL on failure), and initializing the
warp.

\section warptut_options Other Warping Options

The GDALWarpOptions structures contains a number of items that can be set
to control warping behavior.  A few of particular interest are:

<ol>

<li> GDALWarpOptions::dfWarpMemoryLimit - Set the maximum amount of memory to 
be used by the GDALWarpOperation when selecting a size of image chunk to
operate on.  The value is in bytes, and the default is likely to be 
conservative (small).  Increasing the chunk size can help substantially in
some situations but care should be taken to ensure that this size, plus the
GDAL cache size plus the working set of GDAL, your application and the
operating system are less than the size of RAM or else excessive swapping is
likely to interfere with performance.  On a system with 256MB of RAM, a value
of at least 64MB (roughly 64000000 bytes) is reasonable.  Note that this
value does <b>not</b> include the memory used by GDAL for low level block
caching.

<li> GDALWarpOpations::eResampleAlg - One of GRA_NearestNeighbour (the default,
and fastest), GRA_Bilinear (2x2 bilinear resampling) or GRA_Cubic.  The
GRA_NearestNeighbour type should generally be used for thematic or color mapped 
images.  The other resampling types may give better results for thematic 
images, especially when substantially changing resolution. 

<li> GDALWarpOptions::padfSrcNoDataReal - This array (one entry per band
being processed) may be setup with a "nodata" value for each band if you wish
to avoid having pixels of some background value copied to the destination
image. 

<li><a name="#warpoptions"></a> GDALWarpOptions::papszWarpOptions - This is
a string list of NAME=VALUE options passed to the warper.  See the 
GDALWarpOptions::papszWarpOptions docs for all options.  Supported values 
include:

<ul>
<li> INIT_DEST=[value] or INIT_DEST=NO_DATA: This option forces the 
 destination image to be initialized to the indicated value (for all bands)
 or indicates that it should be initialized to the NO_DATA value in
 padfDstNoDataReal/padfDstNoDataImag.  If this value isn't set the
 destination image will be read and the source warp overlaid on it.

<li> WRITE_FLUSH=YES/NO: This option forces a flush to disk of data after
 each chunk is processed.  In some cases this helps ensure a serial 
 writing of the output data otherwise a block of data may be written to disk
 each time a block of data is read for the input buffer resulting in a lot
 of extra seeking around the disk, and reduced IO throughput.  The default
 at this time is NO.
</ul>

</ol>

\section warptut_output Creating the Output File

In the previous case an appropriate output file was already assumed to 
exist.  Now we will go through a case where a new file with appropriate
bounds in a new coordinate system is created.  This operation doesn't
relate specifically to the warp API.  It is just using the transformation API.

\code
#include "gdalwarper.h"
#include "ogr_spatialref.h"

...

    GDALDriverH hDriver;
    GDALDataType eDT;
    GDALDatasetH hDstDS;
    GDALDatasetH hSrcDS;

    // Open the source file. 

    hSrcDS = GDALOpen( "in.tif", GA_ReadOnly );
    CPLAssert( hSrcDS != NULL );
    
    // Create output with same datatype as first input band. 

    eDT = GDALGetRasterDataType(GDALGetRasterBand(hSrcDS,1));

    // Get output driver (GeoTIFF format)

    hDriver = GDALGetDriverByName( "GTiff" );
    CPLAssert( hDriver != NULL );

    // Get Source coordinate system. 

    const char *pszSrcWKT, *pszDstWKT = NULL;

    pszSrcWKT = GDALGetProjectionRef( hSrcDS );
    CPLAssert( pszSrcWKT != NULL && strlen(pszSrcWKT) > 0 );

    // Setup output coordinate system that is UTM 11 WGS84. 

    OGRSpatialReference oSRS;

    oSRS.SetUTM( 11, TRUE );
    oSRS.SetWellKnownGeogCS( "WGS84" );

    oSRS.exportToWkt( &pszDstWKT );

    // Create a transformer that maps from source pixel/line coordinates
    // to destination georeferenced coordinates (not destination 
    // pixel line).  We do that by omitting the destination dataset
    // handle (setting it to NULL). 

    void *hTransformArg;

    hTransformArg = 
        GDALCreateGenImgProjTransformer( hSrcDS, pszSrcWKT, NULL, pszDstWKT, 
                                         FALSE, 0, 1 );
    CPLAssert( hTransformArg != NULL );

    // Get approximate output georeferenced bounds and resolution for file. 

    double adfDstGeoTransform[6];
    int nPixels=0, nLines=0;
    CPLErr eErr;

    eErr = GDALSuggestedWarpOutput( hSrcDS, 
				    GDALGenImgProjTransform, hTransformArg, 
                                    adfDstGeoTransform, &nPixels, &nLines );
    CPLAssert( eErr == CE_None );

    GDALDestroyGenImgProjTransformer( hTransformArg );

    // Create the output file.  

    hDstDS = GDALCreate( hDriver, "out.tif", nPixels, nLines, 
                         GDALGetRasterCount(hSrcDS), eDT, NULL );
    
    CPLAssert( hDstDS != NULL );

    // Write out the projection definition. 

    GDALSetProjection( hDstDS, pszDstWKT );
    GDALSetGeoTransform( hDstDS, adfDstGeoTransform );

    // Copy the color table, if required.

    GDALColorTableH hCT;

    hCT = GDALGetRasterColorTable( GDALGetRasterBand(hSrcDS,1) );
    if( hCT != NULL )
        GDALSetRasterColorTable( GDALGetRasterBand(hDstDS,1), hCT );

    ... proceed with warp as before ...
\endcode

Some notes on this logic:

<ul>

<li> We need to create the transformer to output coordinates such that the
output of the transformer is georeferenced, not pixel line coordinates since
we use the transformer to map pixels around the source image into destination
georeferenced coordinates.  

<li> The GDALSuggestedWarpOutput() function will return an adfDstGeoTransform,
nPixels and nLines that describes an output image size and georeferenced 
extents that should hold all pixels from the source image.  The resolution
is intended to be comparable to the source, but the output pixels are always
square regardless of the shape of input pixels. 

<li> The warper requires an output file in a format that can be "randomly"
written to.  This generally limits things to uncompressed formats that
have an implementation of the Create() method (as opposed to CreateCopy()). 
To warp to compressed formats, or CreateCopy() style formats it is necessary
to produce a full temporary copy of the image in a better behaved format, and
then CreateCopy() it to the desired final format. 

<li> The Warp API copies only pixels.  All color maps, georeferencing and
other metadata must be copied to the destination by the application.  

</ul>

\section warptut_performance Performance Optimization

There are a number of things that can be done to optimize the performance
of the warp API.

<ol>

<li> Increase the amount of memory available for the Warp API chunking so that
larger chunks can be operated on at a time.  This is the 
GDALWarpOptions::dfWarpMemoryLimit parameter.  In theory the larger the chunk
size operated on the more efficient the I/O strategy, and the more efficient
the approximated transformation will be.   However, the sum of the warp 
memory and the GDAL cache should be less than RAM size, likely around 2/3
of RAM size.

<li> Increase the amount of memory for GDAL caching.  This is especially 
important when working with very large input and output images that are 
scanline oriented.  If all the input or output scanlines have to be re-read
for each chunk they intersect performance may degrade greatly.  Use 
GDALSetCacheMax() to control the amount of memory available for caching
within GDAL. 

<li> Use an approximated transformation instead of exact reprojection for
each pixel to be transformed.  This code illustrates how an approximated
transformation could be created based on a reprojection transformation, but
with a given error threshold (dfErrorThreshold in output pixels). 

\code
        hTransformArg = 
            GDALCreateApproxTransformer( GDALGenImgProjTransform, 
                                         hGenImgProjArg, dfErrorThreshold );
        pfnTransformer = GDALApproxTransform;
\endcode

<li> When writing to a blank output file, use the INIT_DEST option in the
GDALWarpOptions::papszWarpOptions to cause the output chunks to be
initialized to a fixed value, instead of being read from the output.  This
can substantially reduce unnecessary IO work. 

<li> Use tiled input and output formats.  Tiled formats allow a given
chunk of source and destination imagery to be accessed without having to 
touch a great deal of extra image data.  Large scanline oriented files 
can result in a great deal of wasted extra IO.

<li> Process all bands in one call.  This ensures the transformation 
calculations don't have to be performed for each band. 

<li> Use the GDALWarpOperation::ChunkAndWarpMulti() method instead of
GDALWarpOperation::ChunkAndWarpImage().  It uses a separate thread for the
IO and the actual image warp operation allowing more effective use of CPU
and IO bandwidth.  For this to work GDAL needs to have been built with
multi-threading support (default on Win32, default on Unix since GDAL 1.8.0,
for previous versions --with-threads was required in configure).

<li> The resampling kernels vary is work required from nearest neighbour
being least, then bilinear then cubic.  Don't use a more complex resampling
kernel than needed. 

<li> Avoid use of esoteric masking options so that special simplified 
logic case be used for common special cases.  For instance, nearest 
neighbour resampling with no masking on 8bit data is highly optimized
compared to the general case.

</ol>

\section warptut_other_opts Other Masking Options

The GDALWarpOptions include a bunch of esoteric masking capabilities, for
validity masks, and density masks on input and output.  Some of these are
not yet implemented and others are implemented but poorly tested.  Other
than per-band validity masks it is advised that these features be used with
caution at this time. 

\htmlonly
<p>
$Id: warptut.dox 33134 2016-01-23 23:10:03Z rouault $
</p>
\endhtmlonly

*/
