GDAL

- Main Page
- Related Pages
- Classes
- Files
- Download
- Issue Tracker

gdalsrsinfo

Lists info about a given SRS in number of formats (WKT, PROJ.4, etc.)

# SYNOPSIS

    Usage: gdalsrsinfo [options] srs_def

    srs_def may be the filename of a dataset supported by GDAL/OGR from which to extract SRS information
    OR any of the usual GDAL/OGR forms (complete WKT, PROJ.4, EPSG:n or a file containing the SRS)

    Options:
       [--help-general] [-h]  Show help and exit
       [-p]                   Pretty-print where applicable (e.g. WKT)
       [-V]                   Validate SRS
       [-e]                   Search for EPSG number(s) corresponding to SRS
       [-o out_type]          Output type { default, all, wkt_all, proj4,
                                            wkt, wkt_simple, wkt_noct, wkt_esri,
                                            mapinfo, xml }

# DESCRIPTION

The gdalsrsinfo utility reports information about a given SRS from one of the following:

- The filename of a dataset supported by GDAL/OGR which contains SRS information
- Any of the usual GDAL/OGR forms (complete WKT, PROJ.4, EPSG:n or a file containing the SRS)

Output types:

- default proj4 and wkt (default option)
- all all options available
- wkt_all all wkt options available
- proj4 PROJ.4 string
- wkt OGC WKT format (full)
- wkt_simple OGC WKT (simplified)
- wkt_noct OGC WKT (without OGC CT params)
- wkt_esri ESRI WKT format
- mapinfo Mapinfo style CoordSys format
- xml XML format (GML based)

# EXAMPLE

    $  gdalsrsinfo   "EPSG:4326"

    PROJ.4 : '+proj=longlat +datum=WGS84 +no_defs '

    OGC WKT :
    GEOGCS["WGS 84",
        DATUM["WGS_1984",
            SPHEROID["WGS 84",6378137,298.257223563,
                AUTHORITY["EPSG","7030"]],
            AUTHORITY["EPSG","6326"]],
        PRIMEM["Greenwich",0,
            AUTHORITY["EPSG","8901"]],
        UNIT["degree",0.0174532925199433,
            AUTHORITY["EPSG","9122"]],
        AUTHORITY["EPSG","4326"]]

    $ gdalsrsinfo -o proj4 osr/data/lcc_esri.prj
    '+proj=lcc +lat_1=34.33333333333334 +lat_2=36.16666666666666 +lat_0=33.75 +lon_0=-79 +x_0=609601.22 +y_0=0 +datum=NAD83 +units=m +no_defs '

    $ gdalsrsinfo -o proj4 landsat.tif
    PROJ.4 : '+proj=utm +zone=19 +south +datum=WGS84 +units=m +no_defs '

    $ gdalsrsinfo  -o wkt -p  "EPSG:32722"

    PROJCS["WGS 84 / UTM zone 22S",
        GEOGCS["WGS 84",
            DATUM["WGS_1984",
                SPHEROID["WGS 84",6378137,298.257223563,
                    AUTHORITY["EPSG","7030"]],
                AUTHORITY["EPSG","6326"]],
            PRIMEM["Greenwich",0,
                AUTHORITY["EPSG","8901"]],
            UNIT["degree",0.0174532925199433,
                AUTHORITY["EPSG","9122"]],
            AUTHORITY["EPSG","4326"]],
        PROJECTION["Transverse_Mercator"],
        PARAMETER["latitude_of_origin",0],
        PARAMETER["central_meridian",-51],
        PARAMETER["scale_factor",0.9996],
        PARAMETER["false_easting",500000],
        PARAMETER["false_northing",10000000],
        UNIT["metre",1,
            AUTHORITY["EPSG","9001"]],
        AXIS["Easting",EAST],
        AXIS["Northing",NORTH],
        AUTHORITY["EPSG","32722"]]

    $ gdalsrsinfo  -o wkt_all  "EPSG:4618"

    OGC WKT :
    GEOGCS["SAD69",
        DATUM["South_American_Datum_1969",
            SPHEROID["GRS 1967 Modified",6378160,298.25,
                AUTHORITY["EPSG","7050"]],
            TOWGS84[-57,1,-41,0,0,0,0],
            AUTHORITY["EPSG","6618"]],
        PRIMEM["Greenwich",0,
            AUTHORITY["EPSG","8901"]],
        UNIT["degree",0.0174532925199433,
            AUTHORITY["EPSG","9122"]],
        AUTHORITY["EPSG","4618"]]

    OGC WKT (simple) :
    GEOGCS["SAD69",
        DATUM["South_American_Datum_1969",
            SPHEROID["GRS 1967 Modified",6378160,298.25],
            TOWGS84[-57,1,-41,0,0,0,0]],
        PRIMEM["Greenwich",0],
        UNIT["degree",0.0174532925199433]]

    OGC WKT (no CT) :
    GEOGCS["SAD69",
        DATUM["South_American_Datum_1969",
            SPHEROID["GRS 1967 Modified",6378160,298.25]],
        PRIMEM["Greenwich",0],
        UNIT["degree",0.0174532925199433]]

    ESRI WKT :
    GEOGCS["SAD69",
        DATUM["D_South_American_1969",
            SPHEROID["GRS_1967_Truncated",6378160,298.25]],
        PRIMEM["Greenwich",0],
        UNIT["Degree",0.017453292519943295]]

Generated for GDAL by 1.8.8.