# `gdal raster`

Added in version 3.11.

Entry point for raster commands

## Synopsis

    Usage: gdal raster <SUBCOMMAND> [OPTIONS]
    where <SUBCOMMAND> is one of:
      - aspect:       Generate an aspect map
      - calc:         Perform raster algebra
      - clean-collar: Clean the collar of a raster dataset, removing noise.
      - clip:         Clip a raster dataset.
      - color-map:    Generate a RGB or RGBA dataset from a single band, using a color map
      - contour:      Creates a vector contour from a raster elevation model (DEM).
      - convert:      Convert a raster dataset.
      - create:       Create a new raster dataset.
      - edit:         Edit a raster dataset.
      - fill-nodata:  Fill nodata raster regions by interpolation from edges.
      - footprint:    Compute the footprint of a raster dataset.
      - hillshade:    Generate a shaded relief map
      - index:        Create a vector index of raster datasets.
      - info:         Return information on a raster dataset.
      - mosaic:       Build a mosaic, either virtual (VRT) or materialized.
      - overview:     Manage overviews of a raster dataset.
      - pipeline:     Process a raster dataset.
      - pixel-info:   Return information on a pixel of a raster dataset.
      - polygonize:   Create a polygon feature dataset from a raster band.
      - reclassify:   Reclassify values in a raster dataset
      - reproject:    Reproject a raster dataset.
      - resize:       Resize a raster dataset without changing the georeferenced extents.
      - roughness:    Generate a roughness map
      - scale:        Scale the values of the bands of a raster dataset.
      - select:       Select a subset of bands from a raster dataset.
      - set-type:     Modify the data type of bands of a raster dataset.
      - sieve:        Remove small polygons from a raster dataset.
      - slope:        Generate a slope map
      - stack:        Combine together input bands into a multi-band output, either virtual (VRT) or materialized.
      - tile:         Generate tiles in separate files from a raster dataset.
      - tpi:          Generate a Topographic Position Index (TPI) map
      - tri:          Generate a Terrain Ruggedness Index (TRI) map
      - unscale:      Convert scaled values of a raster dataset into unscaled values.
      - viewshed:     Compute the viewshed of a raster dataset.

    Common Options:
      -h, --help              Display help message and exit
      --json-usage            Display usage as JSON document and exit
      --config <KEY>=<VALUE>  Configuration option [may be repeated]

    Options:
      --drivers               Display raster driver list as JSON document

## Available sub-commands

- gdal raster info

- gdal raster aspect

- gdal raster calc

- gdal raster clean-collar

- gdal raster clip

- gdal raster color-map

- gdal raster convert

- gdal raster create

- gdal raster footprint

- gdal raster fill-nodata

- gdal raster hillshade

- gdal raster index

- gdal raster mosaic

- gdal raster overview

- gdal raster pipeline

- gdal raster pixel-info

- gdal raster polygonize

- gdal raster reproject

- gdal raster resize

- gdal raster roughness

- gdal raster scale

- gdal raster select

- gdal raster sieve

- gdal raster slope

- gdal raster stack

- gdal raster tile

- gdal raster tpi

- gdal raster tri

- gdal raster unscale

- gdal raster viewshed

## Examples

### Example 1: Getting information on the file `utm.tif` (with JSON output)

    $ gdal raster info utm.tif

### Example 2: Converting file `utm.tif` to GeoPackage raster

    $ gdal raster convert utm.tif utm.gpkg

### Example 3: Getting the list of raster drivers (with JSON output)

    $ gdal raster --drivers