# `gdal vector`

Added in version 3.11.

Entry point for vector commands

## Synopsis

    Usage: gdal vector <SUBCOMMAND> [OPTIONS]
    where <SUBCOMMAND> is one of:
      - buffer:              Compute a buffer around geometries of a vector dataset.
      - check-coverage:      Check a polygon coverage for validity
      - check-geometry:      Check a dataset for invalid geometries
      - clean-coverage:      Alter polygon boundaries to make shared edges identical, removing gaps and overlaps
      - clip:                Clip a vector dataset.
      - concat:              Concatenate vector datasets.
      - convert:             Convert a vector dataset.
      - edit:                Edit metadata of a vector dataset.
      - explode-collections: Explode geometries of type collection of a vector dataset.
      - filter:              Filter a vector dataset.
      - grid:                Create a regular grid from scattered points.
      - index:               Create a vector index of vector datasets.
      - info:                Return information on a vector dataset.
      - layer-algebra:       Perform algebraic operation between 2 layers.
      - make-point:          Create point geometries from attribute fields
      - make-valid:          Fix validity of geometries of a vector dataset.
      - partition:           Partition a vector dataset into multiple files.
      - pipeline:            Process a vector dataset applying several steps.
      - rasterize:           Burns vector geometries into a raster.
      - reproject:           Reproject a vector dataset.
      - segmentize:          Segmentize geometries of a vector dataset.
      - select:              Select a subset of fields from a vector dataset.
      - set-field-type:      Modify the type of a field of a vector dataset.
      - set-geom-type:       Modify the geometry type of a vector dataset.
      - simplify:            Simplify geometries of a vector dataset.
      - simplify-coverage:   Simplify shared boundaries of a polygonal vector dataset.
      - sql:                 Apply SQL statement(s) to a dataset.
      - swap-xy:             Swap X and Y coordinates of geometries of a vector dataset.

    Common Options:
      -h, --help              Display help message and exit
      --json-usage            Display usage as JSON document and exit
      --config <KEY>=<VALUE>  Configuration option [may be repeated]

    Options:
      --drivers               Display vector driver list as JSON document and exit

## Available sub-commands

- gdal vector clip

- gdal vector concat

- gdal vector convert

- gdal vector edit

- gdal vector filter

- gdal vector index

- gdal vector info

- gdal vector layer-algebra

- gdal vector partition

- gdal vector pipeline

- gdal vector rasterize

- gdal vector reproject

- gdal vector select

- gdal vector set-field-type

- gdal vector set-geom-type

- gdal vector sql

## Examples

### Example 1: Getting information on the file `poly.gpkg` (with text output)

    $ gdal vector info poly.gpkg

### Example 2: Converting file `poly.gpkg` to Esri File Geodatabase

    $ gdal vector convert --format=OpenFileGDB poly.gpkg poly.gdb