# `gdal raster convert`

Added in version 3.11.

Convert a raster dataset.

## Synopsis

    Usage: gdal raster convert [OPTIONS] <INPUT> <OUTPUT>

    Convert a raster dataset.

    Positional arguments:
      -i, --input <INPUT>                                  Input raster datasets [required]
      -o, --output <OUTPUT>                                Output raster dataset [required]

    Common Options:
      -h, --help                                           Display help message and exit
      --json-usage                                         Display usage as JSON document and exit
      --config <KEY>=<VALUE>                               Configuration option [may be repeated]
      -q, --quiet                                          Quiet mode (no progress bar)

    Options:
      -f, --of, --format, --output-format <OUTPUT-FORMAT>  Output format ("GDALG" allowed)
      --co, --creation-option <KEY>=<VALUE>                Creation option [may be repeated]
      --overwrite                                          Whether overwriting existing output is allowed
                                                           Mutually exclusive with --append
      --append                                             Append as a subdataset to existing output
                                                           Mutually exclusive with --overwrite

    Advanced Options:
      --if, --input-format <INPUT-FORMAT>                  Input formats [may be repeated]
      --oo, --open-option <KEY>=<VALUE>                    Open options [may be repeated]

## Description

gdal raster convert can be used to convert raster data between different formats.

The following options are available:

### Standard options

-f, --of, --format, --output-format <OUTPUT-FORMAT>

  Which output raster format to use. Allowed values may be given by `gdal --formats | grep raster | grep rw | sort`

--co, --creation-option <NAME>=<VALUE>

  Many formats have one or more optional creation options that can be used to control particulars about the file created. For instance, the GeoTIFF driver supports creation options to control compression, and whether the file should be tiled.

  May be repeated.

  The creation options available vary by format driver, and some simple formats have no creation options at all. A list of options supported for a format can be listed with the --formats command line option but the documentation for the format is the definitive source of information on driver creation options. See Raster drivers format specific documentation for legal creation options for each format.

--overwrite

  Allow program to overwrite existing target file or dataset. Otherwise, by default, gdal errors out if the target file or dataset already exists.

--append

  Append input raster as a new subdataset to existing output file. Only works with drivers that support adding subdatasets such as GTiff -- GeoTIFF File Format and GPKG -- GeoPackage raster

### Advanced options

--oo, --open-option <NAME>=<VALUE>

  Dataset open option (format specific).

  May be repeated.

--if, --input-format <format>

  Format/driver name to be attempted to open the input file(s). It is generally not necessary to specify it, but it can be used to skip automatic driver detection, when it fails to select the appropriate driver. This option can be repeated several times to specify several candidate drivers. Note that it does not force those drivers to open the dataset. In particular, some drivers have requirements on file extensions.

  May be repeated.

## Examples

### Example 1: Converting file `utm.tif` to a cloud-optimized GeoTIFF using JPEG compression

    $ gdal raster convert --format=COG --co COMPRESS=JPEG utm.tif utm_cog.tif

### Example 2: Converting file `utm.tif` to GeoPackage raster

    $ gdal raster convert utm.tif utm.gpkg