# OGR WCTS Interactive Form

Action:

Enter the source and destination Coordinate Reference Systems (CRS) as EPSG PCS or GCS codes. Some examples are:

- 4326: Lat/Long WGS84
- 4269: Lat/Long NAD83
- 4267: Lat/Long NAD27
- 32611: UTM 11 WGS84
- 26911: UTM 11 NAD83
- 26711: UTM 11 NAD27

Source CRS:

Target CRS:

Input Location (angles in decimal degrees):
Long/Northing
Lat/Easting

or an URL to a GML dataset:

or a whole GML dataset:

WCTS Server: