# gdalinfo

lists information about a raster dataset

## SYNOPSIS

    gdalinfo [--help-general] [-mm] [-stats] [-hist] [-nogcp] [-nomd]
             [-noct] [-checksum] [-mdd domain]* datasetname

## DESCRIPTION

The gdalinfo program lists various information about a GDAL supported raster dataset.

-mm
  Force computation of the actual min/max values for each band in the dataset.
-stats
  Read and display image statistics. Force computation if no statistics are stored in an image.
-hist
  Report histogram information for all bands.
-nogcp
  Suppress ground control points list printing. It may be useful for datasets with huge amount of GCPs, such as L1B AVHRR or HDF4 MODIS which contain thousands of the ones.
-nomd
  Suppress metadata printing. Some datasets may contain a lot of metadata strings.
-noct
  Suppress printing of color table.
-checksum
  Force computation of the checksum for each band in the dataset.
-mdd domain
  Report metadata for the specified domain

The gdalinfo will report all of the following (if known):

- The format driver used to access the file.
- Raster size (in pixels and lines).
- The coordinate system for the file (in OGC WKT).
- The geotransform associated with the file (rotational coefficients are currently not reported).
- Corner coordinates in georeferenced, and if possible lat/long based on the full geotransform (but not GCPs).
- Ground control points.
- File wide (including subdatasets) metadata.
- Band data types.
- Band color interpretations.
- Band block size.
- Band descriptions.
- Band min/max values (internally known and possibly computed).
- Band checksum (if computation asked).
- Band NODATA value.
- Band overview resolutions available.
- Band unit type (i.e.. "meters" or "feet" for elevation bands).
- Band pseudo-color tables.

## EXAMPLE

    gdalinfo ~/openev/utm.tif
    Driver: GTiff/GeoTIFF
    Size is 512, 512
    Coordinate System is:
    PROJCS["NAD27 / UTM zone 11N",
        GEOGCS["NAD27",
            DATUM["North_American_Datum_1927",
                SPHEROID["Clarke 1866",6378206.4,294.978698213901]],
            PRIMEM["Greenwich",0],
            UNIT["degree",0.0174532925199433]],
        PROJECTION["Transverse_Mercator"],
        PARAMETER["latitude_of_origin",0],
        PARAMETER["central_meridian",-117],
        PARAMETER["scale_factor",0.9996],
        PARAMETER["false_easting",500000],
        PARAMETER["false_northing",0],
        UNIT["metre",1]]
    Origin = (440720.000000,3751320.000000)
    Pixel Size = (60.000000,-60.000000)
    Corner Coordinates:
    Upper Left  (  440720.000, 3751320.000) (117d38'28.21"W, 33d54'8.47"N)
    Lower Left  (  440720.000, 3720600.000) (117d38'20.79"W, 33d37'31.04"N)
    Upper Right (  471440.000, 3751320.000) (117d18'32.07"W, 33d54'13.08"N)
    Lower Right (  471440.000, 3720600.000) (117d18'28.50"W, 33d37'35.61"N)
    Center      (  456080.000, 3735960.000) (117d28'27.39"W, 33d45'52.46"N)
    Band 1 Block=512x16 Type=Byte, ColorInterp=Gray

Generated for GDAL by 1.5.6.